\def\pgfcircversion{0.8.3}
\def\pgfcircversiondate{2017/05/28}
\writestatus{loading}{\pgfcircversiondate{} The CircuiTikz circuit drawing package version \pgfcircversion}

\usemodule[tikz]

\startmodule[circuitikzgit-0.8.3]
\usetikzlibrary[calc]
\usetikzlibrary[arrows]

\unprotect

\edef\tikzatcode{\the\catcode`\@}
\edef\tikzbarcode{\the\catcode`\|}
\edef\tikzexclaimcode{\the\catcode`\!}
\catcode`\@=11
\catcode`\|=12
\catcode`\!=12

%%%%%%%%%%% Springe nach tex/pgfcirc.defines
%%%---------- open: tex/pgfcirc.defines.tex

%% Options

%%%%%%%%%%%%
%% Dimensions

% coordinates
\newdimen\pgf@circ@res@up
\newdimen\pgf@circ@res@down
\newdimen\pgf@circ@res@zero
\newdimen\pgf@circ@res@left
\newdimen\pgf@circ@res@right
\newdimen\pgf@circ@res@other
\newdimen\pgf@circ@res@step
\newdimen\pgf@circ@res@temp
% inital thickness
\newdimen \pgfstartlinewidth
%% Keys

\long\def\pgf@circ@comment#1{}

\def\circuitikzbasekey{/tikz/circuitikz}

\pgfkeys{\circuitikzbasekey/.is family}

\def\circuitikzset#1{\pgfkeys{\circuitikzbasekey,#1}}
\let\ctikzset\circuitikzset
\def\ctikzvalof#1{\pgfkeysvalueof{\circuitikzbasekey/#1}}
\def\ctikzsetvalof#1#2{\pgfkeyssetvalue{\circuitikzbasekey/#1}{#2}}

\newif\ifpgf@circ@siunitx
\newif\ifpgf@circuit@compat
\newif\ifpgf@circ@oldvoltagedirection

% Option ">" for twoports
\newif\ifpgf@circuit@inputarrow
\ctikzset{>/.add code={}{\pgf@circuit@inputarrowtrue}}
\ctikzset{inputarrow/.is choice}
\ctikzset{inputarrow/true/.code={\pgf@circuit@inputarrowtrue}}
\ctikzset{inputarrow/false/.code={\pgf@circuit@inputarrowfalse}}

% Option "boxed" for nodes and twoports
\newif\ifpgf@circuit@boxed
\pgfkeys{/tikz/boxed/.add code={}{\pgf@circuit@boxedtrue}}
\ctikzset{boxed/.add code={}{\pgf@circuit@boxedtrue}}
\pgfkeys{/tikz/box/.add code={}{\pgf@circuit@boxedtrue}}
\ctikzset{box/.add code={}{\pgf@circuit@boxedtrue}}

% Option "dashed" for nodes and twoports
\newif\ifpgf@circuit@dashed
\pgfkeys{/tikz/dashed/.add code={}{\pgf@circuit@dashedtrue}}
\ctikzset{dashed/.add code={}{\pgf@circuit@dashedtrue}}

% Option "t=*" for nodes
\pgfkeys{/tikz/t/.add code={}{\ctikzset{text=#1}}}



\ctikzset{bipoles/.is family}
\ctikzset{bipoles/border margin/.initial=1.1}
\ctikzset{bipoles/thickness/.initial=2} 
\ctikzset{nodes width/.initial=.04}
\newdimen\pgf@circ@Rlen 
\ctikzset{bipoles/length/.code={\pgf@circ@Rlen = #1}}
\pgf@circ@Rlen = 1.4cm

\ctikzset{monopoles/.is family}
\ctikzset{monopoles/ground/width/.initial=.25}
\ctikzset{monopoles/tground/thickness/.initial=3}
\ctikzset{monopoles/vcc/width/.initial=.2}
\ctikzset{monopoles/match/width/.initial=.4}
\ctikzset{monopoles/chassis/width/.initial=.25}
\ctikzset{monopoles/alternative chassis/width/.initial=.25}
\ctikzset{monopoles/equipotentiality/width/.initial=.25}
\ctikzset{monopoles/tlinestub/width/.initial=.25}          
\ctikzset{monopoles/antenna/width/.initial=.25}            
\ctikzset{monopoles/antenna/label/xanchor/.initial=.4}            
\ctikzset{monopoles/antenna/label/yanchor/.initial=.75}            
\ctikzset{monopoles/txantenna/label/xanchor/.initial=.4}            
\ctikzset{monopoles/txantenna/label/yanchor/.initial=.75}            
\ctikzset{monopoles/txantenna/width/.initial=.25}
\ctikzset{monopoles/rxantenna/label/xanchor/.initial=.4}            
\ctikzset{monopoles/rxantenna/label/yanchor/.initial=.75}            
\ctikzset{monopoles/rxantenna/width/.initial=.25}

\ctikzset{bipoles/resistor/height/.initial=.3}
\ctikzset{bipoles/resistor/width/.initial=.8}
\ctikzset{bipoles/potentiometer/height/.initial=.8}
\ctikzset{bipoles/potentiometer/height 2/.initial=.3}
\ctikzset{bipoles/potentiometer/width/.initial=.8}
\ctikzset{bipoles/photoresistor/height/.initial=.6}
\ctikzset{bipoles/photoresistor/height 2/.initial=.3}
\ctikzset{bipoles/photoresistor/width/.initial=.8}
\ctikzset{bipoles/thermistor/main/.initial=.7}
\ctikzset{bipoles/thermistor/height/.initial=.428}%.3/.7
\ctikzset{bipoles/thermistorntc/width/.initial=.8}
\ctikzset{bipoles/thermistorntc/main/.initial=.7}
\ctikzset{bipoles/thermistorntc/height/.initial=.428}%.3/.7
\ctikzset{bipoles/thermistorntc/height 2/.initial=.75}%.3/.7
\ctikzset{bipoles/thermistorptc/width/.initial=.8}
\ctikzset{bipoles/thermistorptc/main/.initial=.7}
\ctikzset{bipoles/thermistorptc/height/.initial=.428}%.3/.7
\ctikzset{bipoles/thermistorptc/height 2/.initial=.75}%.3/.7
\ctikzset{bipoles/thermistor/width/.initial=.8}
\ctikzset{bipoles/varistor/main/.initial=.7}
\ctikzset{bipoles/varistor/height/.initial=.428}%.3/.7
\ctikzset{bipoles/varistor/width/.initial=.8}
\ctikzset{bipoles/vresistor/height/.initial=.6}
\ctikzset{bipoles/vresistor/width/.initial=.8}
\ctikzset{bipoles/cuteinductor/height/.initial=.3}
\ctikzset{bipoles/cuteinductor/lower coil height/.initial=.15}	
\ctikzset{bipoles/cuteinductor/width/.initial=.6}
\ctikzset{bipoles/cuteinductor/coils/.initial=5}
\ctikzset{bipoles/cuteinductor/coil aspect/.initial=.5}%percentage of inductor width, which is covered by lower coil
\ctikzset{bipoles/americaninductor/height/.initial=.3}
\ctikzset{bipoles/americaninductor/height 2/.initial=.1}
\ctikzset{bipoles/americaninductor/width/.initial=.8}
\ctikzset{bipoles/americaninductor/coils/.initial=4}
\ctikzset{bipoles/americaninductor/coil height/.initial=.15}
\ctikzset{bipoles/vcuteinductor/height/.initial=.6}
\ctikzset{bipoles/vcuteinductor/lower coil height/.initial=.3}	
\ctikzset{bipoles/vcuteinductor/width/.initial=.6}
\ctikzset{bipoles/vcuteinductor/coils/.initial=5}
\ctikzset{bipoles/vcuteinductor/coil aspect/.initial=.5}%percentage of inductor width, which is covered by lower coil
\ctikzset{bipoles/vamericaninductor/height/.initial=.6}
\ctikzset{bipoles/vamericaninductor/height 2/.initial=.2}
\ctikzset{bipoles/vamericaninductor/width/.initial=.8}
\ctikzset{bipoles/vamericaninductor/coils/.initial=4}
\ctikzset{bipoles/vamericaninductor/coil height/.initial=.15}
\ctikzset{bipoles/esource/height/.initial=.60}
\ctikzset{bipoles/esource/width/.initial=.60}
\ctikzset{bipoles/pvsource/height/.initial=.60}
\ctikzset{bipoles/pvsource/width/.initial=.60}
\ctikzset{bipoles/isource/height/.initial=.60}
\ctikzset{bipoles/isource/width/.initial=.60}
\ctikzset{bipoles/oosource/height/.initial=.60}
\ctikzset{bipoles/oosource/width/.initial=.60}
\ctikzset{bipoles/oosource/circlesize/.initial=.65}%circlesize+circleoffset should be =1
\ctikzset{bipoles/oosource/circleoffset/.initial=.35}%circlesize+circleoffset should be =1
\ctikzset{bipoles/dcisource/height/.initial=.60}
\ctikzset{bipoles/dcisource/width/.initial=.60}
\ctikzset{bipoles/dcvsource/height/.initial=.60}
\ctikzset{bipoles/dcvsource/width/.initial=.60}
\ctikzset{bipoles/vsourcetri/height/.initial=.60}
\ctikzset{bipoles/vsourcetri/width/.initial=.60}
\ctikzset{bipoles/isourceam/height/.initial=.60}
\ctikzset{bipoles/isourceam/width/.initial=.60}
\ctikzset{bipoles/vsource/height/.initial=.60}
\ctikzset{bipoles/vsource/width/.initial=.60}
\ctikzset{bipoles/vsourceam/height/.initial=.60}
\ctikzset{bipoles/vsourceam/width/.initial=.60}
\ctikzset{bipoles/vsourceam/margin/.initial=.7}
\ctikzset{bipoles/isourcesin/height/.initial=.60}
\ctikzset{bipoles/isourcesin/width/.initial=.60}
\ctikzset{bipoles/vsourcesin/height/.initial=.60}
\ctikzset{bipoles/vsourcesin/width/.initial=.60}
\ctikzset{bipoles/vsourcesquare/height/.initial=.60}
\ctikzset{bipoles/vsourcesquare/width/.initial=.60}
\ctikzset{bipoles/cisource/height/.initial=.7}
\ctikzset{bipoles/cisource/width/.initial=.7}
\ctikzset{bipoles/cisourceam/height/.initial=.7}
\ctikzset{bipoles/cisourceam/width/.initial=.7}
\ctikzset{bipoles/cvsource/height/.initial=.7}
\ctikzset{bipoles/cvsource/width/.initial=.7}
\ctikzset{bipoles/cvsourceam/height/.initial=.7}
\ctikzset{bipoles/cvsourceam/width/.initial=.7}
\ctikzset{bipoles/cvsourceam/margin/.initial=.7}
\ctikzset{bipoles/cvsourceam/text scale/.initial=1}
\ctikzset{bipoles/cisourcesin/width/.initial=.7}
\ctikzset{bipoles/cvsourcesin/height/.initial=.7}
\ctikzset{bipoles/cvsourcesin/width/.initial=.7}
\ctikzset{bipoles/capacitor/height/.initial=.6}
\ctikzset{bipoles/capacitor/width/.initial=.2}
\ctikzset{bipoles/ecapacitor/height/.initial=.5}
\ctikzset{bipoles/ecapacitor/width/.initial=.2}
\ctikzset{bipoles/ecapacitor/font/.initial= \fontsize{6}{0}\selectfont\boldmath}
\ctikzset{bipoles/pcapacitor/height/.initial=.6}
\ctikzset{bipoles/pcapacitor/width/.initial=.2}
\ctikzset{bipoles/pcapacitor/bend width/.initial=1.1}
\ctikzset{bipoles/vcapacitor/height/.initial=.6}
\ctikzset{bipoles/vcapacitor/width/.initial=.5}
\ctikzset{bipoles/vcapacitor/capacitor width/.initial=.4}
\ctikzset{bipoles/piezoelectric/height/.initial=.7}
\ctikzset{bipoles/piezoelectric/width/.initial=.5}
\ctikzset{bipoles/battery/height/.initial=.6}
\ctikzset{bipoles/battery/width/.initial=.3}
\ctikzset{bipoles/battery1/height/.initial=.6}
\ctikzset{bipoles/battery1/width/.initial=.3}
\ctikzset{bipoles/battery2/height/.initial=.6}
\ctikzset{bipoles/battery2/width/.initial=.3}
\ctikzset{bipoles/diode/height/.initial=.50}
\ctikzset{bipoles/diode/width/.initial=.40}
\ctikzset{bipoles/varcap/height/.initial=.50}
\ctikzset{bipoles/varcap/width/.initial=.45}
\ctikzset{bipoles/spst/height/.initial=.35}
\ctikzset{bipoles/spst/width/.initial=.35}
\ctikzset{bipoles/spst/depth/.initial=.2}
\ctikzset{bipoles/nos/height/.initial=.3}
\ctikzset{bipoles/nos/width/.initial=.35}
\ctikzset{bipoles/ncs/height/.initial=.35}
\ctikzset{bipoles/ncs/width/.initial=.35}
\ctikzset{bipoles/generic/height/.initial=.30}
\ctikzset{bipoles/generic/width/.initial=.80}
\ctikzset{bipoles/european gas filled surge arrester/height/.initial=.30}
\ctikzset{bipoles/european gas filled surge arrester/width/.initial=.80}
\ctikzset{bipoles/european gas filled surge arrester/inside/.initial=.30}
\ctikzset{bipoles/american gas filled surge arrester/height/.initial=.60}
\ctikzset{bipoles/american gas filled surge arrester/width/.initial=.60}
\ctikzset{bipoles/american gas filled surge arrester/inside/.initial=.15}
\ctikzset{bipoles/american gas filled surge arrester/dot x/.initial=.25}
\ctikzset{bipoles/american gas filled surge arrester/dot y/.initial=.45}
\ctikzset{bipoles/american gas filled surge arrester/size/.initial=.1}
\ctikzset{bipoles/fuse/height/.initial=.20}
\ctikzset{bipoles/fuse/width/.initial=.50}
\ctikzset{bipoles/afuse/height/.initial=.20}
\ctikzset{bipoles/afuse/width/.initial=.50}
\ctikzset{bipoles/generic potentiometer/height/.initial=.80}
\ctikzset{bipoles/generic potentiometer/height 2/.initial=.30}
\ctikzset{bipoles/generic potentiometer/width/.initial=.80}
\ctikzset{bipoles/ageneric/height/.initial=.30}
\ctikzset{bipoles/ageneric/width/.initial=.80}
\ctikzset{bipoles/memristor/height/.initial=.30}
\ctikzset{bipoles/memristor/wave height/.initial=.5}
\ctikzset{bipoles/memristor/width/.initial=.80}
\ctikzset{bipoles/tgeneric/height/.initial=.70}
\ctikzset{bipoles/tgeneric/width/.initial=.80}
\ctikzset{bipoles/tfullgeneric/height/.initial=.70}
\ctikzset{bipoles/tfullgeneric/width/.initial=.80}
\ctikzset{bipoles/fullgeneric/height/.initial=.30}
\ctikzset{bipoles/fullgeneric/width/.initial=.80}
\ctikzset{bipoles/open/height/.initial=.3} %necessary for curly voltages
\ctikzset{bipoles/open/width/.initial=.3} %necessary for curly voltages
\ctikzset{bipoles/open/voltage/straight label distance/.initial=0}
\ctikzset{bipoles/open/voltage/distance from node/.initial=.2}
\ctikzset{bipoles/short/height/.initial=0} %dummy height for voltage positioning
\ctikzset{bipoles/short/width/.initial=0} %dummy width for voltage positioning
%\ctikzset{bipoles/short/voltage/straight label distance/.initial=.2}
%\ctikzset{bipoles/short/voltage/distance from node/.initial=.5}
\ctikzset{bipoles/ammeter/height/.initial=.60}
\ctikzset{bipoles/ammeter/width/.initial=.60}
\ctikzset{bipoles/ohmmeter/height/.initial=.60}
\ctikzset{bipoles/ohmmeter/width/.initial=.60}
\ctikzset{bipoles/voltmeter/height/.initial=.60}
\ctikzset{bipoles/voltmeter/width/.initial=.60}
\ctikzset{bipoles/buffer/height/.initial=1}
\ctikzset{bipoles/buffer/width/.initial=1}
\ctikzset{bipoles/not port/width/.initial=1}
\ctikzset{bipoles/not port/height/.initial=.8}
\ctikzset{bipoles/not port/circle width/.initial=.15}
\ctikzset{bipoles/lamp/height/.initial=.60}
\ctikzset{bipoles/lamp/width/.initial=.60}
\ctikzset{bipoles/tline/height/.initial=.3}
\ctikzset{bipoles/tline/width/.initial=.8}
\ctikzset{bipoles/squid/height/.initial=.60}
\ctikzset{bipoles/squid/width/.initial=.60}
\ctikzset{bipoles/barrier/height/.initial=.60}
\ctikzset{bipoles/barrier/width/.initial=.60}
\ctikzset{bipoles/thermocouple/height/.initial=.250}
\ctikzset{bipoles/thermocouple/height 2/.initial=.60}
\ctikzset{bipoles/thermocouple/width/.initial=.140}
\ctikzset{bipoles/pushbutton/height/.initial=.5}
\ctikzset{bipoles/pushbutton/height 2/.initial=.0}
\ctikzset{bipoles/pushbutton/width/.initial=.50}

\ctikzset{bipoles/twoport/width/.initial=.7}
\ctikzset{bipoles/twoport/height/.initial=.7}
\ctikzset{bipoles/twoport/text/.initial=}
\ctikzset{bipoles/vco/width/.initial=.7}
\ctikzset{bipoles/bandpass/width/.initial=.7}
\ctikzset{bipoles/bandstop/width/.initial=.7}
\ctikzset{bipoles/highpass/width/.initial=.7}
\ctikzset{bipoles/lowpass/width/.initial=.7}
\ctikzset{bipoles/adc/width/.initial=.7}
\ctikzset{bipoles/dac/width/.initial=.7}
\ctikzset{bipoles/dsp/width/.initial=.7}
\ctikzset{bipoles/fft/width/.initial=.7}
\ctikzset{bipoles/amp/width/.initial=.7}
\ctikzset{bipoles/vamp/width/.initial=.7}
\ctikzset{bipoles/piattenuator/width/.initial=.7}
\ctikzset{bipoles/vpiattenuator/width/.initial=.7}
\ctikzset{bipoles/tattenuator/width/.initial=.7}
\ctikzset{bipoles/vtattenuator/width/.initial=.7}
\ctikzset{bipoles/phaseshifter/width/.initial=.7}
\ctikzset{bipoles/vphaseshifter/width/.initial=.7}
\ctikzset{bipoles/detector/width/.initial=.7}


\newif\ifpgf@circuit@trans@depletiontype
\pgf@circuit@trans@depletiontypefalse

\newif\ifpgf@circuit@mos@arrows
\ctikzset{tripoles/mos style/.is choice}
\ctikzset{tripoles/mos style/no arrows/.code={\pgf@circuit@mos@arrowsfalse}}
\ctikzset{tripoles/mos style/arrows/.code={\pgf@circuit@mos@arrowstrue}}

% Option solderdot for fet 
\newif\ifpgf@circuit@fet@solderdot
\pgfkeys{/tikz/solderdot/.add code={}{\pgf@circuit@fet@solderdottrue}}
\ctikzset{solderdot/.add code={}{\pgf@circuit@fet@solderdottrue}}
\pgfkeys{/tikz/nosolderdot/.add code={}{\pgf@circuit@fet@solderdotfalse}}
\ctikzset{nosolderdot/.add code={}{\pgf@circuit@fet@solderdotfalse}}

% Option bodydiode for fet 
\newif\ifpgf@circuit@fet@bodydiode
\pgfkeys{/tikz/bodydiode/.add code={}{\pgf@circuit@fet@bodydiodetrue}}
\ctikzset{bodydiode/.add code={}{\pgf@circuit@fet@bodydiodetrue}}
\pgfkeys{/tikz/nobodydiode/.add code={}{\pgf@circuit@fet@bodydiodefalse}}
\ctikzset{nobodydiode/.add code={}{\pgf@circuit@fet@bodydiodefalse}}

% Option draw fet without gate connection
\newif\ifpgf@circuit@bpt@drawgate
\pgf@circuit@bpt@drawgatetrue
\pgfkeys{/tikz/nogate/.add code={}{\pgf@circuit@bpt@drawgatefalse}}
\ctikzset{nogate/.add code={}{\pgf@circuit@bpt@drawgatefalse}}
\pgfkeys{/tikz/nobase/.add code={}{\pgf@circuit@bpt@drawgatefalse}}
\ctikzset{nobase/.add code={}{\pgf@circuit@bpt@drawgatefalse}}

% Option draw bpt without base connection
\newif\ifpgf@circuit@bpt@drawbase
\pgf@circuit@bpt@drawbasetrue
\pgfkeys{/tikz/nobase/.add code={}{\pgf@circuit@bpt@drawbasefalse}}
\ctikzset{nobase/.add code={}{\pgf@circuit@bpt@drawbasefalse}}
\pgfkeys{/tikz/nogate/.add code={}{\pgf@circuit@bpt@drawbasefalse}}
\ctikzset{nogate/.add code={}{\pgf@circuit@bpt@drawbasefalse}}

% Option draw bpt with optical input
\newif\ifpgf@circuit@bpt@drawphoto
\pgf@circuit@bpt@drawphotofalse
\pgfkeys{/tikz/photo/.add code={}{\pgf@circuit@bpt@drawphototrue}}
\ctikzset{photo/.add code={}{\pgf@circuit@bpt@drawphototrue}}
\pgfkeys{/tikz/photo/.add code={}{\pgf@circuit@bpt@drawphototrue}}
\ctikzset{photo/.add code={}{\pgf@circuit@bpt@drawphototrue}}

% Option draw pmos with empty circle
\newif\ifpgf@circuit@pmos@emptycircle
\newif\ifpgf@circuit@pmos@emptycircle
\pgf@circuit@pmos@emptycirclefalse
\pgfkeys{/tikz/emptycircle/.add code={}{\pgf@circuit@pmos@emptycircletrue}}
\ctikzset{tripoles/pmos style/emptycircle/.add code={}{\pgf@circuit@pmos@emptycircletrue}}


\newif\ifpgf@circuit@trans@ntype
\pgf@circuit@trans@ntypetrue %default true
%\newif\ifpgf@circuit@trans@ptype
%\ctikzset{tripoles/nmos/.add code={\pgf@circuit@trans@ntypetrue}}
\ctikzset{tripoles/nmos/width/.initial=.7}
\ctikzset{tripoles/nmos/gate height/.initial=.35}
\ctikzset{tripoles/nmos/base height/.initial=.5}
\ctikzset{tripoles/nmos/conn height/.initial=0}
\ctikzset{tripoles/nmos/height/.initial=1.1}
\ctikzset{tripoles/nmos/base width/.initial=.5}
\ctikzset{tripoles/nmos/gate width/.initial=.62}
\ctikzset{tripoles/nmos/bodydiode scale/.initial=.3}
\ctikzset{tripoles/nmos/bodydiode distance/.initial=.3}
\ctikzset{tripoles/nmos/bodydiode conn/.initial=.6}
\ctikzset{tripoles/nmos/curr direction/.initial=1}

\ctikzset{tripoles/pmos/width/.initial=.7}
\ctikzset{tripoles/pmos/gate height/.initial=.35}
\ctikzset{tripoles/pmos/base height/.initial=.5}
\ctikzset{tripoles/pmos/conn height/.initial=0}
\ctikzset{tripoles/pmos/height/.initial=1.1}
\ctikzset{tripoles/pmos/base width/.initial=.5}
\ctikzset{tripoles/pmos/gate width/.initial=.62}
\ctikzset{tripoles/pmos/bodydiode scale/.initial=.3}
\ctikzset{tripoles/pmos/bodydiode distance/.initial=.3}
\ctikzset{tripoles/pmos/bodydiode conn/.initial=.6}
\ctikzset{tripoles/pmos/curr direction/.initial=-1}

\ctikzset{tripoles/nfet/width/.initial=.7}
\ctikzset{tripoles/nfet/gate height/.initial=.35}
\ctikzset{tripoles/nfet/base height/.initial=.5}
\ctikzset{tripoles/nfet/conn height/.initial=0}
\ctikzset{tripoles/nfet/height/.initial=1.1}
\ctikzset{tripoles/nfet/base width/.initial=.5}
\ctikzset{tripoles/nfet/gate width/.initial=.62}
\ctikzset{tripoles/nfet/bodydiode scale/.initial=.3}
\ctikzset{tripoles/nfet/bodydiode distance/.initial=.3}
\ctikzset{tripoles/nfet/bodydiode conn/.initial=.6}
\ctikzset{tripoles/nfet/curr direction/.initial=1}

\ctikzset{tripoles/pfet/width/.initial=.7}
\ctikzset{tripoles/pfet/gate height/.initial=.35}
\ctikzset{tripoles/pfet/base height/.initial=.5}
\ctikzset{tripoles/pfet/conn height/.initial=0}
\ctikzset{tripoles/pfet/height/.initial=1.1}
\ctikzset{tripoles/pfet/base width/.initial=.5}
\ctikzset{tripoles/pfet/gate width/.initial=.62}
\ctikzset{tripoles/pfet/bodydiode scale/.initial=.3}
\ctikzset{tripoles/pfet/bodydiode distance/.initial=.3}
\ctikzset{tripoles/pfet/bodydiode conn/.initial=.6}
\ctikzset{tripoles/pfet/curr direction/.initial=-1}

\ctikzset{tripoles/nigfete/width/.initial=.7}
\ctikzset{tripoles/nigfete/gate height/.initial=.35}
\ctikzset{tripoles/nigfete/base height/.initial=.5}
\ctikzset{tripoles/nigfete/conn height/.initial=.35}
\ctikzset{tripoles/nigfete/height/.initial=1.1}
\ctikzset{tripoles/nigfete/base width/.initial=.5}
\ctikzset{tripoles/nigfete/gate width/.initial=.62}
\ctikzset{tripoles/nigfete/bodydiode scale/.initial=.3}
\ctikzset{tripoles/nigfete/bodydiode distance/.initial=.3}
\ctikzset{tripoles/nigfete/bodydiode conn/.initial=.6}
\ctikzset{tripoles/nigfete/curr direction/.initial=1}

\ctikzset{tripoles/nigfetd/width/.initial=.7}
\ctikzset{tripoles/nigfetd/gate height/.initial=.35}
\ctikzset{tripoles/nigfetd/base height/.initial=.5}
\ctikzset{tripoles/nigfetd/conn height/.initial=.35}
\ctikzset{tripoles/nigfetd/height/.initial=1.1}
\ctikzset{tripoles/nigfetd/base width/.initial=.5}
\ctikzset{tripoles/nigfetd/gate width/.initial=.62}
\ctikzset{tripoles/nigfetd/bodydiode scale/.initial=.3}
\ctikzset{tripoles/nigfetd/bodydiode distance/.initial=.3}
\ctikzset{tripoles/nigfetd/bodydiode conn/.initial=.6}
\ctikzset{tripoles/nigfetd/curr direction/.initial=1}

\ctikzset{tripoles/nigfetebulk/width/.initial=.7}
\ctikzset{tripoles/nigfetebulk/gate height/.initial=.35}
\ctikzset{tripoles/nigfetebulk/base height/.initial=.5}
\ctikzset{tripoles/nigfetebulk/conn height/.initial=.35}
\ctikzset{tripoles/nigfetebulk/height/.initial=1.1}
\ctikzset{tripoles/nigfetebulk/base width/.initial=.5}
\ctikzset{tripoles/nigfetebulk/gate width/.initial=.62}
\ctikzset{tripoles/nigfetebulk/bodydiode scale/.initial=.3}
\ctikzset{tripoles/nigfetebulk/bodydiode distance/.initial=.3}
\ctikzset{tripoles/nigfetebulk/bodydiode conn/.initial=.6}
\ctikzset{tripoles/nigfetebulk/curr direction/.initial=1}

\ctikzset{tripoles/pigfete/width/.initial=.7}
\ctikzset{tripoles/pigfete/gate height/.initial=.35}
\ctikzset{tripoles/pigfete/base height/.initial=.5}
\ctikzset{tripoles/pigfete/conn height/.initial=.35}
\ctikzset{tripoles/pigfete/height/.initial=1.1}
\ctikzset{tripoles/pigfete/base width/.initial=.5}
\ctikzset{tripoles/pigfete/gate width/.initial=.62}
\ctikzset{tripoles/pigfete/bodydiode scale/.initial=.3}
\ctikzset{tripoles/pigfete/bodydiode distance/.initial=.3}
\ctikzset{tripoles/pigfete/bodydiode conn/.initial=.6}
\ctikzset{tripoles/pigfete/curr direction/.initial=-1}

\ctikzset{tripoles/pigfetd/width/.initial=.7}
\ctikzset{tripoles/pigfetd/gate height/.initial=.35}
\ctikzset{tripoles/pigfetd/base height/.initial=.5}
\ctikzset{tripoles/pigfetd/conn height/.initial=.35}
\ctikzset{tripoles/pigfetd/height/.initial=1.1}
\ctikzset{tripoles/pigfetd/base width/.initial=.5}
\ctikzset{tripoles/pigfetd/gate width/.initial=.62}
\ctikzset{tripoles/pigfetd/bodydiode scale/.initial=.3}
\ctikzset{tripoles/pigfetd/bodydiode distance/.initial=.3}
\ctikzset{tripoles/pigfetd/bodydiode conn/.initial=.6}
\ctikzset{tripoles/pigfetd/curr direction/.initial=-1}

\ctikzset{tripoles/pigfetebulk/width/.initial=.7}
\ctikzset{tripoles/pigfetebulk/gate height/.initial=.35}
\ctikzset{tripoles/pigfetebulk/conn height/.initial=.35}
\ctikzset{tripoles/pigfetebulk/base height/.initial=.5}
\ctikzset{tripoles/pigfetebulk/height/.initial=1.1}
\ctikzset{tripoles/pigfetebulk/base width/.initial=.5}
\ctikzset{tripoles/pigfetebulk/gate width/.initial=.62}
\ctikzset{tripoles/pigfetebulk/bodydiode scale/.initial=.3}
\ctikzset{tripoles/pigfetebulk/bodydiode distance/.initial=.3}
\ctikzset{tripoles/pigfetebulk/bodydiode conn/.initial=.6}
\ctikzset{tripoles/pigfetebulk/curr direction/.initial=-1}

\ctikzset{tripoles/npn/width/.initial=.6}
\ctikzset{tripoles/npn/base height/.initial=.45}
\ctikzset{tripoles/npn/base height 2/.initial=.15}
\ctikzset{tripoles/npn/base height/.initial=.4}
\ctikzset{tripoles/npn/conn height/.initial=0}
\ctikzset{tripoles/npn/height/.initial=1.1}
\ctikzset{tripoles/npn/base width/.initial=.5}
\ctikzset{tripoles/npn/bodydiode scale/.initial=.3}
\ctikzset{tripoles/npn/bodydiode distance/.initial=.3}
\ctikzset{tripoles/npn/bodydiode conn/.initial=.6}
\ctikzset{tripoles/npn/curr direction/.initial=1}

\ctikzset{tripoles/pnp/width/.initial=.6}
\ctikzset{tripoles/pnp/base height/.initial=.45}
\ctikzset{tripoles/pnp/base height 2/.initial=.15}
\ctikzset{tripoles/pnp/base height/.initial=.4}
\ctikzset{tripoles/pnp/conn height/.initial=0}
\ctikzset{tripoles/pnp/height/.initial=1.1}
\ctikzset{tripoles/pnp/base width/.initial=.5}
\ctikzset{tripoles/pnp/bodydiode scale/.initial=.3}
\ctikzset{tripoles/pnp/bodydiode distance/.initial=.3}
\ctikzset{tripoles/pnp/bodydiode conn/.initial=.6}
\ctikzset{tripoles/pnp/curr direction/.initial=-1}

\ctikzset{tripoles/pigbt/width/.initial=.6}
\ctikzset{tripoles/pigbt/gate height/.initial=.45}
\ctikzset{tripoles/pigbt/gate height 2/.initial=.15}
\ctikzset{tripoles/pigbt/base height/.initial=.4}
\ctikzset{tripoles/pigbt/conn height/.initial=0}
\ctikzset{tripoles/pigbt/height/.initial=1.1}
\ctikzset{tripoles/pigbt/gate width/.initial=.62}
\ctikzset{tripoles/pigbt/base width/.initial=.5}
\ctikzset{tripoles/pigbt/bodydiode scale/.initial=.3}
\ctikzset{tripoles/pigbt/bodydiode distance/.initial=.3}
\ctikzset{tripoles/pigbt/bodydiode conn/.initial=.6}
\ctikzset{tripoles/pigbt/curr direction/.initial=-1}

\ctikzset{tripoles/nigbt/width/.initial=.6}
\ctikzset{tripoles/nigbt/gate height/.initial=.45}
\ctikzset{tripoles/nigbt/gate height 2/.initial=.15}
\ctikzset{tripoles/nigbt/base height/.initial=.4}
\ctikzset{tripoles/nigbt/conn height/.initial=0}
\ctikzset{tripoles/nigbt/height/.initial=1.1}
\ctikzset{tripoles/nigbt/gate width/.initial=.62}
\ctikzset{tripoles/nigbt/base width/.initial=.5}
\ctikzset{tripoles/nigbt/bodydiode scale/.initial=.3}
\ctikzset{tripoles/nigbt/bodydiode distance/.initial=.3}
\ctikzset{tripoles/nigbt/bodydiode conn/.initial=.6}
\ctikzset{tripoles/nigbt/curr direction/.initial=1}

\ctikzset{tripoles/Lpigbt/width/.initial=.6}
\ctikzset{tripoles/Lpigbt/gate height/.initial=.45}
\ctikzset{tripoles/Lpigbt/gate height 2/.initial=.15}
\ctikzset{tripoles/Lpigbt/base height/.initial=.4}
\ctikzset{tripoles/Lpigbt/conn height/.initial=.4}
\ctikzset{tripoles/Lpigbt/height/.initial=1.1}
\ctikzset{tripoles/Lpigbt/gate width/.initial=.62}
\ctikzset{tripoles/Lpigbt/base width/.initial=.5}
\ctikzset{tripoles/Lpigbt/bodydiode scale/.initial=.3}
\ctikzset{tripoles/Lpigbt/bodydiode distance/.initial=.3}
\ctikzset{tripoles/Lpigbt/bodydiode conn/.initial=.6}
\ctikzset{tripoles/Lpigbt/curr direction/.initial=-1}

\ctikzset{tripoles/Lnigbt/width/.initial=.6}
\ctikzset{tripoles/Lnigbt/gate height/.initial=.45}
\ctikzset{tripoles/Lnigbt/gate height 2/.initial=.15}
\ctikzset{tripoles/Lnigbt/base height/.initial=.4}
\ctikzset{tripoles/Lnigbt/conn height/.initial=.4}
\ctikzset{tripoles/Lnigbt/height/.initial=1.1}
\ctikzset{tripoles/Lnigbt/gate width/.initial=.62}
\ctikzset{tripoles/Lnigbt/base width/.initial=.5}
\ctikzset{tripoles/Lnigbt/bodydiode scale/.initial=.3}
\ctikzset{tripoles/Lnigbt/bodydiode distance/.initial=.3}
\ctikzset{tripoles/Lnigbt/bodydiode conn/.initial=.6}
\ctikzset{tripoles/Lnigbt/curr direction/.initial=1}

\ctikzset{tripoles/njfet/width/.initial=.7}
\ctikzset{tripoles/njfet/gate height/.initial=.5}
\ctikzset{tripoles/njfet/gate height 2/.initial=.35}
\ctikzset{tripoles/njfet/gate width/.initial=.5}
\ctikzset{tripoles/njfet/conn height/.initial=.35}
\ctikzset{tripoles/njfet/height/.initial=1.1}
\ctikzset{tripoles/njfet/bodydiode scale/.initial=.3}
\ctikzset{tripoles/njfet/bodydiode distance/.initial=.3}
\ctikzset{tripoles/njfet/bodydiode conn/.initial=.6}
\ctikzset{tripoles/njfet/curr direction/.initial=1}

\ctikzset{tripoles/pjfet/width/.initial=.7}
\ctikzset{tripoles/pjfet/gate height/.initial=.5}
\ctikzset{tripoles/pjfet/gate height 2/.initial=.35}
\ctikzset{tripoles/pjfet/gate width/.initial=.5}
\ctikzset{tripoles/pjfet/conn height/.initial=.35}
\ctikzset{tripoles/pjfet/height/.initial=1.1}
\ctikzset{tripoles/pjfet/bodydiode scale/.initial=.3}
\ctikzset{tripoles/pjfet/bodydiode distance/.initial=.3}
\ctikzset{tripoles/pjfet/bodydiode conn/.initial=.6}
\ctikzset{tripoles/pjfet/curr direction/.initial=-1}

\ctikzset{tripoles/isfet/width/.initial=1}
\ctikzset{tripoles/isfet/gate height/.initial=.35}
\ctikzset{tripoles/isfet/base height/.initial=.5}
\ctikzset{tripoles/isfet/height/.initial=1.1}
\ctikzset{tripoles/isfet/base width/.initial=.3}
\ctikzset{tripoles/isfet/gate width/.initial=.5}
\ctikzset{tripoles/isfet/conn height/.initial=0}
\ctikzset{tripoles/isfet/wave width/.initial=.16}
\ctikzset{tripoles/isfet/wave amp/.initial=.06}
\ctikzset{tripoles/isfet/waves y sep/.initial=.22}
\ctikzset{tripoles/isfet/waves x sep/.initial=.8}
\ctikzset{tripoles/isfet/bodydiode scale/.initial=.3}
\ctikzset{tripoles/isfet/bodydiode distance/.initial=.3}
\ctikzset{tripoles/isfet/bodydiode conn/.initial=.6}
\ctikzset{tripoles/isfet/curr direction/.initial=1}

\newif\ifpgf@circuit@europeanlogicport
\ctikzset{logic ports/.is choice}
\ctikzset{logic ports/european/.code= {\pgf@circuit@europeanlogicporttrue } }
\ctikzset{logic ports/american/.code= {\pgf@circuit@europeanlogicportfalse } } 


\ctikzset{tripoles/american and port/width/.initial=1.1}
\ctikzset{tripoles/american and port/height/.initial=.8}
\ctikzset{tripoles/american and port/port width/.initial=.7}
\ctikzset{tripoles/american and port/input height/.initial=.5}
\ctikzset{tripoles/american nand port/width/.initial=1.1}
\ctikzset{tripoles/american nand port/height/.initial=.8}
\ctikzset{tripoles/american nand port/port width/.initial=.7}
\ctikzset{tripoles/american nand port/circle width/.initial=.15}
\ctikzset{tripoles/american nand port/input height/.initial=.5}
\ctikzset{tripoles/american or port/width/.initial=1.1}
\ctikzset{tripoles/american or port/height/.initial=.8}
\ctikzset{tripoles/american or port/port width/.initial=.7}
\ctikzset{tripoles/american or port/input height/.initial=.5}
\ctikzset{tripoles/american or port/input skip/.initial=.25}
\ctikzset{tripoles/american or port/aaa/.initial=.6}
\ctikzset{tripoles/american or port/bbb/.initial=.4} 
\ctikzset{tripoles/american or port/ccc/.initial=.5} 
\ctikzset{tripoles/american or port/ddd/.initial=.0}
\ctikzset{tripoles/american nor port/width/.initial=1.1}
\ctikzset{tripoles/american nor port/height/.initial=.8}
\ctikzset{tripoles/american nor port/port width/.initial=.7}
\ctikzset{tripoles/american nor port/input height/.initial=.5}
\ctikzset{tripoles/american nor port/input skip/.initial=.25}
\ctikzset{tripoles/american nor port/circle width/.initial=.15}
\ctikzset{tripoles/american nor port/aaa/.initial=.6}
\ctikzset{tripoles/american nor port/bbb/.initial=.4} 
\ctikzset{tripoles/american nor port/ccc/.initial=.5} 
\ctikzset{tripoles/american nor port/ddd/.initial=.0}
\ctikzset{tripoles/american xor port/width/.initial=1.1}
\ctikzset{tripoles/american xor port/height/.initial=.8}
\ctikzset{tripoles/american xor port/port width/.initial=.7}
\ctikzset{tripoles/american xor port/input height/.initial=.5}
\ctikzset{tripoles/american xor port/input skip/.initial=.15}
\ctikzset{tripoles/american xor port/distance/.initial=.1} 
\ctikzset{tripoles/american xor port/aaa/.initial=.6}
\ctikzset{tripoles/american xor port/bbb/.initial=.4} 
\ctikzset{tripoles/american xor port/ccc/.initial=.5} 
\ctikzset{tripoles/american xor port/ddd/.initial=.0}
\ctikzset{tripoles/american xnor port/width/.initial=1.1}
\ctikzset{tripoles/american xnor port/height/.initial=.8}
\ctikzset{tripoles/american xnor port/port width/.initial=.7}
\ctikzset{tripoles/american xnor port/input height/.initial=.5}
\ctikzset{tripoles/american xnor port/input skip/.initial=.15}
\ctikzset{tripoles/american xnor port/distance/.initial=.1} 
\ctikzset{tripoles/american xnor port/aaa/.initial=.6}
\ctikzset{tripoles/american xnor port/bbb/.initial=.4} 
\ctikzset{tripoles/american xnor port/ccc/.initial=.5} 
\ctikzset{tripoles/american xnor port/ddd/.initial=.0}
\ctikzset{tripoles/american xnor port/circle width/.initial=.15}
\ctikzset{tripoles/european and port/width/.initial=1.4}
\ctikzset{tripoles/european and port/height/.initial=.65}
\ctikzset{tripoles/european and port/reserved/.initial=.6}
\ctikzset{tripoles/european and port/input height/.initial=.6}
\ctikzset{tripoles/european or port/width/.initial=1.4}
\ctikzset{tripoles/european or port/height/.initial=.65}
\ctikzset{tripoles/european or port/reserved/.initial=.6}
\ctikzset{tripoles/european or port/input height/.initial=.6}
\ctikzset{tripoles/european xor port/width/.initial=1.4}
\ctikzset{tripoles/european xor port/height/.initial=.65}
\ctikzset{tripoles/european xor port/reserved/.initial=.6}
\ctikzset{tripoles/european xor port/input height/.initial=.6}
\ctikzset{tripoles/european nand port/width/.initial=1.4}
\ctikzset{tripoles/european nand port/not height/.initial=.3}
\ctikzset{tripoles/european nand port/not width/.initial=.8}
\ctikzset{tripoles/european nand port/height/.initial=.65}
\ctikzset{tripoles/european nand port/reserved/.initial=.6}
\ctikzset{tripoles/european nand port/input height/.initial=.6}
\ctikzset{tripoles/european not port/width/.initial=1.4}
\ctikzset{tripoles/european not port/not height/.initial=.3}
\ctikzset{tripoles/european not port/not width/.initial=.8}
\ctikzset{tripoles/european not port/height/.initial=.65}
\ctikzset{tripoles/european not port/reserved/.initial=.6}
\ctikzset{tripoles/european not port/input height/.initial=0}
\ctikzset{tripoles/european xnor port/width/.initial=1.4}
\ctikzset{tripoles/european xnor port/not height/.initial=.3}
\ctikzset{tripoles/european xnor port/not width/.initial=.8}
\ctikzset{tripoles/european xnor port/height/.initial=.65}
\ctikzset{tripoles/european xnor port/reserved/.initial=.6}
\ctikzset{tripoles/european xnor port/input height/.initial=.6}
\ctikzset{tripoles/european nor port/width/.initial=1.4}
\ctikzset{tripoles/european nor port/not height/.initial=.3}
\ctikzset{tripoles/european nor port/not width/.initial=.8}
\ctikzset{tripoles/european nor port/height/.initial=.65}
\ctikzset{tripoles/european nor port/reserved/.initial=.6}
\ctikzset{tripoles/european nor port/input height/.initial=.6}
\ctikzset{tripoles/op amp/width/.initial=1.7}
\ctikzset{tripoles/op amp/port width/.initial=.7}
\ctikzset{tripoles/op amp/height/.initial=1.4}
\ctikzset{tripoles/op amp/input height/.initial=.5}
\ctikzset{tripoles/op amp/up pos/.initial=.45}
\ctikzset{tripoles/op amp/font/.initial= \fontsize{10}{0}\selectfont\boldmath}%absolut font size needed!
\ctikzset{tripoles/en amp/width/.initial=1.7}
\ctikzset{tripoles/en amp/port width/.initial=.7}
\ctikzset{tripoles/en amp/height/.initial=1.6}
\ctikzset{tripoles/en amp/input height/.initial=.3}
\ctikzset{tripoles/en amp/up pos/.initial=.45}
\ctikzset{tripoles/en amp/font/.initial= \fontsize{10}{0}\selectfont\boldmath}%absolut font size needed!
\ctikzset{tripoles/en amp/font2/.initial= \fontsize{14}{0}\selectfont\boldmath}%absolut font size needed!
\ctikzset{tripoles/gm amp/width/.initial=1.7}
\ctikzset{tripoles/gm amp/port width/.initial=.7}
\ctikzset{tripoles/gm amp/height/.initial=1.4}
\ctikzset{tripoles/gm amp/input height/.initial=.5}
\ctikzset{tripoles/gm amp/up pos/.initial=.45}
\ctikzset{tripoles/plain amp/width/.initial=1.7}
\ctikzset{tripoles/plain amp/port width/.initial=.7}
\ctikzset{tripoles/plain amp/height/.initial=1.4}
\ctikzset{tripoles/plain amp/input height/.initial=.5}
\ctikzset{tripoles/plain amp/up pos/.initial=.45}

\ctikzset{tripoles/thyristor/height/.initial=1.10}
\ctikzset{tripoles/thyristor/height 2/.initial=.5}
\ctikzset{tripoles/thyristor/width/.initial=1.0}
\ctikzset{tripoles/thyristor/diode height/.initial=.5}
\ctikzset{tripoles/thyristor/diode width left/.initial=.4}
\ctikzset{tripoles/thyristor/diode width right/.initial=.3}

\ctikzset{tripoles/triac/height/.initial=1.1}
\ctikzset{tripoles/triac/width/.initial=1}
\ctikzset{tripoles/triac/diode width left/.initial=.3}
\ctikzset{tripoles/triac/diode width right/.initial=.3}

\ctikzset{tripoles/spdt/width/.initial=.85}
\ctikzset{tripoles/spdt/height/.initial=.45}
\ctikzset{tripoles/spdt/margin/.initial=.45}

\ctikzset{tripoles/toggleswitch/height/.initial=.8}
\ctikzset{tripoles/toggleswitch/height 2/.initial=.0}
\ctikzset{tripoles/toggleswitch/width/.initial=.80}

\ctikzset{tripoles/mixer/width/.initial=0.7}
\ctikzset{tripoles/adder/width/.initial=0.7}
\ctikzset{tripoles/circulator/width/.initial=.7}
\ctikzset{tripoles/oscillator/width/.initial=.7}


\ctikzset{tripoles/wilkinson/height/.initial=1.3}
\ctikzset{tripoles/wilkinson/width/.initial=1.3}

\ctikzset{quadpoles/transformer/width/.initial=1.5}
\ctikzset{quadpoles/transformer/width1/.initial=.4}
\ctikzset{quadpoles/transformer/height/.initial=1.5}
\ctikzset{quadpoles/transformer/height1/.initial=.8}
\ctikzset{quadpoles/transformer core/width/.initial=1.5}
\ctikzset{quadpoles/transformer core/height/.initial=1.5}
\ctikzset{quadpoles/transformer core/core height/.initial=.5}
\ctikzset{quadpoles/transformer core/core width/.initial=.05}
\ctikzset{quadpoles/gyrator/width/.initial=1.5}
\ctikzset{quadpoles/gyrator/height/.initial=1.5}
\ctikzset{quadpoles/fourport/width/.initial=1.3}
\ctikzset{quadpoles/fourport/height/.initial=1.3}
\ctikzset{quadpoles/coupler/width/.initial=1.3}
\ctikzset{quadpoles/coupler/height/.initial=1.3}
\ctikzset{quadpoles/coupler2/width/.initial=1.3}
\ctikzset{quadpoles/coupler2/height/.initial=1.3}

\ctikzset{/tikz/circuitikz/tripoles/magnetron/width/.initial=1}


% %Mechanical section
\ctikzset{/tikz/circuitikz/tripoles/elmech/height/.initial=.8}
\ctikzset{/tikz/circuitikz/tripoles/elmech/width/.initial=.6}
\ctikzset{bipoles/spring/height/.initial=.5}
\ctikzset{bipoles/spring/width/.initial=.5}
\ctikzset{bipoles/mass/height/.initial=.55}
\ctikzset{bipoles/mass/box height/.initial=.4}
\ctikzset{bipoles/mass/width/.initial=.5}

\ctikzset{bipoles/damper/height/.initial=.35}
\ctikzset{bipoles/damper/length/.initial=.3}
\ctikzset{bipoles/damper/width/.initial=.4}


\ctikzset{bipole/.is family}
\ctikzset{bipole/kind/.initial = }
\ctikzset{bipole/name/.initial = }
\newif\ifpgf@circuit@bipole@isvoltage
\ctikzset{bipole/is voltage/.is if=pgf@circuit@bipole@isvoltage}
\newif\ifpgf@circuit@bipole@voltageoutsideofsymbol
\ctikzset{bipole/is voltageoutsideofsymbol/.is if=pgf@circuit@bipole@voltageoutsideofsymbol}
\newif\ifpgf@circuit@bipole@strokedsymbol
\ctikzset{bipole/is strokedsymbol/.is if=pgf@circuit@bipole@strokedsymbol}
\newif\ifpgf@circuit@bipole@iscurrent
\ctikzset{bipole/is current/.is if=pgf@circuit@bipole@iscurrent}

\ctikzset{bipole/voltage/.is family}
\newif\ifpgf@circuit@bipole@voltage@backward
\ctikzset{bipole/voltage/direction/.is choice}
\ctikzset{bipole/voltage/direction/forward/.code={\pgf@circuit@bipole@voltage@backwardfalse}}
\ctikzset{bipole/voltage/direction/backward/.code={\pgf@circuit@bipole@voltage@backwardtrue}}
\newif\ifpgf@circuit@bipole@voltage@below
\ctikzset{bipole/voltage/position/.is choice}
\ctikzset{bipole/voltage/position/above/.code={\pgf@circuit@bipole@voltage@belowfalse}}
\ctikzset{bipole/voltage/position/below/.code={\pgf@circuit@bipole@voltage@belowtrue}}

\ctikzset{bipole/voltage/label/unit/.initial=}
\ctikzset{bipole/voltage/label/name/.initial=}

\ctikzset{bipole/current/.is family}
\newif\ifpgf@circuit@bipole@current@backward
\ctikzset{bipole/current/direction/.is choice}
\ctikzset{bipole/current/direction/forward/.code={\pgf@circuit@bipole@current@backwardfalse}}
\ctikzset{bipole/current/direction/backward/.code={\pgf@circuit@bipole@current@backwardtrue}}
\newif\ifpgf@circuit@bipole@current@before
\ctikzset{bipole/current/x position/.is choice}
\ctikzset{bipole/current/x position/after/.code={\pgf@circuit@bipole@current@beforefalse}}
\ctikzset{bipole/current/x position/before/.code={\pgf@circuit@bipole@current@beforetrue}}
\newif\ifpgf@circuit@bipole@current@below
\ctikzset{bipole/current/y position/.is choice}
\ctikzset{bipole/current/y position/above/.code={\pgf@circuit@bipole@current@belowfalse}}
\ctikzset{bipole/current/y position/below/.code={\pgf@circuit@bipole@current@belowtrue}}
\ctikzset{bipole/current/label/unit/.initial=}
\ctikzset{bipole/current/label/name/.initial=}

\ctikzset{bipole/flow/.is family}
\newif\ifpgf@circuit@bipole@flow@backward
\ctikzset{bipole/flow/direction/.is choice}
\ctikzset{bipole/flow/direction/forward/.code={\pgf@circuit@bipole@flow@backwardfalse}}
\ctikzset{bipole/flow/direction/backward/.code={\pgf@circuit@bipole@flow@backwardtrue}}
\newif\ifpgf@circuit@bipole@flow@before
\ctikzset{bipole/flow/x position/.is choice}
\ctikzset{bipole/flow/x position/after/.code={\pgf@circuit@bipole@flow@beforefalse}}
\ctikzset{bipole/flow/x position/before/.code={\pgf@circuit@bipole@flow@beforetrue}}
\newif\ifpgf@circuit@bipole@flow@below
\ctikzset{bipole/flow/y position/.is choice}
\ctikzset{bipole/flow/y position/above/.code={\pgf@circuit@bipole@flow@belowfalse}}
\ctikzset{bipole/flow/y position/below/.code={\pgf@circuit@bipole@flow@belowtrue}}
\ctikzset{bipole/flow/label/unit/.initial=}
\ctikzset{bipole/flow/label/name/.initial=}
\ctikzset{flow/distance/.initial = .5}
\ctikzset{flow/offset/.initial = .2}%distance between flow-arrow and conductor


\ctikzset{bipole/label/.is family}
\ctikzset{bipole/label/position/.initial=90}
\ctikzset{bipole/label/unit/.initial=}
\ctikzset{bipole/label/name/.initial=}
\ctikzset{bipole/annotation/.is family}
\ctikzset{bipole/annotation/position/.initial=-90}
\ctikzset{bipole/annotation/unit/.initial=}
\ctikzset{bipole/annotation/name/.initial=}
\ctikzset{bipole/nodes/.is family}
\ctikzset{bipole/nodes/left/.is choice}
\ctikzset{bipole/nodes/left/none/.code={\ctikzsetvalof{bipole/nodes/left}{none}}}
\ctikzset{bipole/nodes/left/empty/.code={\ctikzsetvalof{bipole/nodes/left}{empty}}}
\ctikzset{bipole/nodes/left/full/.code={\ctikzsetvalof{bipole/nodes/left}{full}}}
\ctikzset{bipole/nodes/left/diamond/.code={\ctikzsetvalof{bipole/nodes/left}{diamond}}}
\ctikzset{bipole/nodes/left/rectjoinfill/.code={\ctikzsetvalof{bipole/nodes/left}{rectjoinfill}}}
\ctikzset{bipole/nodes/right/.is choice}
\ctikzset{bipole/nodes/right/none/.code={\ctikzsetvalof{bipole/nodes/right}{none}}}
\ctikzset{bipole/nodes/right/empty/.code={\ctikzsetvalof{bipole/nodes/right}{empty}}}
\ctikzset{bipole/nodes/right/full/.code={\ctikzsetvalof{bipole/nodes/right}{full}}}
\ctikzset{bipole/nodes/right/diamond/.code={\ctikzsetvalof{bipole/nodes/right}{diamond}}}
\ctikzset{bipole/nodes/right/rectjoinfill/.code={\ctikzsetvalof{bipole/nodes/right}{rectjoinfill}}}




\newif\ifpgf@circuit@europeanresistor
\ctikzset{resistor/.is choice}
\ctikzset{resistor/american/.code = \pgf@circuit@europeanresistorfalse }
\ctikzset{resistor/european/.code = \pgf@circuit@europeanresistortrue }

\ctikzset{inductor/.is choice}
\ctikzset{inductor/cute/.code={\ctikzsetvalof{inductor}{cute}}}
\ctikzset{inductor/european/.code={\ctikzsetvalof{inductor}{european}}}
\ctikzset{inductor/american/.code={\ctikzsetvalof{inductor}{american}}}

\newif\ifpgf@circuit@strokediode
\newif\ifpgf@circuit@fulldiode
\pgf@circuit@strokediodefalse
\pgf@circuit@fulldiodefalse

\ctikzset{diode/.is choice}
\ctikzset{diode/empty/.code = \pgf@circuit@fulldiodefalse\pgf@circuit@strokediodefalse}%default
\ctikzset{diode/full/.code = \pgf@circuit@fulldiodetrue }
\ctikzset{diode/stroke/.code = \pgf@circuit@strokediodetrue}

\tikzset{full diodes/.style = { \circuitikzbasekey/diode = full }}
\tikzset{empty diodes/.style = { \circuitikzbasekey/diode = empty }}
\tikzset{stroke diodes/.style = { \circuitikzbasekey/diode = stroke }}

\ctikzset{thickness/.initial=2}
\ctikzset{color/.initial=black}
\pgfkeys{/tikz/color/.add code={}{\ctikzset{color={#1}}}}


\newif\ifpgf@circ@siunitx
\newif\ifpgf@circ@siunitx@res

\ctikzset{straight/.is choice}
\ctikzset{straightvoltage value/.initial=true}
\ctikzset{straight/true/.code = {\pgf@circuit@bipole@voltage@straighttrue}}
\ctikzset{straight/false/.code = {\pgf@circuit@bipole@voltage@straightfalse}}
\ctikzset{straightvoltage/.style = {/tikz/circuitikz/straight=true}}
\newif\ifpgf@circuit@bipole@voltage@straight
\ctikzset{bipole/straight/.is if=pgf@circuit@bipole@voltage@straight}


\ctikzset{voltage/.is family}
\ctikzset{voltage/distance from node/.initial=.5} %\pgf@circ@Rlen units
\ctikzset{voltage/distance from line/.initial=.08} % pos, tra 0 e 1
\ctikzset{voltage/bump a/.initial=1.2}
\ctikzset{voltage/bump b/.initial=1.5}
\ctikzset{voltage/european label distance/.initial=1.4}
\ctikzset{voltage/american label distance/.initial=1.1}
% special cases
\ctikzset{bipoles/generic/voltage/distance from node/.initial=.4}
\ctikzset{bipoles/generic/voltage/bump b/.initial=2}
\ctikzset{bipoles/generic/voltage/european label distance/.initial=1.8}
%\ctikzset{bipoles/thermocouple/voltage/distance from node/.initial=.3}
\ctikzset{bipoles/thermocouple/voltage/bump b/.initial=2.2}
\ctikzset{bipoles/thermocouple/voltage/european label distance/.initial=1.5}
\ctikzset{bipoles/ageneric/voltage/distance from node/.initial=.4}
\ctikzset{bipoles/ageneric/voltage/bump b/.initial=2}
\ctikzset{bipoles/ageneric/voltage/european label distance/.initial=1.8}
\ctikzset{bipoles/fullgeneric/voltage/distance from node/.initial=.4}
\ctikzset{bipoles/fullgeneric/voltage/bump b/.initial=2}
\ctikzset{bipoles/fullgeneric/voltage/european label distance/.initial=1.8}
\ctikzset{bipoles/memristor/voltage/distance from node/.initial=.4}
\ctikzset{bipoles/memristor/voltage/bump b/.initial=2}
\ctikzset{bipoles/memristor/voltage/european label distance/.initial=1.8}
%\ctikzset{bipoles/tline/voltage/distance from node/.initial=.2}
\ctikzset{bipoles/tline/voltage/bump b/.initial=2.4}
\ctikzset{bipoles/tline/voltage/european label distance/.initial=2.1}
%\ctikzset{bipoles/varistor/voltage/distance from node/.initial=.2}
\ctikzset{bipoles/varistor/voltage/bump b/.initial=2.4}
\ctikzset{bipoles/varistor/voltage/european label distance/.initial=2}
%\ctikzset{bipoles/photoresistor/voltage/distance from node/.initial=.2}
\ctikzset{bipoles/photoresistor/voltage/bump b/.initial=2}
\ctikzset{bipoles/photoresistor/voltage/european label distance/.initial=1.8}
%\ctikzset{bipoles/thermistor/voltage/distance from node/.initial=.2}
\ctikzset{bipoles/thermistor/voltage/bump b/.initial=2.4}
\ctikzset{bipoles/thermistor/voltage/european label distance/.initial=2}
%\ctikzset{bipoles/thermistorntc/voltage/distance from node/.initial=.2}
\ctikzset{bipoles/thermistorntc/voltage/bump b/.initial=1.6}
%\ctikzset{bipoles/thermistorptc/voltage/distance from node/.initial=.2}
\ctikzset{bipoles/thermistorptc/voltage/bump b/.initial=1.6}

\ctikzset{current/.is family}
\ctikzset{current/distance/.initial = .5}


\tikzset{american currents/.style = { \circuitikzbasekey/current = american } }
\tikzset{european currents/.style = { \circuitikzbasekey/current = european } }
\tikzset{american voltages/.style = { \circuitikzbasekey/voltage = american } }
\tikzset{european voltages/.style = { \circuitikzbasekey/voltage = european } }
\tikzset{american resistors/.style = { \circuitikzbasekey/resistor = american } }
\tikzset{european resistors/.style = { \circuitikzbasekey/resistor = european } }

\newif\ifpgf@circuit@europeangfsurgearrester
\ctikzset{gas filled surge arrester choice/.is choice}
\ctikzset{gas filled surge arrester choice/european/.code= {\pgf@circuit@europeangfsurgearrestertrue } }
\ctikzset{gas filled surge arrester choice/american/.code= {\pgf@circuit@europeangfsurgearresterfalse } }

\tikzset{american gas filled surge arrester set/.style = { \circuitikzbasekey/gas filled surge arrester choice=american } }
\tikzset{european gas filled surge arrester set/.style = { \circuitikzbasekey/gas filled surge arrester choice=european } }
\tikzset{american inductors/.style = { \circuitikzbasekey/inductor = american } }
\tikzset{european inductors/.style = { \circuitikzbasekey/inductor = european } }
\tikzset{cute inductors/.style = { \circuitikzbasekey/inductor = cute } }
\tikzset{american ports/.style = { \circuitikzbasekey/logic ports = american } }
\tikzset{european ports/.style = { \circuitikzbasekey/logic ports = european } }
\tikzset{european/.style = { european currents, european voltages, european resistors, european inductors, european ports, european gas filled surge arrester set} }
\tikzset{american/.style = { american currents, american voltages, american resistors, american inductors, american ports, american gas filled surge arrester set} }
\tikzset{cute/.style = { european currents, european voltages, american resistors, cute inductors, american ports } }

% I should try to make the tree clearer (this voltaege conflicts with the options above)

\newif\ifpgf@circuit@europeanvoltage
\ctikzset{voltage/.is choice}
\ctikzset{voltage/american/.code = {\pgf@circuit@europeanvoltagefalse } }
\ctikzset{voltage/european/.code = {\pgf@circuit@europeanvoltagetrue } }

\newif\ifpgf@circuit@europeancurrent
\ctikzset{current/.is choice}
\ctikzset{current/american/.code = \pgf@circuit@europeancurrentfalse }
\ctikzset{current/european/.code = \pgf@circuit@europeancurrenttrue }

\ctikzset{label/align/.is choice}
\ctikzset{label/align/straight/.code={\ctikzsetvalof{label/align}{straight}}}
\ctikzset{label/align/rotate/.code={\ctikzsetvalof{label/align}{rotate}}}
\ctikzset{label/align/smart/.code={\ctikzsetvalof{label/align}{smart}}}

%%%%%%%%%% new
\pgfkeys{\circuitikzbasekey/.search also={/tikz}}
%%%---------- close: tex/pgfcirc.defines
%%%%%%%%%%% Springe nach tex/pgfcircutils
%%%---------- open: tex/pgfcircutils.tex
% Copyright 2007-2009 by Massimo Redaelli
%
% This file may be distributed and/or modified
%
% 1. under the LaTeX Project Public License and/or
% 2. under the GNU Public License.
%
% See the file doc/LICENSE for more details.

%\def\pgf@circ@handleSI#1{%
 % \pgf@circ@siunitx@resfalse
%  
 % \edef\len{\stringlength[e]{#1}}
  %\testmatchingchar[e]{#1}{\len}{>}%
  %\ifmatchingchar%
  %  \ifnum\findchars{#1}{<}=0
	%  \def\pgf@circ@handleSI@val{\substring{#1}{1}{\findchars{#1}{<}-1}}
	  %\def\pgf@circ@handleSI@unit{\substring{#1}{\findchars{#1}{<}-1}+1}{\stringlength{#1}}
	  %\pgf@circ@siunitx@restrue
%	\else
%	\fi
  %\else 
  %\fi
%}

\def\pgf@circ@handleSI#1{
	\noexpandarg
        	\def\pgf@temp{}
	\StrBetween{#1}{<}{>}[\pgf@circ@handleSI@unit]
	\StrLen{\pgf@circ@handleSI@unit}[\pgf@circ@handleSI@unit@len]

	\ifnum\pgf@circ@handleSI@unit@len=0  
	  \pgf@circ@siunitx@resfalse  
	\else  
	  \IfEndWith{#1}{>}{
	  	\pgf@circ@siunitx@restrue 
		\noexpandarg
	  	\StrBefore{#1}{<}[\pgf@circ@handleSI@val]		
                %\typeout{si |#1|}
	  }{
	  	\pgf@circ@siunitx@resfalse 
                %\typeout{no si |#1|}
	  }
	\fi
}

\def\pgf@circ@ifkeyempty#1{
	\pgfextra{
		\ctikzset{#1/.get=\pgf@circ@temp}
		\edef\pgf@temp{}
	}
	\ifx\pgf@circ@temp\pgf@temp
}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%%    Math routines

\def\pgf@circ@stripdecimals#1.#2\pgf@nil{#1}


%%%---------- close: tex/pgfcircutils

%%%%%%%%%%% Springe nach tex/pgfcircshapes
%%%---------- open: tex/pgfcircshapes.tex
% Copyright 2007-2009 by Massimo Redaelli
%
% This file may be distributed and/or modified
%
% 1. under the LaTeX Project Public License and/or
% 2. under the GNU Public License.
%
% See the file doc/LICENSE for more details.

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%%  Other shapes


%% Nothing

\pgfdeclareshape{emptyshape}{
	\savedanchor{\northeast}{%
		\pgf@x=.5\wd\pgfnodeparttextbox%
		\pgf@y=.5\ht\pgfnodeparttextbox%
   }
	\anchor{north}{
		\northeast
		\pgf@x=0cm
	}
	\anchor{east}{%
		\northeast
		\pgf@y=0cm
   }
	\anchor{south}{%
		\northeast
		\pgf@y=-\pgf@y
		\pgf@x=0cm
   }
	\anchor{west}{
		\northeast
		\pgf@y=0cm
		\pgf@x=-\pgf@x
	}
	\anchor{text}{%
		\pgfpointorigin
   }
	\anchor{center}{
		\pgfpointorigin
	}
}

%% Full terminal

\pgfdeclareshape{circ}{
	\anchor{center}{
		\pgfpointorigin
	}
	\anchorborder{
		\pgf@circ@res@left=\pgf@x
		\pgf@circ@res@up=\pgf@y
		\pgfpointborderellipse{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}
}{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/nodes width}*\pgf@circ@Rlen}{\pgfkeysvalueof{/tikz/circuitikz/nodes width}*\pgf@circ@Rlen}}		
	}
	\behindforegroundpath{		
		
		\pgfscope
			\pgfpathcircle{\pgfpointorigin}{\pgfkeysvalueof{/tikz/circuitikz/nodes width}*\pgf@circ@Rlen}
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}
			\pgfusepath{draw,fill}		
		\endpgfscope

		}
}

%% Empty terminal

\pgfdeclareshape{ocirc}{
	\anchor{center}{
		\pgfpointorigin
	}
	\anchorborder{
		\pgf@circ@res@left=\pgf@x
		\pgf@circ@res@up=\pgf@y
		\pgfpointborderellipse{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}
}{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/nodes width}*\pgf@circ@Rlen}{\pgfkeysvalueof{/tikz/circuitikz/nodes width}*\pgf@circ@Rlen}}		
	}

	\behindforegroundpath{		
		
		\pgfscope
			\pgfpathcircle{\pgfpointorigin}{\pgfkeysvalueof{/tikz/circuitikz/nodes width}*\pgf@circ@Rlen}
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}
			\pgfsetfillcolor{white}
			\pgfusepath{draw,fill}		
		\endpgfscope

		}
}

%% Diamond terminal

\pgfdeclareshape{diamondpole}{
	\anchor{center}{
		\pgfpointorigin
	}
	\anchorborder{
		\pgf@circ@res@left=\pgf@x
		\pgf@circ@res@up=\pgf@y
	}
	\behindforegroundpath{		
		\pgfscope
			\pgfmathsetlength{\pgf@circ@res@temp}{\pgfkeysvalueof{/tikz/circuitikz/nodes width}*\pgf@circ@Rlen}
			\pgftransformrotate{45}
			\pgfpathrectanglecorners
			{\pgfpoint{\pgf@circ@res@left-\pgf@circ@res@temp}{\pgf@circ@res@up+\pgf@circ@res@temp}}
			{\pgfpoint{\pgf@circ@res@left+\pgf@circ@res@temp}{\pgf@circ@res@up-\pgf@circ@res@temp}}
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}
			\pgfusepath{draw,fill}		
		\endpgfscope
		}
}

%% Fill for correct rectangular joins

\pgfdeclareshape{rectjoinfill}{
	\anchor{center}{
		\pgfpointorigin
	}
	\anchorborder{
		\pgf@circ@res@left=\pgf@x
		\pgf@circ@res@up=\pgf@y
	}
	\behindforegroundpath{		
		\pgfscope
			\pgfpathrectanglecorners
			{\pgfpoint{0}{.5\pgflinewidth}}
			{\pgfpoint{0}{-.5\pgflinewidth}}
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}
			\pgfusepath{draw,fill}		
		\endpgfscope
		}
}


%% Current arrow

\pgfdeclareshape{currarrow}{
	\anchor{center}{
		\pgfpointorigin
	}
		\anchor{tip}{
		\pgfpointorigin
			\pgf@circ@res@step = \pgf@circ@Rlen
				\divide \pgf@circ@res@step by 16
		\pgf@x	=\pgf@circ@res@step
		}
	\behindforegroundpath{		
		
		\pgfscope
			\pgf@circ@res@step = \pgf@circ@Rlen
			\divide \pgf@circ@res@step by 16

			\pgfpathmoveto{\pgfpoint{-.7\pgf@circ@res@step}{0pt}}
			\pgfpathlineto{\pgfpoint{-.7\pgf@circ@res@step}{-.8\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{1\pgf@circ@res@step}{0pt}}
			\pgfpathlineto{\pgfpoint{-.7\pgf@circ@res@step}{.8\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{-.7\pgf@circ@res@step}{0pt}}			
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}
			\pgfusepath{draw,fill}

		\endpgfscope
	}

}

%% Flow arrow

\pgfdeclareshape{flowarrow}{
	\anchor{center}{
		\pgfpointorigin
	}
		\anchor{tip}{
		\pgfpointorigin
			\pgf@circ@res@step = \pgf@circ@Rlen
				\divide \pgf@circ@res@step by 16
		\pgf@x	=\pgf@circ@res@step
		}
	\behindforegroundpath{
		\pgfscope
			\pgf@circ@res@step = \pgf@circ@Rlen
			\divide \pgf@circ@res@step by 4
			\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@step}{0pt}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{0pt}}
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}
			\pgfusepath{draw}
			\pgftransformshift{\pgfpoint{\pgf@circ@res@step}{0pt}}
			\pgfnode{currarrow}{tip}{}{}{\pgfusepath{fill}}
		\endpgfscope
	}
}

%% Input arrow

\pgfdeclareshape{inputarrow}{
	\savedanchor{\tip}{
		\pgfpointorigin
	}
	\anchor{center}{
		\tip
	}
	\anchor{tip}{
		\tip
	}
	\behindforegroundpath{		
		
		\pgfscope
			\pgf@circ@res@step = \pgf@circ@Rlen
			\divide \pgf@circ@res@step by 16

			\pgfpathmoveto{\pgfpoint{-1.7\pgf@circ@res@step}{0pt}}
			\pgfpathlineto{\pgfpoint{-1.7\pgf@circ@res@step}{-.8\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{0pt}{0pt}}
			\pgfpathlineto{\pgfpoint{-1.7\pgf@circ@res@step}{.8\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{-1.7\pgf@circ@res@step}{0pt}}			
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}
			\pgfusepath{fill}

		\endpgfscope
	}

}


%% box

\pgfdeclareshape{box}{
	\anchor{center}{
		\pgfpointorigin
	}
	\behindforegroundpath{		
		
		\pgfscope
			\pgf@circ@res@step = \ctikzvalof{bipoles/twoport/width}\pgf@circ@Rlen
			\pgf@circ@res@step = 0.5\pgf@circ@res@step
			\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
			\pgfpathrectanglecorners{\pgfpoint{-\pgf@circ@res@step}{\pgf@circ@res@step}}{\pgfpoint{\pgf@circ@res@step}{-\pgf@circ@res@step}}
			\pgfusepath{draw}
		\endpgfscope
	}

}

%%%---------- close: tex/pgfcircshapes
%%%%%%%%%%% Springe nach tex/pgfcircmonopoles
%%%---------- open: tex/pgfcircmonopoles.tex
% Copyright 2007-2009 by Massimo Redaelli
%
% This file may be distributed and/or modified
%
% 1. under the LaTeX Project Public License and/or
% 2. under the GNU Public License.
%
% See the file doc/LICENSE for more details.

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%% Monopoles

%% Ground symbol

\pgfdeclareshape{ground}{
	\anchor{center}{
		\pgfpointorigin
	}
	\behindforegroundpath{		
		\pgf@circ@res@step=\ctikzvalof{monopoles/ground/width}\pgf@circ@Rlen
		
		\pgfscope		
			\pgfpathmoveto{\pgfpointorigin}
			\pgfpathlineto{\pgfpoint{0pt}{-\pgf@circ@res@step}}
			\pgfusepath{draw}

			\pgfstartlinewidth=\pgflinewidth
			%\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

			\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@step}{-\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{-\pgf@circ@res@step}}
			\pgfusepath{draw}
						
			\pgfsetlinewidth{\pgfstartlinewidth}
			\pgfpathmoveto{\pgfpoint{-.8\pgf@circ@res@step}{-1.2\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{.8\pgf@circ@res@step}{-1.2\pgf@circ@res@step}}
			\pgfpathmoveto{\pgfpoint{-.6\pgf@circ@res@step}{-1.4\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{.6\pgf@circ@res@step}{-1.4\pgf@circ@res@step}}
			\pgfpathmoveto{\pgfpoint{-.4\pgf@circ@res@step}{-1.6\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{.4\pgf@circ@res@step}{-1.6\pgf@circ@res@step}}
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}
			\pgfusepath{draw}
		
			
			\pgfsetlinewidth{\pgfstartlinewidth}
	
		\endpgfscope
	}

}



\pgfdeclareshape{rground}{
	\anchor{center}{
		\pgfpointorigin
	}
	\behindforegroundpath{		
		\pgf@circ@res@step=\ctikzvalof{monopoles/ground/width}\pgf@circ@Rlen
		
		\pgfscope		
			\pgfpathmoveto{\pgfpointorigin}
			\pgfpathlineto{\pgfpoint{0pt}{-\pgf@circ@res@step}}
			\pgfusepath{draw}

			\pgfstartlinewidth=\pgflinewidth
			\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

			\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@step}{-\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{-\pgf@circ@res@step}}
			\pgfusepath{draw}
						
						
			\pgfsetlinewidth{\pgfstartlinewidth}
	
		\endpgfscope
	}
}

\pgfdeclareshape{tground}{
	\anchor{center}{
		\pgfpointorigin
	}
	\behindforegroundpath{		
		\pgf@circ@res@step=\ctikzvalof{monopoles/ground/width}\pgf@circ@Rlen
		
		\pgfscope		
			\pgfpathmoveto{\pgfpointorigin}
			%\pgfpathlineto{\pgfpoint{0pt}{-\pgf@circ@res@step}}
			\pgfusepath{draw}

			\pgfstartlinewidth=\pgflinewidth
			\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/monopoles/tground/thickness}\pgfstartlinewidth}

			\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@step}{0pt}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{0pt}}
			\pgfusepath{draw}
						
						
			\pgfsetlinewidth{\pgfstartlinewidth}
	
		\endpgfscope
	}
}

\pgfdeclareshape{sground}{
	\anchor{center}{
		\pgfpointorigin
	}
	\behindforegroundpath{		
		\pgf@circ@res@step=\ctikzvalof{monopoles/ground/width}\pgf@circ@Rlen
		
		\pgfscope		
			\pgfpathmoveto{\pgfpointorigin}
			\pgfpathlineto{\pgfpoint{0pt}{-\pgf@circ@res@step}}
			\pgfusepath{draw}

			\pgfstartlinewidth=\pgflinewidth
			\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

			\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@step}{-\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{-\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{0}{-1.8\pgf@circ@res@step}}
			\pgfpathclose
			\pgfusepath{draw}
						
						
			\pgfsetlinewidth{\pgfstartlinewidth}
	
		\endpgfscope
	}

}

% noiseless ground
\pgfdeclareshape{nground}{
	\anchor{center}{
		\pgfpointorigin
	}
	\behindforegroundpath{		
		\pgf@circ@res@step=\ctikzvalof{monopoles/ground/width}\pgf@circ@Rlen
		
		\pgfscope		
			\pgfpathmoveto{\pgfpointorigin}
			\pgfpathlineto{\pgfpoint{0pt}{-\pgf@circ@res@step}}
			\pgfusepath{draw}

			\pgfstartlinewidth=\pgflinewidth
			%\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

			\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@step}{-\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{-\pgf@circ@res@step}}
			\pgfusepath{draw}
						
			\pgfsetlinewidth{\pgfstartlinewidth}
			\pgfpathmoveto{\pgfpoint{-.8\pgf@circ@res@step}{-1.2\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{.8\pgf@circ@res@step}{-1.2\pgf@circ@res@step}}
			\pgfpathmoveto{\pgfpoint{-.6\pgf@circ@res@step}{-1.4\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{.6\pgf@circ@res@step}{-1.4\pgf@circ@res@step}}
			\pgfpathmoveto{\pgfpoint{-.4\pgf@circ@res@step}{-1.6\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{.4\pgf@circ@res@step}{-1.6\pgf@circ@res@step}}
			\pgfusepath{draw}
			
			\pgfpathmoveto{\pgfpoint{1.3\pgf@circ@res@step}{-1.6\pgf@circ@res@step}}
			\pgfpatharc{0}{180}{1.3\pgf@circ@res@step}
			\pgfusepath{draw}
					
			\pgfsetlinewidth{\pgfstartlinewidth}
		\endpgfscope
	}
}

% protective ground
\pgfdeclareshape{pground}{
	\anchor{center}{
		\pgfpointorigin
	}
	\behindforegroundpath{		
		\pgf@circ@res@step=\ctikzvalof{monopoles/ground/width}\pgf@circ@Rlen
		
		\pgfscope		
			\pgfpathmoveto{\pgfpointorigin}
			\pgfpathlineto{\pgfpoint{0pt}{-\pgf@circ@res@step}}
			\pgfusepath{draw}

			\pgfstartlinewidth=\pgflinewidth
			%\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

			\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@step}{-\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{-\pgf@circ@res@step}}
			\pgfpathcircle{\pgfpoint{0pt}{-\pgf@circ@res@step}} {1.2\pgf@circ@res@step}
			\pgfusepath{draw}
						
			\pgfsetlinewidth{\pgfstartlinewidth}
			\pgfpathmoveto{\pgfpoint{-.8\pgf@circ@res@step}{-1.2\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{.8\pgf@circ@res@step}{-1.2\pgf@circ@res@step}}
			\pgfpathmoveto{\pgfpoint{-.6\pgf@circ@res@step}{-1.4\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{.6\pgf@circ@res@step}{-1.4\pgf@circ@res@step}}
			\pgfpathmoveto{\pgfpoint{-.4\pgf@circ@res@step}{-1.6\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{.4\pgf@circ@res@step}{-1.6\pgf@circ@res@step}}
			\pgfusepath{draw}
					
			\pgfsetlinewidth{\pgfstartlinewidth}
		\endpgfscope
	}
}

% chassis ground 
\pgfdeclareshape{cground}{ 
\anchor{center}{ 
    \pgfpointorigin 
} 
\behindforegroundpath{       
    \pgf@circ@res@step=\ctikzvalof{monopoles/chassis/width}\pgf@circ@Rlen 
 
    \pgfscope        
        \pgfpathmoveto{\pgfpointorigin} 
        \pgfpathlineto{\pgfpoint{0pt}{-\pgf@circ@res@step}} 
        \pgfusepath{draw}

        \pgfpathmoveto{\pgfpoint{-1.5\pgf@circ@res@step}{-2\pgf@circ@res@step}}
        \pgfpathlineto{\pgfpoint{-\pgf@circ@res@step}{-\pgf@circ@res@step}}
        \pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{-\pgf@circ@res@step}}
        \pgfpathlineto{\pgfpoint{0.5\pgf@circ@res@step}{-2\pgf@circ@res@step}}
        \pgfpathmoveto{\pgfpoint{0pt}{-\pgf@circ@res@step}}
        \pgfpathlineto{\pgfpoint{-0.5\pgf@circ@res@step}{-2\pgf@circ@res@step}}
        \pgfusepath{draw}                        
    \endpgfscope 
    } 
}

% Contributed by Leonardo Azzinnari
\pgfdeclareshape{tlinestub}{
	\anchor{center}{\pgfpointorigin}
	\behindforegroundpath{
		\pgfstartlinewidth=\pgflinewidth
		
		\pgf@circ@res@step=\ctikzvalof{bipoles/tline/width} \pgf@circ@Rlen
        \pgfpathmoveto{\pgfpoint{0.5\pgf@circ@res@step}{0.25\pgf@circ@res@step}}
        
            \pgfpathmoveto{\pgfpointorigin}
            \pgfpathlineto{\pgfpoint{0.5\pgf@circ@res@step}{0pt}}
            \pgfusepath{draw}
         \pgfscope
            \pgfpathellipse{\pgfpoint{0.5\pgf@circ@res@step}{0\pgf@circ@res@step}}{\pgfpoint{0.125\pgf@circ@res@step}{0\pgf@circ@res@step}}{\pgfpoint{0\pgf@circ@res@step}{0.25\pgf@circ@res@step}}
			\pgfpathmoveto{\pgfpoint{0.5\pgf@circ@res@step}{0.25\pgf@circ@res@step}}
            \pgfpathlineto{\pgfpoint{1.5\pgf@circ@res@step}{0.25\pgf@circ@res@step}}
            \pgfpatharc{90}{-90}{0.125\pgf@circ@res@step and 0.25\pgf@circ@res@step}
            \pgfpathlineto{\pgfpoint{0.5\pgf@circ@res@step}{-0.25\pgf@circ@res@step}}
            \pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
            \pgfusepath{draw}
         \endpgfscope
      }
}
                            



\pgfdeclareshape{antenna}{
\anchor{center}{\pgfpointorigin}
	\savedanchor{\northeast}{
		\pgf@circ@res@step=\ctikzvalof{monopoles/antenna/width}\pgf@circ@Rlen
		\pgf@x=5\pgf@circ@res@step%-0.5\pgflinewidth
		\pgf@y=6\pgf@circ@res@step
	}
	\anchor{text}{
		\northeast
		\pgf@x=\ctikzvalof{monopoles/antenna/label/xanchor}\pgf@x
		\pgf@y=\ctikzvalof{monopoles/antenna/label/yanchor}\pgf@y
	}
   \behindforegroundpath{
     \pgfstartlinewidth=\pgflinewidth
     \pgf@circ@res@step=\ctikzvalof{monopoles/antenna/width}\pgf@circ@Rlen
                           
        % \pgfpathmoveto{\pgfpointorigin}
        % \pgfpathlineto{\pgfpoint{4\pgf@circ@res@step}{0pt}}
        % \pgfpathmoveto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{0pt}}
        %     \pgfpathlineto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
        
        \pgftransformxshift{ -4\pgf@circ@res@step }

        \pgfpathmoveto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{0pt}}
        \pgfpathlineto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             
         \pgfusepath{draw}
             
          \pgfscope   
          \pgfpathmoveto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             \pgfpathlineto{\pgfpoint{5\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             \pgfpathlineto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{4\pgf@circ@res@step}}
             \pgfpathlineto{\pgfpoint{3\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             \pgfpathlineto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             \pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}
             \pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
             \pgfusepath{draw}
           \endpgfscope
                           \pgfsetlinewidth{\pgfstartlinewidth}
                        
                           }
     }


\pgfdeclareshape{txantenna}{
	\anchor{center}{\pgfpointorigin}
	\savedanchor{\northeast}{
		\pgf@circ@res@step=\ctikzvalof{monopoles/txantenna/width}\pgf@circ@Rlen
		\pgf@x=5\pgf@circ@res@step%-0.5\pgflinewidth
		\pgf@y=6\pgf@circ@res@step
	}
	\anchor{text}{
		\northeast
		\pgf@x=\ctikzvalof{monopoles/txantenna/label/xanchor}\pgf@x
		\pgf@y=\ctikzvalof{monopoles/txantenna/label/yanchor}\pgf@y
	}
       \behindforegroundpath{
       \pgfstartlinewidth=\pgflinewidth
       \pgf@circ@res@step=\ctikzvalof{monopoles/txantenna/width}\pgf@circ@Rlen
        
         \pgfpathmoveto{\pgfpointorigin}
         \pgfpathlineto{\pgfpoint{4\pgf@circ@res@step}{0pt}}
         \pgfpathmoveto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{0pt}}
             \pgfpathlineto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             
         \pgfusepath{draw}
             
          \pgfscope   
          \pgfpathmoveto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             \pgfpathlineto{\pgfpoint{5\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             \pgfpathlineto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{4\pgf@circ@res@step}}
             \pgfpathlineto{\pgfpoint{3\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             \pgfpathlineto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             \pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}
             \pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
             \pgfusepath{draw}
           \endpgfscope
          \pgfpathmoveto{\pgfpoint{5.5\pgf@circ@res@step}{6\pgf@circ@res@step}}
%        \pgfpatharc{60}{-60}{\pgf@circ@res@step and \pgf@circ@res@step}
        \pgfpatharc{30}{-30}{2\pgf@circ@res@step}         \pgfpathmoveto{\pgfpoint{6\pgf@circ@res@step}{6.25\pgf@circ@res@step}}
        \pgfpatharc{30}{-30}{2.5\pgf@circ@res@step}
        \pgfpathmoveto{\pgfpoint{6.5\pgf@circ@res@step}{6.5\pgf@circ@res@step}}
        \pgfpatharc{30}{-30}{3\pgf@circ@res@step}
        \pgfpathmoveto{\pgfpoint{7\pgf@circ@res@step}{6.75\pgf@circ@res@step}}
        \pgfpatharc{30}{-30}{3.5\pgf@circ@res@step}
        \pgfpathmoveto{\pgfpoint{7.5\pgf@circ@res@step}{7\pgf@circ@res@step}}
        \pgfpatharc{30}{-30}{4\pgf@circ@res@step}
        \pgfusepath{draw}
        \pgfsetlinewidth{\pgfstartlinewidth}
        
        }
     }


\pgfdeclareshape{rxantenna}{
	\anchor{center}{\pgfpointorigin}
	\savedanchor{\northeast}{
		\pgf@circ@res@step=\ctikzvalof{monopoles/txantenna/width}\pgf@circ@Rlen
		\pgf@x=5\pgf@circ@res@step%-0.5\pgflinewidth
		\pgf@y=6\pgf@circ@res@step
	}
	\anchor{text}{
		\northeast
		\pgf@x=\ctikzvalof{monopoles/rxantenna/label/xanchor}\pgf@x
		\pgf@y=\ctikzvalof{monopoles/rxantenna/label/yanchor}\pgf@y
	}
    \behindforegroundpath{
        \pgfstartlinewidth=\pgflinewidth
        \pgf@circ@res@step=\ctikzvalof{monopoles/rxantenna/width}\pgf@circ@Rlen
             
         \pgfpathmoveto{\pgfpointorigin}
         \pgfpathlineto{\pgfpoint{4\pgf@circ@res@step}{0pt}}
         \pgfpathmoveto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{0pt}}
             \pgfpathlineto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             
         \pgfusepath{draw}
             
          \pgfscope   
          \pgfpathmoveto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             \pgfpathlineto{\pgfpoint{5\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             \pgfpathlineto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{4\pgf@circ@res@step}}
             \pgfpathlineto{\pgfpoint{3\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             \pgfpathlineto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             \pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}
             \pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
             \pgfusepath{draw}
           \endpgfscope
           
           \pgfpathmoveto{\pgfpoint{6\pgf@circ@res@step}{7\pgf@circ@res@step}}
%             \pgfpatharc{60}{-60}{\pgf@circ@res@step and \pgf@circ@res@step}
             \pgfpatharc{150}{210}{4\pgf@circ@res@step}              \pgfpathmoveto{\pgfpoint{6.5\pgf@circ@res@step}{6.75\pgf@circ@res@step}}
             \pgfpatharc{150}{210}{3.5\pgf@circ@res@step}
             \pgfpathmoveto{\pgfpoint{7\pgf@circ@res@step}{6.5\pgf@circ@res@step}}
             \pgfpatharc{150}{210}{3\pgf@circ@res@step}
             \pgfpathmoveto{\pgfpoint{7.5\pgf@circ@res@step}{6.25\pgf@circ@res@step}}
             \pgfpatharc{150}{210}{2.5\pgf@circ@res@step}
             \pgfpathmoveto{\pgfpoint{8\pgf@circ@res@step}{6\pgf@circ@res@step}}
             \pgfpatharc{150}{210}{2\pgf@circ@res@step}
             \pgfusepath{draw}
             \pgfsetlinewidth{\pgfstartlinewidth}
             
             }
}

% Vcc
\pgfdeclareshape{vcc}{
\anchor{center}{\pgfpointorigin}
\anchor{text}{
	\pgf@circ@res@step=\ctikzvalof{monopoles/vcc/width}\pgf@circ@Rlen
	\pgfpathmoveto{\pgfpoint{-.5\wd\pgfnodeparttextbox}{2\pgf@circ@res@step+2\ht\pgfnodeparttextbox}}                          
	\pgfpathmoveto{\pgfpoint{.5\wd\pgfnodeparttextbox}{2\pgf@circ@res@step+2\ht\pgfnodeparttextbox}}                
	\pgf@x=0pt
	\pgf@y=2\pgf@circ@res@step
	\advance \pgf@y by 0.5\ht\pgfnodeparttextbox
	\pgf@x=-.5\wd\pgfnodeparttextbox
	}
\behindforegroundpath{                             
	\pgf@circ@res@step=\ctikzvalof{monopoles/vcc/width}\pgf@circ@Rlen           
	\pgfscope           
		\pgfpathmoveto{\pgfpointorigin}
		\pgfpathlineto{\pgfpoint{0pt}{1.5\pgf@circ@res@step}}
		\pgfusepath{draw}

		\pgfstartlinewidth=\pgflinewidth
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

		\pgfpathmoveto{\pgfpoint{-0.5\pgf@circ@res@step}{.8\pgf@circ@res@step}}
		\pgfpathlineto{\pgfpoint{0}{1.5\pgf@circ@res@step}}
		\pgfpathlineto{\pgfpoint{0.5\pgf@circ@res@step}{.8\pgf@circ@res@step}}
		\pgfusepath{draw}
																						
		\pgfsetlinewidth{\pgfstartlinewidth}

	\endpgfscope
}

}

% Vee
\pgfdeclareshape{vee}{
\anchor{center}{\pgfpointorigin}
\anchor{text}{
	\pgf@circ@res@step=\ctikzvalof{monopoles/vcc/width}\pgf@circ@Rlen
	\pgfpathmoveto{\pgfpoint{-.5\wd\pgfnodeparttextbox}{-2\pgf@circ@res@step-2\ht\pgfnodeparttextbox}}                        
	\pgfpathmoveto{\pgfpoint{.5\wd\pgfnodeparttextbox}{-2\pgf@circ@res@step-2\ht\pgfnodeparttextbox}}        
	\pgf@x=0pt
	\pgf@y=-2\pgf@circ@res@step
	\advance \pgf@y by -1.5\ht\pgfnodeparttextbox
	\pgf@x=-.5\wd\pgfnodeparttextbox
	}

\behindforegroundpath{                             
	\pgf@circ@res@step=\ctikzvalof{monopoles/vcc/width}\pgf@circ@Rlen
	
	\pgfscope                           
		\pgfpathmoveto{\pgfpointorigin}
		\pgfpathlineto{\pgfpoint{0pt}{-1.5\pgf@circ@res@step}}
		\pgfusepath{draw}

		\pgfstartlinewidth=\pgflinewidth
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

		\pgfpathmoveto{\pgfpoint{-0.5\pgf@circ@res@step}{-.8\pgf@circ@res@step}}
		\pgfpathlineto{\pgfpoint{0}{-1.5\pgf@circ@res@step}}
		\pgfpathlineto{\pgfpoint{0.5\pgf@circ@res@step}{-.8\pgf@circ@res@step}}
		\pgfusepath{draw}
		\pgfsetlinewidth{\pgfstartlinewidth}

	\endpgfscope
}

}


% match
\pgfdeclareshape{match}{
	\anchor{center}{
		\pgfpointorigin
	}
	\anchor{text}{
		\pgf@x=\ctikzvalof{monopoles/match/width}\pgf@circ@Rlen
		\pgf@x=1.5\pgf@x
		\advance \pgf@x by -.5\wd\pgfnodeparttextbox
		\pgf@y=-1.5\ht\pgfnodeparttextbox
	}
	\behindforegroundpath{		
		\pgf@circ@res@step=\ctikzvalof{monopoles/match/width}\pgf@circ@Rlen
		
		\pgfscope		
			\pgfpathmoveto{\pgfpointorigin}
			\pgfpathlineto{\pgfpoint{2\pgf@circ@res@step}{0pt}}
			\pgfusepath{draw}

			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{0pt}}
			\pgfpathlineto{\pgfpoint{2\pgf@circ@res@step}{0.5\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{2\pgf@circ@res@step}{0}}
			\pgfusepath{fill}
									
			\pgfsetlinewidth{\pgfstartlinewidth}
	
		\endpgfscope
	}

}


%%%---------- close: tex/pgfcircmonopoles
%%%%%%%%%%% Springe nach tex/pgfcircbipoles
%%%---------- open: tex/pgfcircbipoles.tex
% Copyright 2007-2009 by Massimo Redaelli
%
% This file may be distributed and/or modified
%
% 1. under the LaTeX Project Public License and/or
% 2. under the GNU Public License.
%
% See the file doc/LICENSE for more details.

%% Generic macro for defining a bipole shape
% #1 - additional anchors
% #2 - lower y-size of the bipole (from the center).
% #3 - #shape is the name of the shape
% #4 - upper y-size of the bipole (from the center)
% #5 - width of the bipole
% #6 - macros drawing the bipole


\long\def\pgfcircdeclarebipole#1#2#3#4#5#6{
	\pgfdeclareshape{#3shape}{
	
	\savedanchor{\northeast}{
		\pgf@y=#4\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@x=#5\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
	}
	\savedanchor{\northeastborder}{
		\pgf@y=#4\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@y=\ctikzvalof{bipoles/border margin}\pgf@y
		\pgf@x=#5\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
		\pgf@x=\ctikzvalof{bipoles/border margin}\pgf@x
	}
	\savedanchor{\southwestborder}{
		\pgf@y=-#2\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@y=\ctikzvalof{bipoles/border margin}\pgf@y
		\pgf@x=-#5\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
		\pgf@x=\ctikzvalof{bipoles/border margin}\pgf@x
	}
	\savedanchor{\southwest}{
		\pgf@y=-#2\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@x=-#5\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
	}
	\savedanchor{\centerpoint}{
		\pgf@circ@res@down=-#2\pgf@circ@Rlen
		\pgf@circ@res@up=#4\pgf@circ@Rlen
		\pgfpointorigin
		\pgf@y=\pgf@circ@res@up
		\advance\pgf@y by\pgf@circ@res@down
		\pgf@y=.5\pgf@y
	}
	\anchor{center}{\pgfpointorigin}
	\anchor{n}{
		\northeast
		\pgf@x=0cm
	}
	\anchor{ne}{
		\northeast
	}
	\anchor{nw}{
		\northeast
		\pgf@x=-\pgf@x
	}
	\anchor{e}{%
		\northeast
		\pgf@y=0cm
   }
	\anchor{s}{%
		\southwest
		\pgf@x=0cm
   }
	\anchor{se}{%
		\southwest
		\pgf@x=-\pgf@x
   }
	\anchor{sw}{%
		\southwest
   }
	\anchor{w}{
		\southwest
		\pgf@y=0cm
	}
	\anchor{north}{
		\northeast
		\pgf@x=0cm
	}
	\anchor{east}{%
		\northeast
		\pgf@y=0cm
   }
	\anchor{south}{%
		\southwest
		\pgf@x=0cm
   }
	\anchor{west}{
		\southwest
		\pgf@y=0cm
	}
	\anchor{right}{
		\northeast
		\pgf@y=0cm
	}
	\anchor{above}{
		\northeast
		\pgf@x=0cm
	}
	\anchor{left}{%
		\southwest
		\pgf@y=0cm
   }
	\anchor{below}{%
		\southwest
		\pgf@x=0cm                    
   }
	\anchor{a}{%
		\northeast
		\pgf@y=0cm
   }
	\anchor{b} {
		\southwest
		\pgf@y=0cm
	}
	\savedanchor{\textanchor}{%
		\pgf@y=\ht\pgfnodeparttextbox
		\pgf@x=-.5\wd\pgfnodeparttextbox
   }
	\anchor{text}{%
		\textanchor
   }
	\anchorborder{%
		\ifpgf@circuit@bipole@inverted
			\pgf@circ@res@left=-\pgf@x
			\pgf@circ@res@right=-\pgf@y
		\else
			\pgf@circ@res@left=\pgf@x
			\pgf@circ@res@right=\pgf@y
		\fi
		\ifdim\pgf@circ@res@right>0cm
			\pgfpointborderrectangle{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@right}}{\northeastborder}
		\else
	  		\southwestborder	
	  	\pgfpointborderrectangle{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@right}}{\pgfpoint{-\pgf@x}{-\pgf@y}}
		\fi
	}
	
	#1
	
	\backgroundpath{	
		\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}
		
		\northeast
		\pgf@circ@res@up = \pgf@y 
		\pgf@circ@res@zero = 0cm
		\pgf@circ@res@left = -\pgf@x
		\pgf@circ@res@right = \pgf@x
		\southwest
		\pgf@circ@res@down = \pgf@y

 		\pgfstartlinewidth=\pgflinewidth
		\pgfsetcornersarced{\pgfpointorigin}% do not use rounded corners!
		#6
			
		\pgfsetlinewidth{\pgfstartlinewidth}
	}
	}
}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%% Standard bipole shapes declarations

%% Resistor
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/resistor/height}}{resistor}{\ctikzvalof{bipoles/resistor/height}}{\ctikzvalof{bipoles/resistor/width}}{
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgftransformationadjustments
	\pgfmathsetlength{\pgf@circ@res@step}{\ctikzvalof{bipoles/resistor/width}\pgf@circ@Rlen+\pgfhorizontaltransformationadjustment*0.5*\pgflinewidth}
	\divide \pgf@circ@res@step by 12
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left-\pgfhorizontaltransformationadjustment*0.5*\pgflinewidth}{\pgf@circ@res@zero}}
	\pgf@circ@res@other = \pgf@circ@res@left
	\advance\pgf@circ@res@other by \pgf@circ@res@step 
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@up}}
	\advance\pgf@circ@res@other by 2\pgf@circ@res@step 
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@down}}
	\advance\pgf@circ@res@other by 2\pgf@circ@res@step
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@up}}
	\advance\pgf@circ@res@other by 2\pgf@circ@res@step
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@down}}
	\advance\pgf@circ@res@other by 2\pgf@circ@res@step
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@up}}
	\advance\pgf@circ@res@other by 2\pgf@circ@res@step
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@down}}
	\advance\pgf@circ@res@other by \pgf@circ@res@step
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@zero}}
	\pgfsetbeveljoin
	\pgfusepath{draw}
}



%% Variable resistor
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/vresistor/height}}{vresistor}{\ctikzvalof{bipoles/vresistor/height}}{\ctikzvalof{bipoles/vresistor/width}}{		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgftransformationadjustments
	\pgfmathsetlength{\pgf@circ@res@step}{\ctikzvalof{bipoles/resistor/width}\pgf@circ@Rlen+\pgfhorizontaltransformationadjustment*0.5*\pgflinewidth}
	\divide \pgf@circ@res@step by 12
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left-\pgfhorizontaltransformationadjustment*0.5*\pgflinewidth}{\pgf@circ@res@zero}}
	
	\pgf@circ@res@other = \pgf@circ@res@left
	\advance\pgf@circ@res@other by \pgf@circ@res@step 
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{.5\pgf@circ@res@up}}
	\advance\pgf@circ@res@other by 2\pgf@circ@res@step 
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{.5\pgf@circ@res@down}}
	\advance\pgf@circ@res@other by 2\pgf@circ@res@step
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{.5\pgf@circ@res@up}}
	\advance\pgf@circ@res@other by 2\pgf@circ@res@step
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{.5\pgf@circ@res@down}}
	\advance\pgf@circ@res@other by 2\pgf@circ@res@step
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{.5\pgf@circ@res@up}}
	\advance\pgf@circ@res@other by 2\pgf@circ@res@step
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{.5\pgf@circ@res@down}}
	\advance\pgf@circ@res@other by \pgf@circ@res@step
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@zero}}
	\pgfsetbeveljoin
	\pgfusepath{draw}
	
	\pgfscope
		\pgfsetarrowsend{latex'}
		\pgfpathmoveto{\pgfpoint{.4\pgf@circ@res@other}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{-.4\pgf@circ@res@other}{\pgf@circ@res@down}}
		\pgfusepath{draw}
	\endpgfscope
}



%% Capacitor

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/capacitor/height}}{capacitor}{\ctikzvalof{bipoles/capacitor/height}}{\ctikzvalof{bipoles/capacitor/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/capacitor/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 5

		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@down}}

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
}


%% Polar Capacitor

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/pcapacitor/height}}{polarcapacitor}{\ctikzvalof{bipoles/pcapacitor/height}}{\ctikzvalof{bipoles/pcapacitor/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/pcapacitor/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 5

		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
				
		\pgfscope
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left+ \ctikzvalof{bipoles/pcapacitor/bend width}\pgf@circ@res@left}{\pgf@circ@res@up}}
			\pgftransformrotate{-90}
			\pgfpathsine{\pgfpoint{\pgf@circ@res@up}{-\ctikzvalof{bipoles/pcapacitor/bend width}\pgf@circ@res@left}}
			\pgfpathcosine{\pgfpoint{\pgf@circ@res@up}{\ctikzvalof{bipoles/pcapacitor/bend width}\pgf@circ@res@left}}
			\pgfusepath{draw}
		\endpgfscope
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
}

%% Electrolytic Capacitor

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/ecapacitor/height}}{ecapacitor}{\ctikzvalof{bipoles/ecapacitor/height}}{\ctikzvalof{bipoles/ecapacitor/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/ecapacitor/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 5
		\pgfsetrectcap
		% % % Draw plus pole
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{.4\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{.4\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfsetfillcolor{white} 
		\pgfusepath{draw,fill}
		% % Draw minus pole
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{.4\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{.4\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
				 \pgfsetfillcolor{black} 
				\pgfusepath{draw,fill}
		\pgfsetfillcolor{black} 
		% % plus pole annotation
		\pgftext[right,at=\pgfpoint{1.2\pgf@circ@res@left}{.6\pgf@circ@res@up}]
		{\pgfkeysvalueof{/tikz/circuitikz/bipoles/ecapacitor/font} $+$}	
}

%% Battery

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/battery/height}}{battery}{\ctikzvalof{bipoles/battery/height}}{\ctikzvalof{bipoles/battery/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/battery/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 6

		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@down}}

		\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@step}{.5\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{-\pgf@circ@res@step}{.5\pgf@circ@res@down}}

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{\pgf@circ@res@down}}

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{.5\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{.5\pgf@circ@res@down}}

		\pgfusepath{draw}
}


%% Battery 1 % poles with equl thickness

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/battery1/height}}{battery1}{\ctikzvalof{bipoles/battery1/height}}{\ctikzvalof{bipoles/battery1/width}}{
		\pgfpathmoveto{\pgfpoint{.33\pgf@circ@res@right}{0}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0}}
		\pgfpathmoveto{\pgfpoint{.33\pgf@circ@res@left}{0}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{0}}
		\pgfusepath{draw}

		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{.33\pgf@circ@res@right}{.5\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{.33\pgf@circ@res@right}{.5\pgf@circ@res@down}}

		\pgfpathmoveto{\pgfpoint{.33\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{.33\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfusepath{draw}
}

%% Battery 2 % negative pole thicker

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/battery2/height}}{battery2}{\ctikzvalof{bipoles/battery2/height}}{\ctikzvalof{bipoles/battery2/width}}{
		\pgfpathmoveto{\pgfpoint{.33\pgf@circ@res@right}{0}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0}}
		\pgfpathmoveto{\pgfpoint{.33\pgf@circ@res@left}{0}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{0}}
		\pgfusepath{draw}

		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{.33\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{.33\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		\pgfsetlinewidth{3\pgflinewidth}
		\pgfpathmoveto{\pgfpoint{.33\pgf@circ@res@right}{.5\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{.33\pgf@circ@res@right}{.5\pgf@circ@res@down}}
		\pgfusepath{draw}
}


%% cute inductor

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/cuteinductor/lower coil height}}{cuteinductor}{\ctikzvalof{bipoles/cuteinductor/height}}{\ctikzvalof{bipoles/cuteinductor/width}}{
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgftransformationadjustments

	\pgfmathsetlength{\pgf@circ@res@other}%width of small coil
	{0.5*\ctikzvalof{bipoles/cuteinductor/coil aspect}*\ctikzvalof{bipoles/cuteinductor/width}*\pgf@circ@Rlen/(\ctikzvalof{bipoles/cuteinductor/coils}-1)}


	\pgfmathsetlength{\pgf@circ@res@step}
		{(\ctikzvalof{bipoles/cuteinductor/width}*\pgf@circ@Rlen+\pgfhorizontaltransformationadjustment\pgflinewidth+(\ctikzvalof{bipoles/cuteinductor/coils}-1)*2*\pgf@circ@res@other)/\ctikzvalof{bipoles/cuteinductor/coils}/2}

	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left-\pgfhorizontaltransformationadjustment*0.5*\pgflinewidth}{-\pgfverticaltransformationadjustment*0.4*\pgfstartlinewidth}}%correct value would be 0.5 but arcs are not really flat, therefore 0.4 is better is (almost) all cases
	\foreach \x in {2,...,\ctikzvalof{bipoles/cuteinductor/coils}}
	{
		\pgfpatharc{180}{0}{\pgf@circ@res@step and \pgf@circ@res@up}
		\pgfpatharc{0}{-180}{\pgf@circ@res@other and -\pgf@circ@res@down}
	}
	\pgfpatharc{180}{0}{\pgf@circ@res@step and \pgf@circ@res@up}
	\pgfsetbuttcap
	\pgfsetbeveljoin
	\pgfusepath{stroke}
}

%% variable cute inductor

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/vcuteinductor/lower coil height}}{vcuteinductor}{\ctikzvalof{bipoles/vcuteinductor/height}}{\ctikzvalof{bipoles/vcuteinductor/width}}{
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgftransformationadjustments	
	
	\pgfmathsetlength{\pgf@circ@res@other}%width of small coil
	{0.5*\ctikzvalof{bipoles/vcuteinductor/coil aspect}*\ctikzvalof{bipoles/vcuteinductor/width}*\pgf@circ@Rlen/(\ctikzvalof{bipoles/vcuteinductor/coils}-1)}


	\pgfmathsetlength{\pgf@circ@res@step}
		{(\ctikzvalof{bipoles/vcuteinductor/width}*\pgf@circ@Rlen+\pgfhorizontaltransformationadjustment\pgflinewidth+(\ctikzvalof{bipoles/vcuteinductor/coils}-1)*2*\pgf@circ@res@other)/\ctikzvalof{bipoles/vcuteinductor/coils}/2}

	\pgfscope
		\pgfsetarrowsend{latex'}
		\pgfpathmoveto{\pgfpoint{.4\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{.4\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfusepath{draw}
	\endpgfscope

	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left-\pgfhorizontaltransformationadjustment*0.5*\pgflinewidth}{-\pgfverticaltransformationadjustment*0.4*\pgfstartlinewidth}}%correct value would be 0.5 but arcs are not really flat, therefore 0.4 is better is (almost) all cases
	\foreach \x in {2,...,\ctikzvalof{bipoles/vcuteinductor/coils}}
	{
		\pgfpatharc{180}{0}{\pgf@circ@res@step and .5\pgf@circ@res@up}
		\pgfpatharc{0}{-180}{\pgf@circ@res@other and -.5\pgf@circ@res@down}
	}
	\pgfpatharc{180}{0}{\pgf@circ@res@step and .5\pgf@circ@res@up}
	\pgfsetbuttcap
	\pgfsetbeveljoin
	\pgfusepath{stroke}
}

%% american inductor

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/americaninductor/height 2}}{americaninductor}{\ctikzvalof{bipoles/americaninductor/height}}{\ctikzvalof{bipoles/americaninductor/width}}{
	\pgf@circ@res@step=\ctikzvalof{bipoles/americaninductor/width}\pgf@circ@Rlen
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}	
	\pgftransformationadjustments
	\advance \pgf@circ@res@step by \pgfhorizontaltransformationadjustment\pgflinewidth
	\divide \pgf@circ@res@step by \ctikzvalof{bipoles/americaninductor/coils}
	\divide \pgf@circ@res@step by 2
	\pgf@circ@res@other = \ctikzvalof{bipoles/americaninductor/coil height}\pgf@circ@Rlen

	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left-\pgfhorizontaltransformationadjustment*0.5*\pgflinewidth}{-\pgfverticaltransformationadjustment*0.4*\pgfstartlinewidth}}%correct value would be 0.5 but arcs are not really flat, therefore 0.4 is better is (almost) all cases
	\foreach \x in {1,...,\ctikzvalof{bipoles/americaninductor/coils}}
	{
	\pgfpatharc{180}{0}{\pgf@circ@res@step and  \pgf@circ@res@other}
	}
	\pgfsetbuttcap
	\pgfsetbeveljoin
	\pgfusepath{stroke}
}

%% variable american inductor

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/vamericaninductor/height 2}}{vamericaninductor}{\ctikzvalof{bipoles/vamericaninductor/height}}{\ctikzvalof{bipoles/vamericaninductor/width}}{
	\pgf@circ@res@step=\ctikzvalof{bipoles/vamericaninductor/width}\pgf@circ@Rlen
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgftransformationadjustments
	\advance \pgf@circ@res@step by \pgfhorizontaltransformationadjustment\pgflinewidth
	\divide \pgf@circ@res@step by \ctikzvalof{bipoles/vamericaninductor/coils}
	\divide \pgf@circ@res@step by 2
	\pgf@circ@res@other = \ctikzvalof{bipoles/vamericaninductor/coil height}\pgf@circ@Rlen

	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left-\pgfhorizontaltransformationadjustment*0.5*\pgflinewidth}{-\pgfverticaltransformationadjustment*0.4*\pgfstartlinewidth}}%correct value would be 0.5 but arcs are not really flat, therefore 0.4 is better is (almost) all cases
	\foreach \x in {1,...,\ctikzvalof{bipoles/vamericaninductor/coils}}
	{
	\pgfpatharc{180}{0}{\pgf@circ@res@step and  \pgf@circ@res@other}
	}
	\pgfsetbuttcap
	\pgfsetbeveljoin
	\pgfusepath{stroke}

	\pgfscope
		\pgfsetarrowsend{latex'}
		\pgfpathmoveto{\pgfpoint{.4\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{-.4\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfusepath{draw}
	\endpgfscope
}


%% Independent voltage source

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/vsource/height}}{vsource}{\ctikzvalof{bipoles/vsource/height}}{\ctikzvalof{bipoles/vsource/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

	\pgfpathellipse{\pgfpointorigin}{\pgfpoint{0}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@left}{0}}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@zero}}
	\pgfusepath{draw}
}


%% Independent voltage source - American style

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/vsourceam/height}}{vsourceAM}{\ctikzvalof{bipoles/vsourceam/height}}{\ctikzvalof{bipoles/vsourceam/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathellipse{\pgfpointorigin}{\pgfpoint{0}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@left}{0}}
	\pgfusepath{draw}
	\ifpgf@circ@oldvoltagedirection
		\pgftext[bottom,rotate=90,y=\ctikzvalof{bipoles/vsourceam/margin}\pgf@circ@res@down]{$+$}
		\pgftext[top,rotate=90,y=\ctikzvalof{bipoles/vsourceam/margin}\pgf@circ@res@up]{$-$}
	\else
		\pgftext[bottom,rotate=90,y=\ctikzvalof{bipoles/vsourceam/margin}\pgf@circ@res@down]{$-$}
		\pgftext[top,rotate=90,y=\ctikzvalof{bipoles/vsourceam/margin}\pgf@circ@res@up]{$+$}
	\fi
}



%% Independent sinusoidal voltage source
 
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/vsourcesin/height}}{vsourcesin}{\ctikzvalof{bipoles/vsourcesin/height}}{\ctikzvalof{bipoles/vsourcesin/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathellipse{\pgfpointorigin}{\pgfpoint{0}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@left}{0}}
	\pgfusepath{draw}		
		
		\pgf@circ@res@up = .5\pgf@circ@res@up
		\pgfscope
			\pgftransformrotate{90}
			\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@up}{0cm}}
			\pgfpathsine{\pgfpoint{.5\pgf@circ@res@up}{.5\pgf@circ@res@up}}
			\pgfpathcosine{\pgfpoint{.5\pgf@circ@res@up}{-.5\pgf@circ@res@up}}
			\pgfpathsine{\pgfpoint{.5\pgf@circ@res@up}{-.5\pgf@circ@res@up}}
			\pgfpathcosine{\pgfpoint{.5\pgf@circ@res@up}{.5\pgf@circ@res@up}}
			\pgfusepath{draw}
		\endpgfscope
}

% Triangle Voltage source - contributed by Ralf Farkas
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/vsourcetri/height}}{vsourcetri}{\ctikzvalof{bipoles/vsourcetri/height}}{\ctikzvalof{bipoles/vsourcetri/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathellipse{\pgfpointorigin}{\pgfpoint{0}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@left}{0}}
	\pgfusepath{draw}		
		
		\pgf@circ@res@up = .5\pgf@circ@res@up
		\pgfscope
			\pgftransformrotate{90}
			\pgfpathmoveto{\pgfpoint{-1\pgf@circ@res@up}{0cm}}
			\pgfpathlineto{\pgfpoint{-0.5\pgf@circ@res@up}{0.75\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{0.5\pgf@circ@res@up}{-0.75\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{1\pgf@circ@res@up}{0\pgf@circ@res@up}}
			\pgfusepath{draw}
		\endpgfscope
}


% Square Voltage source -  contributed by Alistair Kwan
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/vsourcesquare/height}}{vsourcesquare}{\ctikzvalof{bipoles/vsourcesquare/height}}{\ctikzvalof{bipoles/vsourcesquare/width}}{
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathellipse{\pgfpointorigin}{\pgfpoint{0}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@left}{0}}
	\pgfusepath{draw}
	\pgf@circ@res@up = .5\pgf@circ@res@up
	\pgfscope
		\pgftransformrotate{90}
		\pgfpathmoveto{\pgfpoint{-1\pgf@circ@res@up}{0cm}}
		\pgfpathlineto{\pgfpoint{-1\pgf@circ@res@up}{1\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0\pgf@circ@res@up}{1\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0\pgf@circ@res@up}{-1\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{1\pgf@circ@res@up}{-1\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{1\pgf@circ@res@up}{0\pgf@circ@res@up}}
		\pgfusepath{draw}
	\endpgfscope
}

% Triangle Voltage source - contributed by Ralf Farkas
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/vsourcetri/height}}{vsourcetri}{\ctikzvalof{bipoles/vsourcetri/height}}{\ctikzvalof{bipoles/vsourcetri/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathellipse{\pgfpointorigin}{\pgfpoint{0}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@left}{0}}
	\pgfusepath{draw}		
		
		\pgf@circ@res@up = .5\pgf@circ@res@up
		\pgfscope
			\pgftransformrotate{90}
			\pgfpathmoveto{\pgfpoint{-1\pgf@circ@res@up}{0cm}}
			\pgfpathlineto{\pgfpoint{-0.5\pgf@circ@res@up}{0.75\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{0.5\pgf@circ@res@up}{-0.75\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{1\pgf@circ@res@up}{0\pgf@circ@res@up}}
			\pgfusepath{draw}
		\endpgfscope
}


%% Empty Source
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/esource/height}}{esource}{\ctikzvalof{bipoles/esource/height}}{\ctikzvalof{bipoles/esource/width}}{
	\pgfpointorigin
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathellipse{\pgfpointorigin}{\pgfpoint{0}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@left}{0}}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{\pgf@circ@res@up}}
	\pgfusepath{draw}
}

%% PV Source
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/pvsource/height}}{pvsource}{\ctikzvalof{bipoles/pvsource/height}}{\ctikzvalof{bipoles/pvsource/width}}{
	\pgfpointorigin
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathellipse{\pgfpointorigin}{\pgfpoint{0}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@left}{0}}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{\pgf@circ@res@up}}
	\pgfusepath{draw}

	\pgfpathmoveto{\pgfpoint{.15\pgf@circ@res@right}{0}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0}}
	\pgfpathmoveto{\pgfpoint{.15\pgf@circ@res@left}{0}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{0}}
	\pgfusepath{draw}

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathmoveto{\pgfpoint{.15\pgf@circ@res@left}{.4\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{.15\pgf@circ@res@left}{.4\pgf@circ@res@down}}

	\pgfpathmoveto{\pgfpoint{.15\pgf@circ@res@right}{.6\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{.15\pgf@circ@res@right}{.6\pgf@circ@res@down}}
	\pgfusepath{draw}

	%Arrow Part
	\pgfscope
	\pgfsetarrowsend{latex}
	\pgfpathmoveto{\pgfpointadd{\pgfpoint{.3\pgf@circ@res@left}{0}}{\pgfpointpolar{-45}{2.2\pgf@circ@res@up}}}
	\pgfpathlineto{\pgfpointadd{\pgfpoint{.3\pgf@circ@res@left}{0}}{\pgfpointpolar{-45}{1.3\pgf@circ@res@up}}}
	\pgfusepath{draw}
	\pgfpathmoveto{\pgfpointadd{\pgfpoint{0}{0.3\pgf@circ@res@up}}{\pgfpointpolar{-45}{2.2\pgf@circ@res@up}}}
	\pgfpathlineto{\pgfpointadd{\pgfpoint{0}{0.3\pgf@circ@res@up}}{\pgfpointpolar{-45}{1.3\pgf@circ@res@up}}}
	\pgfusepath{draw}
	\endpgfscope

}

%% Empty Source
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/esource/height}}{esource}{\ctikzvalof{bipoles/esource/height}}{\ctikzvalof{bipoles/esource/width}}{
	\pgfpointorigin
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathellipse{\pgfpointorigin}{\pgfpoint{0}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@left}{0}}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{\pgf@circ@res@up}}
	\pgfusepath{draw}
}

%% DC Current Source with open shape
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/dcisource/height}}{dcisource}{\ctikzvalof{bipoles/dcisource/height}}{\ctikzvalof{bipoles/dcisource/width}}{
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathmoveto{\pgfpointorigin}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0}}\pgfpatharc{0}{90}{0.85\pgf@circ@res@right and \pgf@circ@res@up}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0}}\pgfpatharc{0}{-90}{0.85\pgf@circ@res@right and \pgf@circ@res@up}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0}}\pgfpatharc{180}{270}{0.85\pgf@circ@res@right and \pgf@circ@res@up}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0}}\pgfpatharc{180}{90}{0.85\pgf@circ@res@right and \pgf@circ@res@up}	
	\pgfusepath{draw}

	\pgfpathmoveto{\pgfpoint{.7\pgf@circ@res@left}{\pgf@circ@res@zero}}
	\pgfpathlineto{\pgfpoint{.6\pgf@circ@res@right}{\pgf@circ@res@zero}}
	\pgfusepath{draw}
	\pgfscope

	\pgftransformshift{\pgfpoint{.5\pgf@circ@res@right}{\pgf@circ@res@zero}}
	\pgfnode{currarrow}{center}{}{}{\pgfusepath{stroke}}
	\endpgfscope
}

%% DC-Voltage source
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/dcvsource/height}}{dcvsource}{\ctikzvalof{bipoles/dcvsource/height}}{\ctikzvalof{bipoles/dcvsource/width}}{
	\pgfpointorigin
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathellipse{\pgfpointorigin}{\pgfpoint{0}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@left}{0}}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{\pgf@circ@res@up}}
	\pgfusepath{draw}
	\pgfpathmoveto{\pgfpoint{.2\pgf@circ@res@up}{.5\pgf@circ@res@left}}
	\pgfpathlineto{\pgfpoint{.2\pgf@circ@res@up}{.5\pgf@circ@res@right}}
	\pgfpathmoveto{\pgfpoint{.2\pgf@circ@res@down}{.5\pgf@circ@res@left}}
	\pgfpathlineto{\pgfpoint{.2\pgf@circ@res@down}{.5\pgf@circ@res@right}}
	\pgfusepath{draw}	
}


%% Independent current source

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/isource/height}}{isource}{\ctikzvalof{bipoles/isource/height}}{\ctikzvalof{bipoles/isource/width}}{
	\pgfpointorigin
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathellipse{\pgfpointorigin}{\pgfpoint{0}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@left}{0}}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{\pgf@circ@res@down}}
	\pgfusepath{draw}
}

%% Independent double oo source

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/oosource/height}}{oosource}{\ctikzvalof{bipoles/oosource/height}}{\ctikzvalof{bipoles/oosource/width}}{
	\pgfpointorigin
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathcircle{\pgfpoint{\ctikzvalof{bipoles/oosource/circleoffset}\pgf@circ@res@left}{0}}
		{\ctikzvalof{bipoles/oosource/circlesize}\pgf@circ@res@left}
	\pgfpathcircle{\pgfpoint{\ctikzvalof{bipoles/oosource/circleoffset}\pgf@circ@res@right}{0}}
		{\ctikzvalof{bipoles/oosource/circlesize}\pgf@circ@res@right}	
	\pgfusepath{draw}
}


%% Independent current source - American

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/isourceam/height}}{isourceAM}{\ctikzvalof{bipoles/isourceam/height}}{\ctikzvalof{bipoles/isourceam/width}}{
	\pgfpointorigin
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathellipse{\pgfpointorigin}{\pgfpoint{0}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@left}{0}}
	\pgfusepath{draw}

	\pgfpathmoveto{\pgfpoint{.7\pgf@circ@res@left}{\pgf@circ@res@zero}}
	\pgfpathlineto{\pgfpoint{.7\pgf@circ@res@right}{\pgf@circ@res@zero}}
	\pgfusepath{draw}
	\pgfscope
		\pgftransformshift{\pgfpoint{.5\pgf@circ@res@right}{\pgf@circ@res@zero}}
		\pgfnode{currarrow}{center}{}{}{\pgfusepath{stroke}}
	\endpgfscope
}


%% Independent sinusoidal current source

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/isource/height}}{isourcesin}{\ctikzvalof{bipoles/isource/height}}{\ctikzvalof{bipoles/isource/width}}{
	\pgfpointorigin
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathellipse{\pgfpointorigin}{\pgfpoint{0}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@left}{0}}
	\pgfusepath{draw}
	
		\pgf@circ@res@up = .5\pgf@circ@res@up
		\pgfscope
			\pgftransformrotate{90}
			\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@up}{0cm}}
			\pgfpathsine{\pgfpoint{.5\pgf@circ@res@up}{.5\pgf@circ@res@up}}
			\pgfpathcosine{\pgfpoint{.5\pgf@circ@res@up}{-.5\pgf@circ@res@up}}
			\pgfpathsine{\pgfpoint{.5\pgf@circ@res@up}{-.5\pgf@circ@res@up}}
			\pgfpathcosine{\pgfpoint{.5\pgf@circ@res@up}{.5\pgf@circ@res@up}}
			\pgfusepath{draw}
		\endpgfscope

}


%% Controlled voltage source

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/cvsource/height}}{cvsource}{\ctikzvalof{bipoles/cvsource/height}}{\ctikzvalof{bipoles/cvsource/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@zero}{\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@zero}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@zero}{\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@zero}}
			\pgfusepath{draw}		
}




%% Controlled voltage source - American
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/cvsourceam/height}}{cvsourceAM}{\ctikzvalof{bipoles/cvsourceam/height}}{\ctikzvalof{bipoles/cvsourceam/width}}{
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@zero}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@zero}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@zero}{\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
	\pgfusepath{draw}

	\ifpgf@circ@oldvoltagedirection
		\pgftext[bottom,rotate=90,y=\ctikzvalof{bipoles/cvsourceam/margin}\pgf@circ@res@left]{$+$}
		\pgftext[top,rotate=90,y=\ctikzvalof{bipoles/cvsourceam/margin}\pgf@circ@res@right]{$-$}
	\else
		\pgftext[bottom,rotate=90,y=\ctikzvalof{bipoles/cvsourceam/margin}\pgf@circ@res@left]{$-$}
		\pgftext[top,rotate=90,y=\ctikzvalof{bipoles/cvsourceam/margin}\pgf@circ@res@right]{$+$}
	\fi
}


%% Controlled sinusoidal voltage source
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/cvsourcesin/height}}{cvsourcesin}{\ctikzvalof{bipoles/cvsourcesin/height}}{\ctikzvalof{bipoles/cvsourcesin/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

		\pgfscope
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@zero}{\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@zero}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@zero}{\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
			\pgfusepath{draw}		
		\endpgfscope	

		\pgf@circ@res@up = .5\pgf@circ@res@up
		\pgfscope
			\pgftransformrotate{90}
			\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@up}{0cm}}
			\pgfpathsine{\pgfpoint{.5\pgf@circ@res@up}{.5\pgf@circ@res@up}}
			\pgfpathcosine{\pgfpoint{.5\pgf@circ@res@up}{-.5\pgf@circ@res@up}}
			\pgfpathsine{\pgfpoint{.5\pgf@circ@res@up}{-.5\pgf@circ@res@up}}
			\pgfpathcosine{\pgfpoint{.5\pgf@circ@res@up}{.5\pgf@circ@res@up}}
			\pgfusepath{draw}
		\endpgfscope
}



%% Controlled sinusoidal current source

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/cvsourcesin/height}}{cisourcesin}{\ctikzvalof{bipoles/cvsourcesin/height}}{\ctikzvalof{bipoles/cvsourcesin/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

		\pgfscope
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@zero}{\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@zero}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@zero}{\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
			\pgfusepath{draw}		
		\endpgfscope	

		\pgf@circ@res@up = .5\pgf@circ@res@up
		\pgfscope
			\pgftransformrotate{90}
			\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@up}{0cm}}
			\pgfpathsine{\pgfpoint{.5\pgf@circ@res@up}{.5\pgf@circ@res@up}}
			\pgfpathcosine{\pgfpoint{.5\pgf@circ@res@up}{-.5\pgf@circ@res@up}}
			\pgfpathsine{\pgfpoint{.5\pgf@circ@res@up}{-.5\pgf@circ@res@up}}
			\pgfpathcosine{\pgfpoint{.5\pgf@circ@res@up}{.5\pgf@circ@res@up}}
			\pgfusepath{draw}
		\endpgfscope
}




%% Controlled current source

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/cisource/height}}{cisource}{\ctikzvalof{bipoles/cisource/height}}{\ctikzvalof{bipoles/cisource/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@zero}{\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@zero}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@zero}{\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@zero}{\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@zero}{\pgf@circ@res@down}}
			\pgfusepath{draw}		
}




%% Controlled current source - American

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/cisourceam/height}}{cisourceAM}{\ctikzvalof{bipoles/cisourceam/height}}{\ctikzvalof{bipoles/cisourceam/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@zero}{\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@zero}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@zero}{\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
			\pgfusepath{draw}		

	\pgfpathmoveto{\pgfpoint{.7\pgf@circ@res@left}{\pgf@circ@res@zero}}
	\pgfpathlineto{\pgfpoint{.7\pgf@circ@res@right}{\pgf@circ@res@zero}}
	\pgfusepath{draw}
	\pgfscope
		\pgftransformshift{\pgfpoint{.5\pgf@circ@res@right}{\pgf@circ@res@zero}}
		\pgfnode{currarrow}{center}{}{}{\pgfusepath{stroke}}
	\endpgfscope
}

%% Black generic diode

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/diode/height}}{fulldiode}{\ctikzvalof{bipoles/diode/height}}{\ctikzvalof{bipoles/diode/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

	\pgfscope
		\pgftransformxshift{\pgf@circ@res@left}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfusepath{draw,fill}
	\endpgfscope
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfusepath{draw}
}

%% Black Zener diode

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/diode/height}}{fullzdiode}{\ctikzvalof{bipoles/diode/height}}{\ctikzvalof{bipoles/diode/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

	\pgfscope
		\pgftransformxshift{\pgf@circ@res@left}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfusepath{draw,fill}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-.6\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfusepath{draw}
	\endpgfscope
}

%% Black alternative zigzag Zener diode
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/diode/height}}{fullzzdiode}{\ctikzvalof{bipoles/diode/height}}{\ctikzvalof{bipoles/diode/width}}{

    \pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

    \pgfscope
        \pgftransformxshift{\pgf@circ@res@left}
        \pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
        \pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
        \pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
        \pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
        \pgfusepath{draw,fill}
        \pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-1.8\pgf@circ@res@left}{\pgf@circ@res@down-0.5\pgf@circ@res@up}}
        \pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@down}}
        \pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@up}}
        \pgfpathlineto{\pgfpoint{\pgf@circ@res@right-0.2\pgf@circ@res@left}{\pgf@circ@res@up-0.5\pgf@circ@res@down}}
        \pgfusepath{draw}
    \endpgfscope
}

%% Black Schottky diode

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/diode/height}}{fullsdiode}{\ctikzvalof{bipoles/diode/height}}{\ctikzvalof{bipoles/diode/width}}{
		
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfscope
		\pgftransformxshift{\pgf@circ@res@left}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfusepath{draw,fill}
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-.6\pgf@circ@res@left}{.6\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-.6\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-1.4\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-1.4\pgf@circ@res@left}{.6\pgf@circ@res@up}}
		\pgfusepath{draw}
	\endpgfscope

}

%% Black tunnel diode

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/diode/height}}{fulltdiode}{\ctikzvalof{bipoles/diode/height}}{\ctikzvalof{bipoles/diode/width}}{
		
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfscope
		\pgftransformxshift{\pgf@circ@res@left}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfusepath{draw,fill}

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-.6\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-.6\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfusepath{draw}
	\endpgfscope
}

%% Black light emitting diode

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/diode/height}}{fulllediode}{\ctikzvalof{bipoles/diode/height}}{\ctikzvalof{bipoles/diode/width}}{
		
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfscope
		\pgftransformxshift{\pgf@circ@res@left}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfusepath{draw,fill}
	\endpgfscope
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfusepath{draw}

			\pgfsetlinewidth{\pgfstartlinewidth}
			\pgfsetarrowsend{latex'}
			\pgfpathmoveto{\pgfpoint{-0.4\pgf@circ@res@right}{\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{0.6\pgf@circ@res@right}{2\pgf@circ@res@up}}
			\pgfusepath{draw}
			\pgfpathmoveto{\pgfpoint{0.2\pgf@circ@res@right}{0.8\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{1.2\pgf@circ@res@right}{1.8\pgf@circ@res@up}}
			\pgfusepath{draw}

}

%% Black photodiode

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/diode/height}}{fullpdiode}{\ctikzvalof{bipoles/diode/height}}{\ctikzvalof{bipoles/diode/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfscope
		\pgftransformxshift{\pgf@circ@res@left}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfusepath{draw,fill}
	\endpgfscope
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfusepath{draw}

			\pgfsetlinewidth{\pgfstartlinewidth}
			\pgfsetarrowsstart{latex'}
			\pgfpathmoveto{\pgfpoint{-0.4\pgf@circ@res@right}{\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{0.6\pgf@circ@res@right}{2\pgf@circ@res@up}}
			\pgfusepath{draw}
			\pgfpathmoveto{\pgfpoint{0.2\pgf@circ@res@right}{0.8\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{1.2\pgf@circ@res@right}{1.8\pgf@circ@res@up}}
			\pgfusepath{draw}
}

%% Black varcap

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/varcap/height}}{fullvarcap}{\ctikzvalof{bipoles/varcap/height}}{\ctikzvalof{bipoles/varcap/width}}{
	\pgf@circ@res@temp=\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
	\pgfsetlinewidth{\pgf@circ@res@temp}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-2\pgf@circ@res@temp}{0pt}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-2\pgf@circ@res@temp}{0pt}}
	\pgfusepath{draw,fill}
	%
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-2\pgf@circ@res@temp}{\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-2\pgf@circ@res@temp}{\pgf@circ@res@up}}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
	\pgfusepath{draw}
}

%% Empty generic diode

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/diode/height}}{emptydiode}{\ctikzvalof{bipoles/diode/height}}{\ctikzvalof{bipoles/diode/width}}{


	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

	\pgfscope
		\pgftransformxshift{\pgf@circ@res@left}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfusepath{draw}
	\endpgfscope
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfusepath{draw}
}

%% Empty Zener diode

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/diode/height}}{emptyzdiode}{\ctikzvalof{bipoles/diode/height}}{\ctikzvalof{bipoles/diode/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

	\pgfscope
		\pgftransformxshift{\pgf@circ@res@left}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-0.6\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfusepath{draw}
	\endpgfscope
}

%% Empty alternative zigzag Zener diode
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/diode/height}}{emptyzzdiode}{\ctikzvalof{bipoles/diode/height}}{\ctikzvalof{bipoles/diode/width}}{

    \pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

    \pgfscope
        \pgftransformxshift{\pgf@circ@res@left}
        \pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
        \pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
        \pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
        \pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
        \pgfusepath{draw}
        \pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-1.8\pgf@circ@res@left}{\pgf@circ@res@down-0.5\pgf@circ@res@up}}
        \pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@down}}
        \pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@up}}
        \pgfpathlineto{\pgfpoint{\pgf@circ@res@right-0.2\pgf@circ@res@left}{\pgf@circ@res@up-0.5\pgf@circ@res@down}}
        \pgfusepath{draw}
    \endpgfscope
}
%% Empty Schottky diode

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/diode/height}}{emptysdiode}{\ctikzvalof{bipoles/diode/height}}{\ctikzvalof{bipoles/diode/width}}{
		
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfscope
		\pgftransformxshift{\pgf@circ@res@left}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfusepath{draw}
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-.6\pgf@circ@res@left}{.6\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-.6\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-1.4\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-1.4\pgf@circ@res@left}{.6\pgf@circ@res@up}}
		\pgfusepath{draw}
	\endpgfscope

}

%% Empty tunnel diode

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/diode/height}}{emptytdiode}{\ctikzvalof{bipoles/diode/height}}{\ctikzvalof{bipoles/diode/width}}{
		
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfscope
		\pgftransformxshift{\pgf@circ@res@left}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfusepath{draw}

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-.6\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-.6\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfusepath{draw}
	\endpgfscope
}

%% Empty light emitting diode

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/diode/height}}{emptylediode}{\ctikzvalof{bipoles/diode/height}}{\ctikzvalof{bipoles/diode/width}}{
		
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfscope
		\pgftransformxshift{\pgf@circ@res@left}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfusepath{draw}
	\endpgfscope
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfusepath{draw}

			\pgfsetlinewidth{\pgfstartlinewidth}
			\pgfsetarrowsend{latex'}
			\pgfpathmoveto{\pgfpoint{-0.4\pgf@circ@res@right}{\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{0.6\pgf@circ@res@right}{2\pgf@circ@res@up}}
			\pgfusepath{draw}
			\pgfpathmoveto{\pgfpoint{0.2\pgf@circ@res@right}{0.8\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{1.2\pgf@circ@res@right}{1.8\pgf@circ@res@up}}
			\pgfusepath{draw}
}

%% Empty photodiode

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/diode/height}}{emptypdiode}{\ctikzvalof{bipoles/diode/height}}{\ctikzvalof{bipoles/diode/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfscope
		\pgftransformxshift{\pgf@circ@res@left}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfusepath{draw}
	\endpgfscope
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfusepath{draw}

			\pgfsetlinewidth{\pgfstartlinewidth}
			\pgfsetarrowsstart{latex'}
			\pgfpathmoveto{\pgfpoint{-0.4\pgf@circ@res@right}{\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{0.6\pgf@circ@res@right}{2\pgf@circ@res@up}}
			\pgfusepath{draw}
			\pgfpathmoveto{\pgfpoint{0.2\pgf@circ@res@right}{0.8\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{1.2\pgf@circ@res@right}{1.8\pgf@circ@res@up}}
			\pgfusepath{draw}
}

%% Empty varcap

\pgfcircdeclarebipole{
	\anchor{strokepathstart}{
			\northeast
				\pgf@y=0cm
				\advance\pgf@x by -\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgflinewidth
				\advance\pgf@x by -\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgflinewidth
	}
	\anchor{strokepathend}{
		\northeast
		\pgf@y=0cm
	}	
	}{\ctikzvalof{bipoles/varcap/height}}{emptyvarcap}{\ctikzvalof{bipoles/varcap/height}}{\ctikzvalof{bipoles/varcap/width}}{
	\pgf@circ@res@temp=\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
	\pgfsetlinewidth{\pgf@circ@res@temp}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-2\pgf@circ@res@temp}{0pt}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-2\pgf@circ@res@temp}{0pt}}
	\pgfusepath{draw}
	%
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-2\pgf@circ@res@temp}{\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-2\pgf@circ@res@temp}{\pgf@circ@res@up}}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
	\pgfusepath{draw}
}

%% (Closing) SPST
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/spst/depth}}{cspst}{\ctikzvalof{bipoles/spst/height}}{\ctikzvalof{bipoles/spst/width}}{
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0pt}}
	\pgfpathlineto{\pgfpoint{.6\pgf@circ@res@right}{\pgf@circ@res@up}}
	\pgfusepath{draw}
	
	\pgfsetarrowsstart{latex'}
	\pgfpathmoveto{\pgfpoint{.2\pgf@circ@res@right}{\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{.2\pgf@circ@res@right}{0\pgf@circ@res@down}}
	\pgfpatharcto{1.2\pgf@circ@res@right}{1.2\pgf@circ@res@right}{0}{0}{1}{\pgfpoint{.9\pgf@circ@res@left}{.9\pgf@circ@res@up}}
	\pgfsetbeveljoin
	\pgfusepath{draw}
}

%% Opening SPST
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/spst/depth}}{ospst}{\ctikzvalof{bipoles/spst/height}}{\ctikzvalof{bipoles/spst/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0pt}}
	\pgfpathlineto{\pgfpoint{.6\pgf@circ@res@right}{\pgf@circ@res@up}}
	\pgfusepath{draw}
	
	\pgfpathmoveto{\pgfpoint{.2\pgf@circ@res@right}{0.5\pgf@circ@res@down}}
	\pgfpatharcto{1.1\pgf@circ@res@right}{1.1\pgf@circ@res@right}{0}{0}{1}{\pgfpoint{.7\pgf@circ@res@left}{.9\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{1.2\pgf@circ@res@left}{1\pgf@circ@res@up}}
	\pgfsetarrowsend{latex'}
	\pgfsetbeveljoin
	\pgfusepath{draw}
}

%% Normal open Switch
\pgfcircdeclarebipole{}{0}{nos}{\ctikzvalof{bipoles/nos/height}}{\ctikzvalof{bipoles/nos/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0pt}}
	\pgfpathlineto{\pgfpoint{.9\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfsetbuttcap
	\pgfusepath{draw}
}

%% Normal closed Switch
\pgfcircdeclarebipole{}{0}{ncs}{\ctikzvalof{bipoles/ncs/height}}{\ctikzvalof{bipoles/ncs/width}}{
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0pt}}
	\pgfpathlineto{\pgfpoint{.9\pgf@circ@res@right}{\pgf@circ@res@up}}
	\pgfusepath{draw}
	\pgfsetlinewidth{\pgfstartlinewidth}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
	\pgfpathlineto{\pgfpoint{.2\pgf@circ@res@right}{0pt}}
	\pgfpathlineto{\pgfpoint{.2\pgf@circ@res@right}{\pgf@circ@res@up}}
	\pgfusepath{draw}
}

%% Push Button
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/pushbutton/height 2}}{pushbutton}{\ctikzvalof{bipoles/pushbutton/height}}{\ctikzvalof{bipoles/pushbutton/width}}{
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{.5\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{.5\pgf@circ@res@up}}
	\pgfpathmoveto{\pgfpoint{0}{.5\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{0}{\pgf@circ@res@up}}
	\pgfusepath{draw}
	
	\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
	\pgfnode{ocirc}{center}{}{}{\pgfusepath{draw}}
	\pgftransformshift{\pgfpoint{2\pgf@circ@res@right}{0pt}}
	\pgfnode{ocirc}{center}{}{}{\pgfusepath{draw}}
}

% % METERINGSHAPE
\long\def\drawmeteringcircle{
	\def\pgf@circ@temp{right}
	\ifx\tikz@res@label@pos\pgf@circ@temp
		\pgf@circ@res@step=-1.2\pgf@circ@res@up
	\else
		\def\pgf@circ@temp{below}
		\ifx\tikz@res@label@pos\pgf@circ@temp
			\pgf@circ@res@step=-1.2\pgf@circ@res@up
		\else
			\pgf@circ@res@step=1.2\pgf@circ@res@up
		\fi
	\fi
	%draw connections to circle
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}		
	\pgfpathlineto{\pgfpoint{.9\pgf@circ@res@left}{\pgf@circ@res@zero}}
	\pgfpathmoveto{\pgfpoint{.9\pgf@circ@res@right}{\pgf@circ@res@zero}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@zero}}
	\pgfusepath{draw}
	%draw circle
	\pgfscope
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathcircle{\pgfpointorigin}{.9\pgf@circ@res@up}
		\pgfusepath{draw}
	\endpgfscope
	%draw arrow
	\pgfscope
		\pgfsetarrowsend{latex}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{-\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfusepath{draw}
	\endpgfscope
}
%AMPEREMETER
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/ammeter/height}}{ammeter}{\ctikzvalof{bipoles/ammeter/height}}{\ctikzvalof{bipoles/ammeter/width}}{
	\drawmeteringcircle
	\pgfnode{circle}{center}{\textbf{A}}{}{}
}
%OHMMETER
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/ohmmeter/height}}{ohmmeter}{\ctikzvalof{bipoles/ohmmeter/height}}{\ctikzvalof{bipoles/ohmmeter/width}}{
	\drawmeteringcircle
	\pgfnode{circle}{center}{\boldmath$\Omega$}{}{}
}
%VOLTMETER
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/voltmeter/height}}{voltmeter}{\ctikzvalof{bipoles/voltmeter/height}}{\ctikzvalof{bipoles/voltmeter/width}}{
	\drawmeteringcircle
	\pgfnode{circle}{center}{\textbf{V}}{}{}
		
}

%% Short circuit

\pgfcircdeclarebipole{}{0}{short}{0}{0}{ }

%% Open circuit

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/open/height}}{open}{\ctikzvalof{bipoles/open/height}}{\ctikzvalof{bipoles/open/width}}{

}

%% Generic bipole - used as resistor by some (bleah)

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/generic/height}}{generic}{\ctikzvalof{bipoles/generic/height}}{\ctikzvalof{bipoles/generic/width}}{

		%\pgf@circ@res@step = \ctikzvalof{bipoles/resistor/width}\pgf@circ@Rlen
		%\divide \pgf@circ@res@step by 14

		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
					
		\pgfusepath{draw} 
}


%% fuse

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/fuse/height}}{fuse}{\ctikzvalof{bipoles/fuse/height}}{\ctikzvalof{bipoles/fuse/width}}{

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0}}
		\pgfusepath{draw}
		
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
					
		\pgfusepath{draw} 
}



%% Generic bipole, filled - used as inductor by some (bleah)

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/fullgeneric/height}}{fullgeneric}{\ctikzvalof{bipoles/fullgeneric/height}}{\ctikzvalof{bipoles/fullgeneric/width}}{

		%\pgf@circ@res@step = \ctikzvalof{bipoles/resistor/width}\pgf@circ@Rlen
		%\divide \pgf@circ@res@step by 14

		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
					
		\pgfusepath{draw,fill} 
}


%% Generic asymmetric bipole 

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/ageneric/height}}{ageneric}{\ctikzvalof{bipoles/ageneric/height}}{\ctikzvalof{bipoles/ageneric/width}}{
		%\pgf@circ@res@step = \ctikzvalof{bipoles/resistor/width}\pgf@circ@Rlen
		%\divide \pgf@circ@res@step by 14

		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
					
		\pgfusepath{draw} 

			\pgfpathrectanglecorners{\pgfpoint{.7\pgf@circ@res@right}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
			\pgfusepath{stroke,fill}		
}


%% asymmetric fuse

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/afuse/height}}{afuse}{\ctikzvalof{bipoles/afuse/height}}{\ctikzvalof{bipoles/afuse/width}}{

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0}}
		\pgfusepath{draw}
		
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
					
		\pgfusepath{draw}
		
		\pgfpathrectanglecorners{\pgfpoint{.7\pgf@circ@res@right}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
			\pgfusepath{stroke,fill}		 
}




%% Memristor

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/memristor/height}}{memristor}{\ctikzvalof{bipoles/memristor/height}}{\ctikzvalof{bipoles/memristor/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/resistor/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 14

		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{.72*\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{.72*\pgf@circ@res@left}{\ctikzvalof{bipoles/memristor/wave height}\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{.35*\pgf@circ@res@left}{\ctikzvalof{bipoles/memristor/wave height}\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{.35*\pgf@circ@res@left}{-\ctikzvalof{bipoles/memristor/wave height}\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{-.05*\pgf@circ@res@left}{-\ctikzvalof{bipoles/memristor/wave height}\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{-.05*\pgf@circ@res@left}{\ctikzvalof{bipoles/memristor/wave height}\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{.42*\pgf@circ@res@right}{\ctikzvalof{bipoles/memristor/wave height}\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{.42*\pgf@circ@res@right}{0pt}}
		\pgfpathlineto{\pgfpoint{.8*\pgf@circ@res@right}{0pt}}
					
		\pgfusepath{draw} 

			\pgfpathrectanglecorners{\pgfpoint{.7\pgf@circ@res@right}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
			\pgfusepath{stroke,fill}		
}




%% Generic empty tunable

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/tgeneric/height}}{tgeneric}{\ctikzvalof{bipoles/tgeneric/height}}{\ctikzvalof{bipoles/tgeneric/width}}{
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{.4\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{.4\pgf@circ@res@down}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfusepath{draw}
		
		\pgfscope
		\pgfsetarrowsend{latex'}
		\pgfpathmoveto{\pgfpoint{.5\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{-.5\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		\endpgfscope
}

%% Photoresistor

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/photoresistor/height 2}}{photoresistor}{\ctikzvalof{bipoles/photoresistor/height}}{\ctikzvalof{bipoles/photoresistor/width}}{
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@down}}{\pgfpoint{\pgf@circ@res@right}{-\pgf@circ@res@down}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfusepath{draw}
		
		\pgfscope
		\pgfsetarrowsend{latex'}
		\pgfpathmoveto{\pgfpoint{.7\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{.3\pgf@circ@res@right}{-1.2\pgf@circ@res@down}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{.45\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{.05\pgf@circ@res@right}{-1.2\pgf@circ@res@down}}
		\pgfusepath{draw}
		\endpgfscope
}




%% Thermistor
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/thermistor/height}}{thermistor}{\ctikzvalof{bipoles/thermistor/height}}{\ctikzvalof{bipoles/thermistor/width}}{
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thermistor/main}\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{-\pgfkeysvalueof{/tikz/circuitikz/bipoles/thermistor/main}\pgf@circ@res@up}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfusepath{draw}
		
		%\pgfscope
		\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@left}{-\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{.4\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		%\endpgfscope
}


%% Thermistor PTC
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/thermistorptc/height 2}}{thermistorptc}{\ctikzvalof{bipoles/thermistorptc/height}}{\ctikzvalof{bipoles/thermistorptc/width}}{
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thermistorptc/main}\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{-\pgfkeysvalueof{/tikz/circuitikz/bipoles/thermistorptc/main}\pgf@circ@res@up}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfusepath{draw}
		
		\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{.4\pgf@circ@res@left}{-\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{-\pgf@circ@res@up}}
		\pgfusepath{draw}
		
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgftext[top,x=.85\pgf@circ@res@left,y=.75\pgf@circ@res@down]{\tiny$\vartheta$}
		\pgfsetarrowsend{latex'}
		\pgfpathmoveto{\pgfpoint{.62\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{.62\pgf@circ@res@left}{.7\pgf@circ@res@down}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{.45\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{.45\pgf@circ@res@left}{.7\pgf@circ@res@down}}
		\pgfusepath{draw}
}

%% Thermistor NTC
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/thermistorntc/height 2}}{thermistorntc}{\ctikzvalof{bipoles/thermistorntc/height}}{\ctikzvalof{bipoles/thermistorntc/width}}{
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thermistorntc/main}\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{-\pgfkeysvalueof{/tikz/circuitikz/bipoles/thermistorntc/main}\pgf@circ@res@up}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfusepath{draw}
		
		\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{.4\pgf@circ@res@left}{-\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{-\pgf@circ@res@up}}
		\pgfusepath{draw}
		
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgftext[top,x=.85\pgf@circ@res@left,y=.75\pgf@circ@res@down]{\tiny$\vartheta$}
		\pgfsetarrowsend{latex'}
		\pgfpathmoveto{\pgfpoint{.62\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{.62\pgf@circ@res@left}{.7\pgf@circ@res@down}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{.45\pgf@circ@res@left}{.7\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{.45\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfusepath{draw}
}

%% thermocouple
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/thermocouple/height 2}}{thermocouple}{\ctikzvalof{bipoles/thermocouple/height}}{\ctikzvalof{bipoles/thermocouple/width}}{
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{.5\pgf@circ@res@down}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{.5\pgf@circ@res@down}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathlineto{\pgfpoint{0}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{0}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{.5\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0}}
		\pgfusepath{draw}
}

%% Varistor
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/varistor/height}}{varistor}{\ctikzvalof{bipoles/varistor/height}}{\ctikzvalof{bipoles/varistor/width}}{
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/bipoles/varistor/main}\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{-\pgfkeysvalueof{/tikz/circuitikz/bipoles/varistor/main}\pgf@circ@res@up}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfusepath{draw}
		
		\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@left}{-\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{.4\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\pgftext[top,x=.65\pgf@circ@res@left,y=1.2\pgf@circ@res@down]{{\tiny\textsf{U}}}
}



%% Generic full tunable

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/tfullgeneric/height}}{tfullgeneric}{\ctikzvalof{bipoles/tfullgeneric/height}}{\ctikzvalof{bipoles/tfullgeneric/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/resistor/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 14

		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{.4\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{.4\pgf@circ@res@down}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfusepath{draw,fill}
		
		\pgfscope
		\pgfsetarrowsend{latex'}
		\pgfpathmoveto{\pgfpoint{.5\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{-.5\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		\endpgfscope
}







%% Variable Capacitor

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/vcapacitor/height}}{vcapacitor}{\ctikzvalof{bipoles/vcapacitor/height}}{\ctikzvalof{bipoles/vcapacitor/width}}{
		%\pgf@circ@res@step = \ctikzvalof{bipoles/vcapacitor/width}\pgf@circ@Rlen
		\pgf@circ@res@step = \ctikzvalof{bipoles/vcapacitor/capacitor width} \pgf@circ@res@right

		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@step}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{-\pgf@circ@res@step}{\pgf@circ@res@down}}

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\pgfscope
		\pgfsetarrowsend{latex'}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		\endpgfscope
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{-\pgf@circ@res@step}{0pt}}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{0pt}}
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfusepath{draw}
}


%% Piezoelectric Element

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/piezoelectric/height}}{piezoelectric}{\ctikzvalof{bipoles/piezoelectric/height}}{\ctikzvalof{bipoles/piezoelectric/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/piezoelectric/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 5

		%% Outer markings
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@down}}

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}

		%% Inner Box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left+4}{\pgf@circ@res@up-1}}{\pgfpoint{\pgf@circ@res@right-4}{\pgf@circ@res@down+1}}
		\pgfusepath{draw}

}





%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%% Handling of terminals


%% Easily usable styles

\ctikzset{o-o/.style = {\circuitikzbasekey/bipole/nodes/left=empty, \circuitikzbasekey/bipole/nodes/right=empty}}
\ctikzset{-o/.style = {\circuitikzbasekey/bipole/nodes/left=none, \circuitikzbasekey/bipole/nodes/right=empty}}
\ctikzset{o-/.style = {\circuitikzbasekey/bipole/nodes/left=empty, \circuitikzbasekey/bipole/nodes/right=none}}
\ctikzset{*-o/.style = {\circuitikzbasekey/bipole/nodes/left=full, \circuitikzbasekey/bipole/nodes/right=empty}}
\ctikzset{o-*/.style = {\circuitikzbasekey/bipole/nodes/left=empty, \circuitikzbasekey/bipole/nodes/right=full}}
\ctikzset{d-o/.style = {\circuitikzbasekey/bipole/nodes/left=diamond, \circuitikzbasekey/bipole/nodes/right=empty}}
\ctikzset{o-d/.style = {\circuitikzbasekey/bipole/nodes/left=empty, \circuitikzbasekey/bipole/nodes/right=diamond}}
\ctikzset{*-/.style = {\circuitikzbasekey/bipole/nodes/left=full, \circuitikzbasekey/bipole/nodes/right=none}}
\ctikzset{-*/.style = {\circuitikzbasekey/bipole/nodes/left=none, \circuitikzbasekey/bipole/nodes/right=full}}
\ctikzset{d-/.style = {\circuitikzbasekey/bipole/nodes/left=diamond, \circuitikzbasekey/bipole/nodes/right=none}}
\ctikzset{-d/.style = {\circuitikzbasekey/bipole/nodes/left=none, \circuitikzbasekey/bipole/nodes/right=diamond}}
\ctikzset{*-*/.style = {\circuitikzbasekey/bipole/nodes/left=full, \circuitikzbasekey/bipole/nodes/right=full}}
\ctikzset{d-*/.style = {\circuitikzbasekey/bipole/nodes/left=diamond, \circuitikzbasekey/bipole/nodes/right=full}}
\ctikzset{*-d/.style = {\circuitikzbasekey/bipole/nodes/left=full, \circuitikzbasekey/bipole/nodes/right=diamond}}
\ctikzset{d-d/.style = {\circuitikzbasekey/bipole/nodes/left=diamond, \circuitikzbasekey/bipole/nodes/right=diamond}}

\ctikzset{.-/.style = {\circuitikzbasekey/bipole/nodes/left=rectjoinfill, \circuitikzbasekey/bipole/nodes/right=none}}
\ctikzset{.-*/.style = {\circuitikzbasekey/bipole/nodes/left=rectjoinfill, \circuitikzbasekey/bipole/nodes/right=full}}
\ctikzset{.-o/.style = {\circuitikzbasekey/bipole/nodes/left=rectjoinfill, \circuitikzbasekey/bipole/nodes/right=empty}}
\ctikzset{.-d/.style = {\circuitikzbasekey/bipole/nodes/left=rectjoinfill, \circuitikzbasekey/bipole/nodes/right=diamond}}
\ctikzset{-./.style = {\circuitikzbasekey/bipole/nodes/left=none, \circuitikzbasekey/bipole/nodes/right=rectjoinfill}}
\ctikzset{o-./.style = {\circuitikzbasekey/bipole/nodes/left=empty, \circuitikzbasekey/bipole/nodes/right=rectjoinfill}}
\ctikzset{*-./.style = {\circuitikzbasekey/bipole/nodes/left=full, \circuitikzbasekey/bipole/nodes/right=rectjoinfill}}
\ctikzset{d-./.style = {\circuitikzbasekey/bipole/nodes/left=diamond, \circuitikzbasekey/bipole/nodes/right=rectjoinfill}}
\ctikzset{.-./.style = {\circuitikzbasekey/bipole/nodes/left=rectjoinfill, \circuitikzbasekey/bipole/nodes/right=rectjoinfill}}

\tikzset{reversed/.style = {\circuitikzbasekey/bipole/inverted=true}}


%% The output routine

\def\drawpoles{
	\pgfextra{ \edef\pgf@circ@temp{\ctikzvalof{bipole/nodes/left}} \def\pgf@temp{diamond}  }
	\ifx\pgf@temp\pgf@circ@temp 
		 (\tikztostart) node[diamondpole] {} 
	\else 
		\pgfextra{ \def\pgf@temp{empty}  }
		\ifx\pgf@temp\pgf@circ@temp 
			 (\tikztostart) node[ocirc] {} 
		\else 
			\pgfextra{  \def\pgf@temp{full}  }
			\ifx\pgf@temp\pgf@circ@temp 
				(\tikztostart) node[circ] {} 
			\else 
				\pgfextra{ \def\pgf@temp{rectjoinfill} }
				\ifx\pgf@temp\pgf@circ@temp 
				 (\tikztostart) node[rectjoinfill] {} 
				\else 
				\fi
			\fi
		\fi
	\fi
	\pgfextra{ \edef\pgf@circ@temp{\ctikzvalof{bipole/nodes/right}} \def\pgf@temp{diamond}  }
	\ifx\pgf@temp\pgf@circ@temp 
		 (\tikztotarget) node[diamondpole] {} 
	\else 
		\pgfextra{ \def\pgf@temp{empty}  }
		\ifx\pgf@temp\pgf@circ@temp 
			 (\tikztotarget) node[ocirc] {} 
		\else 
			\pgfextra{  \def\pgf@temp{full}  }
			\ifx\pgf@temp\pgf@circ@temp 
				(\tikztotarget) node[circ] {} 
			\else 
				\pgfextra{ \def\pgf@temp{rectjoinfill} }
				\ifx\pgf@temp\pgf@circ@temp 
				 (\tikztotarget) node[rectjoinfill] {} 
				\else 
				\fi
			\fi
		\fi
	\fi
}



%% Lamp

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/lamp/height}}{lamp}{\ctikzvalof{bipoles/lamp/height}}{\ctikzvalof{bipoles/lamp/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

	\pgfpathellipse{\pgfpointorigin}{\pgfpoint{0}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@left}{0}}
	\pgfpathmoveto{\pgfpoint{.7071*\pgf@circ@res@left}{.7071*\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{.7071*\pgf@circ@res@right}{.7071*\pgf@circ@res@down}}
	\pgfpathmoveto{\pgfpoint{.7071*\pgf@circ@res@left}{.7071*\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{.7071*\pgf@circ@res@right}{.7071*\pgf@circ@res@up}}
	\pgfusepath{draw}
}


\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/tline/height}
                        }{tline}{\ctikzvalof{bipoles/tline/height}
                                 }{\ctikzvalof{bipoles/tline/width}
                                   }    
          {
          \pgf@circ@res@step=.2\pgf@circ@res@right % half x axis
          \pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
          \pgfpathellipse{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@step}{0}}
                         {\pgfpoint{\pgf@circ@res@step}{0}}
                         {\pgfpoint{0}{-\pgf@circ@res@up}}
          \pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@step}{\pgf@circ@res@up}}
          \pgfpathlineto{\pgfpoint{\pgf@circ@res@left+\pgf@circ@res@step}{\pgf@circ@res@up}}
          \pgfpatharc{-90}{90}{-\pgf@circ@res@step and -\pgf@circ@res@up}
          \pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@step}{\pgf@circ@res@down}}
          \pgfusepath{draw}
}




%% SQUID added by Cor Molenaar 5 March 2010

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/squid/height}}{squid}{\ctikzvalof{bipoles/squid/height}}{\ctikzvalof{bipoles/squid/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

	\pgfpathellipse{\pgfpointorigin}{\pgfpoint{0}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@left}{0}}
	\pgfpathmoveto{\pgfpoint{0.35*\pgf@circ@res@left}{1.35*\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{0.35*\pgf@circ@res@right}{0.65*\pgf@circ@res@up}}
	\pgfpathmoveto{\pgfpoint{0.35*\pgf@circ@res@left}{0.65*\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{0.35*\pgf@circ@res@right}{1.35*\pgf@circ@res@up}}
	\pgfpathmoveto{\pgfpoint{0.35*\pgf@circ@res@left}{1.35*\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{0.35*\pgf@circ@res@right}{0.65*\pgf@circ@res@down}}
	\pgfpathmoveto{\pgfpoint{0.35*\pgf@circ@res@left}{0.65*\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{0.35*\pgf@circ@res@right}{1.35*\pgf@circ@res@down}}

	\pgfusepath{draw}
}



% Generic barrier added by Cor Molenaar 5 March 2010

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/barrier/height}}{barrier}{\ctikzvalof{bipoles/barrier/height}}{\ctikzvalof{bipoles/barrier/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@step}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@step}}
	\pgfpathmoveto{\pgfpoint{0.35*\pgf@circ@res@left}{0.35*\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{0.35*\pgf@circ@res@right}{0.35*\pgf@circ@res@down}}
	\pgfpathmoveto{\pgfpoint{0.35*\pgf@circ@res@left}{0.35*\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{0.35*\pgf@circ@res@right}{0.35*\pgf@circ@res@up}}

	\pgfusepath{draw}
}


% Contributed by Danilo Piazzalunga
 
\pgfdeclareshape{buffer}
	{
	  \anchor{center}{\pgfpointorigin}
	  \savedanchor\northwest{%
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/bipoles/buffer/height}\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/bipoles/buffer/width}\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
	  }
	  \anchor{south}{
		\northwest
		\pgf@y=-\pgf@y
	  }
	  \savedanchor\left{%
	  	\pgf@y=0pt
	  }
	  \anchor{in}{
		\northwest
		\pgf@y=0pt
	  }
	  \anchor{out}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	  }
	  
	  \backgroundpath{			
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			
			
			\northwest
			\pgf@circ@res@up = \pgf@y 
			\pgf@circ@res@down = -\pgf@y
			\pgf@circ@res@right = -\pgf@x
			\pgf@circ@res@left = \pgf@x
			
	\pgfscope
		\pgfsetlinewidth{2\pgflinewidth}
		\pgftransformxshift{.7\pgf@circ@res@left}
		\pgf@circ@res@step=\pgf@circ@res@right
		\advance\pgf@circ@res@step by -\pgf@circ@res@left
		\pgf@circ@res@step=.7\pgf@circ@res@step
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{0pt}}
		\pgfusepath{draw}
	\endpgfscope
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{.7\pgf@circ@res@left}{0pt}}
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
		\pgfpathlineto{\pgfpoint{.7\pgf@circ@res@right}{0pt}}
	
		\pgfusepath{draw}
	  
	  }
	}





\pgfdeclareshape{plain amp}
	{
	  \anchor{center}{\pgfpointorigin}
	  \savedanchor\northwest{%
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/height}\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/width}\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
	  }
	  \anchor{south}{
		\northwest
		\pgf@y=-\pgf@y
	  }
	  \savedanchor\left{%
	  	\pgf@y=0pt
	  }
	  \savedanchor\inOne{%
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/height}\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/input height}\pgf@y
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/width}\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
	  }	  
	  \anchor{-}{
		\inOne
	  }
	  \anchor{+}{
		\inOne
		\pgf@y=-\pgf@y
	  }
	  \savedanchor\up{%
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/height}\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/width}\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
			\pgf@circ@res@up = \pgf@y 
			\pgf@circ@res@right = -\pgf@x
			\pgf@circ@res@left = \pgf@x
	    \pgfpointlineattime{
			\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/up pos}}{
			\pgfpoint{
				\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/port width}\pgf@circ@res@left}
				{\pgf@circ@res@up}}
			{\pgfpoint{.7\pgf@circ@res@right}{0pt}}
	  }
	  \anchor{up}{
		\up
	  }
	  \anchor{down}{
		\up
		\pgf@y=-\pgf@y
	  }
	  \anchor{out}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	  }
	  
	  \backgroundpath{			
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			
			
			\northwest
			\pgf@circ@res@up = \pgf@y 
			\pgf@circ@res@down = -\pgf@y
			\pgf@circ@res@right = -\pgf@x
			\pgf@circ@res@left = \pgf@x
			
	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/input height}\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/port width}\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/input height}\pgf@circ@res@up}}
	

	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/input height}\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/port width}\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/input height}\pgf@circ@res@down}}
		
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
	\pgfpathlineto{\pgfpoint{.7\pgf@circ@res@right}{0pt}}
	
	\pgfusepath{draw}

						
	\pgfscope
		\pgfsetlinewidth{2\pgflinewidth}
		\pgftransformxshift{.7\pgf@circ@res@left}
		\pgf@circ@res@step=\pgf@circ@res@right
		\advance\pgf@circ@res@step by -\pgf@circ@res@left
		\pgf@circ@res@step=.7\pgf@circ@res@step
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{0pt}}
		\pgfusepath{draw}
	\endpgfscope
		
		
	  
	  }
	}
	
%% Generic two port box
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/twoport/height}}{twoport}{\ctikzvalof{bipoles/twoport/height}}{\ctikzvalof{bipoles/twoport/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/twoport/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 
		\ifpgf@circuit@dashed
			\pgfsetdash{{0.1cm}{0.1cm}}{0cm} 
		\fi	
		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% rotate inner symbol
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 135 \ifnum \pgfcircmathresult < 225
			\pgftransformrotate{180}
		\fi\fi
		\ifnum \pgfcircmathresult > 225 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
		\fi\fi
		
		% draw inner symbol
		\pgftext[center,x=0,y=0]{\ctikzvalof{bipoles/twoport/text}}
		
}

%% voltage controled oscillator
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/vco/width}}{vco}{\ctikzvalof{bipoles/twoport/width}}{\ctikzvalof{bipoles/vco/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/vco/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 
		
		\ifpgf@circuit@dashed
			\pgfsetdash{{0.1cm}{0.1cm}}{0cm} 
		\fi	
		% draw circle
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathcircle{\pgfpoint{0}{0}} {\pgf@circ@res@step}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi

		% rotate inner symbol
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 134 \ifnum \pgfcircmathresult < 225  % 134 degree, because >= 135 is not possible
			\pgftransformrotate{180}
		\fi\fi
		\ifnum \pgfcircmathresult > 224 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
		\fi\fi
		
		% draw inner sine waves
		\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{-.5\pgf@circ@res@step}{0\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfusepath{draw}
		
}

%% bandpass filter
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/bandpass/width}}{bandpass}{\ctikzvalof{bipoles/bandpass/width}}{\ctikzvalof{bipoles/bandpass/width}}{
		
		\pgf@circ@res@step = \ctikzvalof{bipoles/bandpass/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step
		
		\ifpgf@circuit@dashed
			\pgfsetdash{{0.1cm}{0.1cm}}{0cm} 
		\fi	
		
		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% rotate inner symbol
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 134 \ifnum \pgfcircmathresult < 225  % 134 degree, because >= 135 is not possible
			\pgftransformrotate{180}
		\fi\fi
		\ifnum \pgfcircmathresult > 224 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
		\fi\fi
		
		% draw inner symbol
		\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
		\pgfsetarrows{-} %never draw arrows
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{-0.5\pgf@circ@res@step}{0.5\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{-0.15\pgf@circ@res@step}{0.35\pgf@circ@res@step}}
		\pgfpathlineto{\pgfpoint{0.15\pgf@circ@res@step}{0.65\pgf@circ@res@step}}
		\pgfusepath{draw}

		\pgfpathmoveto{\pgfpoint{-0.5\pgf@circ@res@step}{0}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfusepath{draw}

		\pgfpathmoveto{\pgfpoint{-0.5\pgf@circ@res@step}{-0.5\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{-0.15\pgf@circ@res@step}{-0.65\pgf@circ@res@step}}
		\pgfpathlineto{\pgfpoint{0.15\pgf@circ@res@step}{-0.35\pgf@circ@res@step}}
		\pgfusepath{draw}
}

%% bandstop filter
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/bandstop/width}}{bandstop}{\ctikzvalof{bipoles/bandstop/width}}{\ctikzvalof{bipoles/bandstop/width}}{
	\pgf@circ@res@step = \ctikzvalof{bipoles/bandstop/width}\pgf@circ@Rlen
	\divide \pgf@circ@res@step by 2

	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
	\pgf@circ@res@other = \pgf@circ@res@left
	\advance\pgf@circ@res@other by \pgf@circ@res@step

	\ifpgf@circuit@dashed
	\pgfsetdash{{0.1cm}{0.1cm}}{0cm}
	\fi

	% draw outer box
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
	\pgfusepath{draw}

	\ifpgf@circuit@inputarrow
	{
		\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
		\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
		\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
	}
	\fi

	% rotate inner symbol
	\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
	\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
	\pgftransformrotate{270}
	\fi\fi
	\ifnum \pgfcircmathresult > 134 \ifnum \pgfcircmathresult < 225% 134 degree, because >= 135 is not possible
	\pgftransformrotate{180}
	\fi\fi
	\ifnum \pgfcircmathresult > 224 \ifnum \pgfcircmathresult < 315
	\pgftransformrotate{90}
	\fi\fi

	% draw inner symbol
	\pgfsetdash{}{0pt}% always draw solid line for inner symbol
	\pgfsetarrows{-}%never draw arrows
	\pgfsetlinewidth{\pgfstartlinewidth}
	\pgfpathmoveto{\pgfpoint{-0.5\pgf@circ@res@step}{0.5\pgf@circ@res@step}}
	\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
	\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
	\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
	\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
	\pgfusepath{draw}

	\pgfpathmoveto{\pgfpoint{-0.5\pgf@circ@res@step}{0}}
	\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
	\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
	\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
	\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
	\pgfusepath{draw}
	\pgfpathmoveto{\pgfpoint{-0.15\pgf@circ@res@step}{-0.15\pgf@circ@res@step}}
	\pgfpathlineto{\pgfpoint{0.15\pgf@circ@res@step}{0.15\pgf@circ@res@step}}
	\pgfusepath{draw}

	\pgfpathmoveto{\pgfpoint{-0.5\pgf@circ@res@step}{-0.5\pgf@circ@res@step}}
	\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
	\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
	\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
	\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
	\pgfusepath{draw}
}

%% highpass filter
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/highpass/width}}{highpass}{\ctikzvalof{bipoles/highpass/width}}{\ctikzvalof{bipoles/highpass/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/highpass/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 

		\ifpgf@circuit@dashed
			\pgfsetdash{{0.1cm}{0.1cm}}{0cm} 
		\fi	
		
		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% rotate inner symbol
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 134 \ifnum \pgfcircmathresult < 225  % 134 degree, because >= 135 is not possible
			\pgftransformrotate{180}
		\fi\fi
		\ifnum \pgfcircmathresult > 224 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
		\fi\fi

		% draw inner symbol
		\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
		\pgfsetarrows{-} %never draw arrows
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{-0.5\pgf@circ@res@step}{0.5\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfusepath{draw}

		\pgfpathmoveto{\pgfpoint{-0.5\pgf@circ@res@step}{0}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{-0.15\pgf@circ@res@step}{-0.15\pgf@circ@res@step}}
		\pgfpathlineto{\pgfpoint{0.15\pgf@circ@res@step}{0.15\pgf@circ@res@step}}
		\pgfusepath{draw}

		\pgfpathmoveto{\pgfpoint{-0.5\pgf@circ@res@step}{-0.5\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{-0.15\pgf@circ@res@step}{-0.65\pgf@circ@res@step}}
		\pgfpathlineto{\pgfpoint{0.15\pgf@circ@res@step}{-0.35\pgf@circ@res@step}}
		\pgfusepath{draw}
}

%% lowpass filter
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/lowpass/width}}{lowpass}{\ctikzvalof{bipoles/lowpass/width}}{\ctikzvalof{bipoles/lowpass/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/lowpass/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 

		\ifpgf@circuit@dashed
			\pgfsetdash{{0.1cm}{0.1cm}}{0cm} 
		\fi	
		
		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% rotate inner symbol
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 134 \ifnum \pgfcircmathresult < 225  % 134 degree, because >= 135 is not possible
			\pgftransformrotate{180}
		\fi\fi
		\ifnum \pgfcircmathresult > 224 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
		\fi\fi

		% draw inner symbol
		\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
		\pgfsetarrows{-} %never draw arrows
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{-0.5\pgf@circ@res@step}{0.5\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{-0.15\pgf@circ@res@step}{0.35\pgf@circ@res@step}}
		\pgfpathlineto{\pgfpoint{0.15\pgf@circ@res@step}{0.65\pgf@circ@res@step}}
		\pgfusepath{draw}

		\pgfpathmoveto{\pgfpoint{-0.5\pgf@circ@res@step}{0}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{-0.15\pgf@circ@res@step}{-0.15\pgf@circ@res@step}}
		\pgfpathlineto{\pgfpoint{0.15\pgf@circ@res@step}{0.15\pgf@circ@res@step}}
		\pgfusepath{draw}

		\pgfpathmoveto{\pgfpoint{-0.5\pgf@circ@res@step}{-0.5\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfusepath{draw}
}

%% ADC
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/adc/width}}{adc}{\ctikzvalof{bipoles/adc/width}}{\ctikzvalof{bipoles/adc/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/adc/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 

		\ifpgf@circuit@dashed
			\pgfsetdash{{0.1cm}{0.1cm}}{0cm} 
		\fi	
		
		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% rotate inner symbol
		\def\texti{A}
		\def\textii{D}
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\def\texti{D}
			\def\textii{A}
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 134 \ifnum \pgfcircmathresult < 225  % 134 degree, because >= 135 is not possible
			\def\texti{D}
			\def\textii{A}
			\pgftransformrotate{180}
		\fi\fi
		\ifnum \pgfcircmathresult > 225 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
			\def\texti{A}
			\def\textii{D}
		\fi\fi

		% draw inner symbol
		\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
		\pgfsetarrows{-} %never draw arrows				
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfusepath{draw}
		
		\pgftext[center,x=0.45\pgf@circ@res@left,y=0.45\pgf@circ@res@up]{\textsf{\texti}}
		\pgftext[center,x=0.45\pgf@circ@res@right,y=0.45\pgf@circ@res@down]{\textsf{\textii}}
}

%% DAC
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/dac/width}}{dac}{\ctikzvalof{bipoles/dac/width}}{\ctikzvalof{bipoles/dac/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/dac/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 

		\ifpgf@circuit@dashed
			\pgfsetdash{{0.1cm}{0.1cm}}{0cm} 
		\fi	
		
		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% rotate inner symbol
		\def\texti{D}
		\def\textii{A}
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\def\texti{A}
			\def\textii{D}
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 134 \ifnum \pgfcircmathresult < 225  % 134 degree, because >= 135 is not possible
			\def\texti{A}
			\def\textii{D}
			\pgftransformrotate{180}
		\fi\fi
		\ifnum \pgfcircmathresult > 225 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
			\def\texti{D}
			\def\textii{A}
		\fi\fi

		% draw inner symbol
		\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
		\pgfsetarrows{-} %never draw arrows				
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfusepath{draw}
		
		\pgftext[center,x=0.45\pgf@circ@res@left,y=0.45\pgf@circ@res@up]{\textsf{\texti}}
		\pgftext[center,x=0.45\pgf@circ@res@right,y=0.45\pgf@circ@res@down]{\textsf{\textii}}
}

%% DSP
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/dsp/width}}{dsp}{\ctikzvalof{bipoles/dsp/width}}{\ctikzvalof{bipoles/dsp/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/dsp/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step

		\ifpgf@circuit@dashed
			\pgfsetdash{{0.1cm}{0.1cm}}{0cm} 
		\fi	
		
		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% rotate inner symbol
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 135 \ifnum \pgfcircmathresult < 225
			\pgftransformrotate{180}
		\fi\fi
		\ifnum \pgfcircmathresult > 225 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
		\fi\fi

		% draw inner symbol
		\pgftext[center,x=0,y=0]{\textsf{DSP}}
}

%% FFT
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/fft/width}}{fft}{\ctikzvalof{bipoles/fft/width}}{\ctikzvalof{bipoles/fft/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/fft/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step

		\ifpgf@circuit@dashed
			\pgfsetdash{{0.1cm}{0.1cm}}{0cm} 
		\fi	
		
		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% rotate inner symbol
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 135 \ifnum \pgfcircmathresult < 225
			\pgftransformrotate{180}
		\fi\fi
		\ifnum \pgfcircmathresult > 225 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
		\fi\fi

		% draw inner symbol
		\pgftext[center,x=0,y=0]{\textsf{FFT}}
}

%% Amplifier
\pgfcircdeclarebipole{}{
		\ifpgf@circuit@boxed
			\ctikzvalof{bipoles/twoport/width}
		\else
			\ctikzvalof{bipoles/amp/width}
		\fi
	}{amp}{
		\ifpgf@circuit@boxed
			\ctikzvalof{bipoles/twoport/width}
		\else
			\ctikzvalof{bipoles/amp/width}
		\fi
	}{
		\ifpgf@circuit@boxed
			\ctikzvalof{bipoles/twoport/width}
		\else
			\ctikzvalof{bipoles/amp/width}
		\fi
	}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/amp/width}\pgf@circ@Rlen

		\ifpgf@circuit@dashed
			\pgfsetdash{{0.1cm}{0.1cm}}{0cm} 
		\fi		

		% draw outer box
		\ifpgf@circuit@boxed
			\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}	
			\pgfnode{box}{center}{}{pgf@box}{\pgfusepath{draw}}
		\fi
		
		% draw input arrow
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi

		\ifpgf@circuit@boxed
			\pgfsetlinewidth{\pgfstartlinewidth}
			\pgfsetdash{}{0pt}	% draw solid line for inner symbol if no box is drawn
			\pgf@circ@res@step=.7\pgf@circ@res@step % scale amp symbol when inside a box
		\else
			\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}	
		\fi
		
		\pgfsetarrows{-} %never draw arrows
		\pgfsetlinewidth{\pgfstartlinewidth}

		\pgfpathmoveto{\pgfpoint{-0.5\pgf@circ@res@step}{0.55\pgf@circ@res@step}}
		\pgfpathlineto{\pgfpoint{0.5\pgf@circ@res@step}{0}}
		\pgfpathlineto{\pgfpoint{-0.5\pgf@circ@res@step}{-0.55\pgf@circ@res@step}}

		\pgfpathclose
		\pgfusepath{draw}
		
		% draw inner text
		\pgftext[center,x=-0.12\pgf@circ@res@step,y=0]{\ctikzvalof{bipoles/twoport/text}}
}


%% variable amplifier
\pgfcircdeclarebipole{}{
		\ifpgf@circuit@boxed
			\ctikzvalof{bipoles/twoport/width}
		\else
			\ctikzvalof{bipoles/amp/width}
		\fi
	}{vamp}{
		\ifpgf@circuit@boxed
			\ctikzvalof{bipoles/twoport/width}
		\else
			\ctikzvalof{bipoles/amp/width}
		\fi
	}{
		\ifpgf@circuit@boxed
			\ctikzvalof{bipoles/twoport/width}
		\else
			\ctikzvalof{bipoles/amp/width}
		\fi
	}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/amp/width}\pgf@circ@Rlen

		\ifpgf@circuit@dashed
			\pgfsetdash{{0.1cm}{0.1cm}}{0cm} 
		\fi	
		
		% draw outer box
		\ifpgf@circuit@boxed
			\pgfnode{box}{center}{}{pgf@box}{\pgfusepath{draw}}
		\fi

		% draw input arrow
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi

		\ifpgf@circuit@boxed
			\pgfsetlinewidth{\pgfstartlinewidth}
			\pgfsetdash{}{0pt}	% draw solid line for inner symbol if no box is drawn
			\pgf@circ@res@step=.7\pgf@circ@res@step % scale amp symbol when inside a box
		\else
			\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}	
		\fi
		

		\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
		\pgfsetarrows{-} %never draw arrows
		\pgfsetlinewidth{\pgfstartlinewidth}

		\pgfpathmoveto{\pgfpoint{-0.5\pgf@circ@res@step}{0.55\pgf@circ@res@step}}
		\pgfpathlineto{\pgfpoint{0.5\pgf@circ@res@step}{0}}
		\pgfpathlineto{\pgfpoint{-0.5\pgf@circ@res@step}{-0.55\pgf@circ@res@step}}

		\pgfpathclose
		\pgfusepath{draw}
		
		% draw inner text
		\pgftext[center,x=-0.12\pgf@circ@res@step,y=0]{\ctikzvalof{bipoles/twoport/text}}
		
		% draw arrow
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfsetarrowsend{latex}
		\pgfpathmoveto{\pgfpoint{-0.8\pgf@circ@res@step}{-0.5\pgf@circ@res@step}}
		\pgfpathlineto{\pgfpoint{0.6\pgf@circ@res@step}{0.6\pgf@circ@res@step}}
		\pgfusepath{draw}
}

%% pi attenuator
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/piattenuator/width}}{piattenuator}{\ctikzvalof{bipoles/piattenuator/width}}{\ctikzvalof{bipoles/piattenuator/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/piattenuator/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 
		
		\ifpgf@circuit@dashed
			\pgfsetdash{{0.1cm}{0.1cm}}{0cm} 
		\fi	
		
		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% rotate inner symbol
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 225 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
		\fi\fi

		% draw inner symbol
		\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
		\pgfsetarrows{-} %never draw arrows
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{0.4\pgf@circ@res@left}{0.4\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{0.4\pgf@circ@res@left}{0.4\pgf@circ@res@up}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{0.4\pgf@circ@res@right}{0.4\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{0.4\pgf@circ@res@right}{0.4\pgf@circ@res@up}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{0.6\pgf@circ@res@left}{0.4\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0.6\pgf@circ@res@right}{0.4\pgf@circ@res@up}}
		\pgfusepath{draw}
}

%% variable pi attenuator
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/vpiattenuator/width}}{vpiattenuator}{\ctikzvalof{bipoles/vpiattenuator/width}}{\ctikzvalof{bipoles/vpiattenuator/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/vpiattenuator/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 

		\ifpgf@circuit@dashed
			\pgfsetdash{{0.1cm}{0.1cm}}{0cm} 
		\fi	
		
		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% rotate inner symbol
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 225 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
		\fi\fi

		% draw inner symbol
		\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
		\pgfsetarrows{-} %never draw arrows
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{0.4\pgf@circ@res@left}{0.4\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{0.4\pgf@circ@res@left}{0.4\pgf@circ@res@up}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{0.4\pgf@circ@res@right}{0.4\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{0.4\pgf@circ@res@right}{0.4\pgf@circ@res@up}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{0.6\pgf@circ@res@left}{0.4\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0.6\pgf@circ@res@right}{0.4\pgf@circ@res@up}}
		\pgfusepath{draw}

		\pgfsetarrowsend{latex}
		\pgfpathmoveto{\pgfpoint{0.7\pgf@circ@res@left}{0.5\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{0.7\pgf@circ@res@right}{0.8\pgf@circ@res@up}}
		\pgfusepath{draw}
}

%% T attenuator
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/tattenuator/width}}{tattenuator}{\ctikzvalof{bipoles/tattenuator/width}}{\ctikzvalof{bipoles/tattenuator/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/tattenuator/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 
		
		\ifpgf@circuit@dashed
			\pgfsetdash{{0.1cm}{0.1cm}}{0cm} 
		\fi	
		
		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% rotate inner symbol
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 225 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
		\fi\fi

		% draw inner symbol
		\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
		\pgfsetarrows{-} %never draw arrows
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{0pt}{0.4\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{0pt}{0.4\pgf@circ@res@up}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{0.6\pgf@circ@res@left}{0.4\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0.6\pgf@circ@res@right}{0.4\pgf@circ@res@up}}
		\pgfusepath{draw}
}

%% variable T attenuator
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/vtattenuator/width}}{vtattenuator}{\ctikzvalof{bipoles/vtattenuator/width}}{\ctikzvalof{bipoles/vtattenuator/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/vtattenuator/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 

		\ifpgf@circuit@dashed
			\pgfsetdash{{0.1cm}{0.1cm}}{0cm} 
		\fi	
		
		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% rotate inner symbol
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 225 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
		\fi\fi

		% draw inner symbol
		\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
		\pgfsetarrows{-} %never draw arrows
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{0pt}{0.4\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{0pt}{0.4\pgf@circ@res@up}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{0.6\pgf@circ@res@left}{0.4\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0.6\pgf@circ@res@right}{0.4\pgf@circ@res@up}}
		\pgfusepath{draw}
		
		\pgfsetarrowsend{latex}
		\pgfpathmoveto{\pgfpoint{0.7\pgf@circ@res@left}{0.5\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{0.7\pgf@circ@res@right}{0.8\pgf@circ@res@up}}
		\pgfusepath{draw}
}

%% phase shifter
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/phaseshifter/width}}{phaseshifter}{\ctikzvalof{bipoles/phaseshifter/width}}{\ctikzvalof{bipoles/phaseshifter/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/phaseshifter/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 
		
		\ifpgf@circuit@dashed
			\pgfsetdash{{0.1cm}{0.1cm}}{0cm} 
		\fi	
		
		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% rotate inner symbol
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 135 \ifnum \pgfcircmathresult < 225
			\pgftransformrotate{180}
		\fi\fi
		\ifnum \pgfcircmathresult > 225 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
		\fi\fi
		
		% inner symbol
		\pgftext[center,x=0,y=0]{\Large$\varphi$}
}

%% variable phase shifter
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/phaseshifter/width}}{vphaseshifter}{\ctikzvalof{bipoles/vphaseshifter/width}}{\ctikzvalof{bipoles/vphaseshifter/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/vphaseshifter/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 
		
		\ifpgf@circuit@dashed
			\pgfsetdash{{0.1cm}{0.1cm}}{0cm} 
		\fi	
		
		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% rotate inner symbol
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 135 \ifnum \pgfcircmathresult < 225
			\pgftransformrotate{180}
		\fi\fi
		\ifnum \pgfcircmathresult > 225 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
		\fi\fi
		
		% inner symbol
		\pgftext[center,x=0,y=0]{\Large$\varphi$}
		
		\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfsetarrowsend{latex}
		\pgfpathmoveto{\pgfpoint{0.75\pgf@circ@res@left}{0.65\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{0.7\pgf@circ@res@right}{0.65\pgf@circ@res@up}}
		\pgfusepath{draw}
}

%% detector
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/detector/width}}{detector}{\ctikzvalof{bipoles/detector/width}}{\ctikzvalof{bipoles/detector/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/detector/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 
		
		\ifpgf@circuit@dashed
			\pgfsetdash{{0.1cm}{0.1cm}}{0cm} 
		\fi	
		
		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% draw inner stuff
		\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
		\pgfsetarrows{-} %never draw arrows
		\pgfsetlinewidth{0.8\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{0.75\pgf@circ@res@left}{0}}
		\pgfpathlineto{\pgfpoint{0.75\pgf@circ@res@right}{0}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@fulldiode
			\pgfmathparse{2\pgf@circ@res@up / \pgf@circ@Rlen / \ctikzvalof{bipoles/generic/width}}
			\pgftransformscale{\pgfmathresult}
			\pgfnode{fulldiodeshape}{center}{}{pgf@fulldiode}{\pgfusepath{fill}}
		\else
			\pgfmathparse{2\pgf@circ@res@up / \pgf@circ@Rlen / \ctikzvalof{bipoles/resistor/width}}
			\pgftransformscale{\pgfmathresult}
			\pgfnode{emptydiodeshape}{center}{}{pgf@emptydiode}{\pgfusepath{fill}}
		\fi
		
}




%% european gas filled surge arrester

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/european gas filled surge arrester/height}}{european gas filled surge arrester}{\ctikzvalof{bipoles/european gas filled surge arrester/height}}{\ctikzvalof{bipoles/european gas filled surge arrester/width}}{

		%\pgf@circ@res@step = \ctikzvalof{bipoles/resistor/width}\pgf@circ@Rlen
		%\divide \pgf@circ@res@step by 14

		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
					
		\pgfusepath{draw} 
		
		\pgfscope
		\pgfsetarrowsend{latex'}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/bipoles/european gas filled surge arrester/inside}\pgf@circ@res@left}{0pt}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}	
				\pgfusepath{draw} 
	
		\endpgfscope
}




%% american gas filled surge arrester

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/american gas filled surge arrester/height}}{american gas filled surge arrester}{\ctikzvalof{bipoles/american gas filled surge arrester/height}}{\ctikzvalof{bipoles/american gas filled surge arrester/width}}{
	%\def\pgf@circ@temp{right}
	%\ifx\tikz@res@label@pos\pgf@circ@temp
	%	\pgf@circ@res@step=-1.2\pgf@circ@res@up
	%\else
%		\def\pgf@circ@temp{below}
%		\ifx\tikz@res@label@pos\pgf@circ@temp
%			\pgf@circ@res@step=-1.2\pgf@circ@res@up
%		\else
%			\pgf@circ@res@step=1.2\pgf@circ@res@up
%		\fi
%	\fi

	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}		
	\pgfpointorigin	\pgf@circ@res@other =  \pgf@x  \advance \pgf@circ@res@other by -\pgf@circ@res@up
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@zero}}
	\pgfusepath{draw}

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

		\pgfscope
			\pgfpathcircle{\pgfpointorigin}{.9\pgf@circ@res@up}
			\pgfusepath{draw}		
		\endpgfscope	

	\pgfsetlinewidth{\pgfstartlinewidth}


	\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@zero}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@zero}}
	\pgfusepath{draw}

	\pgfnode{circle}{center}{}{}{}
	
	\pgfscope
		\pgfsetarrowsend{latex}
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@zero}}
		\pgfpathlineto{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/bipoles/american gas filled surge arrester/inside}\pgf@circ@res@right}{\pgf@circ@res@zero}}
		\pgfusepath{draw}	
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgfpathlineto{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/bipoles/american gas filled surge arrester/inside}\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgfusepath{draw}	
	\endpgfscope{}
	
	%\pgftransformshift{\pgfpoint{.25\pgf@circ@res@left}{.45\pgf@circ@res@down}}
	%\pgfnode{circ}{center}{}{}{}
	%\pgftransformshift{}
	\pgfcircle{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/bipoles/american gas filled surge arrester/dot x}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/bipoles/american gas filled surge arrester/dot y}\pgf@circ@res@down}}{\pgfkeysvalueof{/tikz/circuitikz/bipoles/american gas filled surge arrester/size}\pgf@circ@res@down}
	\pgfusepath{fill}
}

% % MECHANICAL SYMBOLS

%% mechanical capacitance - stiffness/spring

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/spring/height}}{spring}{\ctikzvalof{bipoles/spring/height}}{\ctikzvalof{bipoles/spring/width}}{
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgftransformationadjustments

	\pgfmathsetlength{\pgf@circ@res@step}
	{(\ctikzvalof{bipoles/spring/width}*\pgf@circ@Rlen+\pgfhorizontaltransformationadjustment*.5*\pgflinewidth)/16}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left-\pgfhorizontaltransformationadjustment*0.5*\pgflinewidth}{\pgf@circ@res@zero}}
	\pgfsetcornersarced{\pgfpoint{.5\pgf@circ@res@up}{.5\pgf@circ@res@up}}
	\pgf@circ@res@other = \pgf@circ@res@left
	\advance\pgf@circ@res@other by \pgf@circ@res@step
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@up}}
	\advance\pgf@circ@res@other by 2\pgf@circ@res@step 
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@down}}
	\advance\pgf@circ@res@other by 2\pgf@circ@res@step
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@up}}
	\advance\pgf@circ@res@other by 2\pgf@circ@res@step
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@down}}
	\advance\pgf@circ@res@other by 2\pgf@circ@res@step
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@up}}
	\advance\pgf@circ@res@other by 2\pgf@circ@res@step
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@down}}
	\advance\pgf@circ@res@other by 2\pgf@circ@res@step
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@up}}
	\advance\pgf@circ@res@other by 2\pgf@circ@res@step
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@down}}
	\advance\pgf@circ@res@other by \pgf@circ@res@step
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@zero}}
	\pgfsetbuttcap
	\pgfsetbeveljoin
	\pgfusepath{stroke}
}

%% mechanical inductance - mass
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/mass/box height}}{mass}{\ctikzvalof{bipoles/mass/height}}{\ctikzvalof{bipoles/mass/width}}{
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgftransformationadjustments
	\pgfpathrectangle{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@down}}
		{\pgfpoint{-2\pgf@circ@res@down}{-2\pgf@circ@res@down}}

\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}
	\pgfsetrectcap
	\pgfsetmiterjoin
	\pgfusepath{stroke}
}

%% mechanical resistor - damper
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/damper/height}}{damper}{\ctikzvalof{bipoles/damper/height}}{\ctikzvalof{bipoles/damper/width}}{
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
	\pgfpathlineto{\pgfpoint{\ctikzvalof{bipoles/damper/length}\pgf@circ@res@right}
					{\pgf@circ@res@zero}}
	\pgfusepath{stroke}

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}

	\pgfsetrectcap
	\pgfsetmiterjoin
	\pgfusepath{stroke}
	
	\pgfpathmoveto{\pgfpoint{\ctikzvalof{bipoles/damper/length}\pgf@circ@res@right}
						{.8\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\ctikzvalof{bipoles/damper/length}\pgf@circ@res@right}
						{.8\pgf@circ@res@up}}
	\pgfsetbuttcap
	\pgfusepath{stroke}
	
}


%%%---------- close: tex/pgfcircbipoles
%%%%%%%%%%% Springe nach tex/pgfcirctripoles
%%%---------- open: tex/pgfcirctripoles.tex
% Copyright 2007-2009 by Massimo Redaelli
%
% This file may be distributed and/or modified
%
% 1. under the LaTeX Project Public License and/or
% 2. under the GNU Public License.
%
% See the file doc/LICENSE for more details.

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%% Tripoles



\pgfdeclareshape{spdt}
	{
	  \savedanchor\northwest{%
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/spdt/height}\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/spdt/width}\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
	  }
	  \anchor{left}{%
	  	\northwest
	  	\pgf@y=0pt
	  }
	  \anchor{in}{
	  	\northwest
	  	\pgf@y=0pt
	  }	  
	  \anchor{out 1}{
		\northwest
		\pgf@x=-\pgf@x
	  }
	  \anchor{out 2}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@y=-\pgf@y
	  }
  	  \anchor{center}{
		\pgf@y=0pt
		\pgf@x=0pt
	  }
	  \anchor{east}{
	  	\northwest
		\pgf@y=0pt
	  	\pgf@x=-\pgf@x  
	  }
	  \anchor{west}{
	  	\northwest
		\pgf@y=0pt
	  }
	  \anchor{south}{
		\northwest
		\pgf@x=0pt
		\pgf@y=-\pgf@y
	  }
	  \anchor{north}{
		\northwest
		\pgf@x=0pt
	  }
	  \anchor{south west}{
		\northwest
		\pgf@y=-\pgf@y
	  }
	  \anchor{north east}{
		\northwest
		\pgf@x=-\pgf@x
	  }
	  \anchor{north west}{
		\northwest
	  }
	  \anchor{south east}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@y=-\pgf@y
	  }	  
	  \backgroundpath{			
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			
			
			\northwest
			\pgf@circ@res@up = \pgf@y 
			\pgf@circ@res@down = -\pgf@y
			\pgf@circ@res@right = -\pgf@x  
			\pgf@circ@res@left = \pgf@x  
			\pgf@circ@res@other = \pgfkeysvalueof{/tikz/circuitikz/tripoles/spdt/margin}\pgf@circ@res@left
			
		
	  	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@up}}
	  	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@down}}
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{0pt}}
		
		\pgfusepath{draw}
		
		\pgfscope
			\pgftransformshift{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@up}}
			\pgfnode{ocirc}{center}{}{spdt1}{\pgfusepath{stroke}}
		\endpgfscope
		\pgfscope
			\pgftransformshift{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@down}}
			\pgfnode{ocirc}{center}{}{}{\pgfusepath{stroke}}
		\endpgfscope
		\pgfscope
			\pgftransformshift{\pgfpoint{\pgf@circ@res@other}{0pt}}
			\pgfnode{ocirc}{center}{}{spdt2}{\pgfusepath{stroke}}
		\endpgfscope
		
		
		\pgfscope
			\pgfpathmoveto{\pgfpointshapeborder{spdt2}{\pgfpointorigin}}
			\pgfpathlineto{
				\pgfpointadd{\pgfpointshapeborder{spdt1}{\pgfpoint{-\pgf@circ@res@other}{-100pt}}}
				{\pgfpoint{-.05\pgf@circ@res@up}{-.05\pgf@circ@res@up}}
			}
			\pgfsetlinewidth{2\pgflinewidth}
			\pgfusepath{draw}
		\endpgfscope
	  }
	}
	
	
	
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%%
%%       Logic ports
%%






\long\def\pgfcircdeclarelogicport#1#2{
	\pgfdeclareshape{american #1 port}
	{
	  \savedanchor\northwest{%
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/american #1 port/height}\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/american #1 port/width}\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
	  }
	  \savedanchor\left{%
	  	\pgf@y=0pt
	  }
	  \savedanchor\inOne{%
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/american #1 port/height}\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/american #1 port/input height}\pgf@y
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/american #1 port/width}\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
	  }	  
	  \anchor{in 1}{
		\inOne
	  }
	  \anchor{in}{
		\inOne
	  }	  
	  \anchor{in 2}{
		\inOne
		\pgf@y=-\pgf@y
	  }
	  \anchor{out}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	  }
  	  \anchor{center}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-.8\pgf@x  
	  }
	  \anchor{east}{
	  	\left
	  	\pgf@x=-.8\pgf@x  
	  }
	  \anchor{west}{
	  	\left
	  }
	  \anchor{south}{
		\northwest
		\pgf@x=0pt
		\pgf@y=-\pgf@y
	  }
	  \anchor{north}{
		\northwest
		\pgf@x=0pt
	  }
	  \anchor{south west}{
		\northwest
		\pgf@y=-\pgf@y
	  }
	  \anchor{north east}{
		\northwest
		\pgf@x=-\pgf@x
	  }
	  \anchor{north west}{
		\northwest
	  }
	  \anchor{south east}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@y=-\pgf@y
	  }	  
	  \backgroundpath{			
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			
			
			\northwest
			\pgf@circ@res@up = \pgf@y 
			\pgf@circ@res@down = -\pgf@y
			\pgf@circ@res@right = -\pgf@x
			\pgf@circ@res@left = \pgf@x
			
			#2
	  
	  }
	}
}


\pgfcircdeclarelogicport{and}{
	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american and port/input height}\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american and port/port width}\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american and port/input height}\pgf@circ@res@up}}
	
	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american and port/input height}\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american and port/port width}\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american and port/input height}\pgf@circ@res@down}}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american and port/port width}\pgf@circ@res@right}
		{0pt}}
	
	\pgfusepath{draw}
	
	\pgfsetlinewidth{2\pgflinewidth}
	\pgfpathmoveto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american and port/port width}\pgf@circ@res@left}
		{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american and port/port width}\pgf@circ@res@left}
		{\pgf@circ@res@down}}
	\pgfpathcurveto
		{\pgfpoint{.0\pgf@circ@res@left}{\pgf@circ@res@down}}
		{\pgfpoint
			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american and port/port width}\pgf@circ@res@right}
			{.5\pgf@circ@res@down}}
		{\pgfpoint
			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american and port/port width}\pgf@circ@res@right}
			{0pt}}
	\pgfpathcurveto
		{\pgfpoint
			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american and port/port width}\pgf@circ@res@right}
			{.5\pgf@circ@res@up}}
		{\pgfpoint{.0\pgf@circ@res@left}{\pgf@circ@res@up}}
		{\pgfpoint
			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american and port/port width}\pgf@circ@res@left}
			{\pgf@circ@res@up}}	
	\pgfusepath{draw}
}



\pgfcircdeclarelogicport{nand}{
	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nand port/input height}\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nand port/port width}\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nand port/input height}\pgf@circ@res@up}}
	
	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nand port/input height}\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nand port/port width}\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nand port/input height}\pgf@circ@res@down}}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nand port/port width}\pgf@circ@res@right}
		{0pt}}
	
	\pgfusepath{draw}
	
	\pgfsetlinewidth{2\pgflinewidth}

	\pgf@circ@res@step = \pgfkeysvalueof{/tikz/circuitikz/tripoles/american nand port/circle width}\pgf@circ@res@right
	\pgf@circ@res@other = \pgfkeysvalueof{/tikz/circuitikz/tripoles/american nand port/port width}\pgf@circ@res@right
	
	\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@down}}
	\pgfpathcurveto
		{\pgfpoint{.0\pgf@circ@res@left}{\pgf@circ@res@down}}
		{\pgfpoint{\pgf@circ@res@other-\pgf@circ@res@step}{.5\pgf@circ@res@down}}
		{\pgfpoint{\pgf@circ@res@other-\pgf@circ@res@step}{0pt}}
	\pgfpathcurveto
		{\pgfpoint{\pgf@circ@res@other-\pgf@circ@res@step}{.5\pgf@circ@res@up}}
		{\pgfpoint{.0\pgf@circ@res@left}{\pgf@circ@res@up}}
		{\pgfpoint
			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nand port/port width}\pgf@circ@res@left}
			{\pgf@circ@res@up}}	
	\pgfpathellipse
		{\pgfpoint{\pgf@circ@res@other-.5\pgf@circ@res@step}{0pt}}
		{\pgfpoint{.5\pgf@circ@res@step}{0pt}}
		{\pgfpoint{0pt}{.5\pgf@circ@res@step}}

	\pgfusepath{draw}
}


\pgfcircdeclarelogicport{nor}{
	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/input height}\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint
		{(\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/port width}-\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/input skip})*\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/input height}\pgf@circ@res@up}}
	
	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/input height}\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint
		{(\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/port width}-\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/input skip})*\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/input height}\pgf@circ@res@down}}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/port width}\pgf@circ@res@right}
		{0pt}}	
	
	\pgfusepath{draw}
	
	\pgf@circ@res@other=\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/port width}\pgf@circ@res@right
	\pgf@circ@res@step = \pgfkeysvalueof{/tikz/circuitikz/tripoles/american nand port/circle width}\pgf@circ@res@right
		
	\pgfsetlinewidth{2\pgflinewidth}
	\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@up}}
	\pgfpathcurveto
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/aaa}\pgf@circ@res@left}{\pgf@circ@res@up}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/bbb}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/ccc}\pgf@circ@res@up}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/bbb}\pgf@circ@res@left}{0pt}}
	\pgfpathcurveto
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/bbb}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/ccc}\pgf@circ@res@down}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/aaa}\pgf@circ@res@left}{\pgf@circ@res@down}}
		{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@down}}	

	\pgfpathcurveto
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/ddd}\pgf@circ@res@left}{\pgf@circ@res@down}}
		{\pgfpoint{\pgf@circ@res@other-\pgf@circ@res@step}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/ccc}\pgf@circ@res@down}}
		{\pgfpoint{\pgf@circ@res@other-\pgf@circ@res@step}{0pt}}
	\pgfpathcurveto
		{\pgfpoint{\pgf@circ@res@other-\pgf@circ@res@step}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/ccc}\pgf@circ@res@up}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/ddd}\pgf@circ@res@left}{\pgf@circ@res@up}}
		{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@up}}	
		
	\pgfpathellipse
		{\pgfpoint{\pgf@circ@res@other-.5\pgf@circ@res@step}{0pt}}
		{\pgfpoint{.5\pgf@circ@res@step}{0pt}}
		{\pgfpoint{0pt}{.5\pgf@circ@res@step}}
		
	\pgfusepath{draw}
}




\pgfcircdeclarelogicport{or}{

	
	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/input height}\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint
		{(\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/port width}-\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/input skip})*\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/input height}\pgf@circ@res@up}}
	
	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/input height}\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint
		{(\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/port width}-\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/input skip})*\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/input height}\pgf@circ@res@down}}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/port width}\pgf@circ@res@right}
		{0pt}}	
	
	\pgfusepath{draw}
	\pgf@circ@res@other=\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/port width}\pgf@circ@res@right
	\pgfsetlinewidth{2\pgflinewidth}
	\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@up}}
	\pgfpathcurveto
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/aaa}\pgf@circ@res@left}{\pgf@circ@res@up}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/bbb}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/ccc}\pgf@circ@res@up}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/bbb}\pgf@circ@res@left}{0pt}}
	\pgfpathcurveto
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/bbb}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/ccc}\pgf@circ@res@down}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/aaa}\pgf@circ@res@left}{\pgf@circ@res@down}}
		{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@down}}	

	\pgfpathcurveto
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/ddd}\pgf@circ@res@left}{\pgf@circ@res@down}}
		{\pgfpoint{\pgf@circ@res@other}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/ccc}\pgf@circ@res@down}}
		{\pgfpoint{\pgf@circ@res@other}{0pt}}
	\pgfpathcurveto
		{\pgfpoint{\pgf@circ@res@other}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/ccc}\pgf@circ@res@up}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/ddd}\pgf@circ@res@left}{\pgf@circ@res@up}}
		{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@up}}	
	\pgfusepath{draw}
}


\pgfcircdeclarelogicport{xor}{

	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/input height}\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint
		{(\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/port width}-\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/input skip})*\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/input height}\pgf@circ@res@up}}
	
	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/input height}\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint
		{(\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/port width}-\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/input skip})*\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/input height}\pgf@circ@res@down}}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/port width}\pgf@circ@res@right}
		{0pt}}	
	
	\pgfusepath{draw}
	\pgf@circ@res@other=\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/port width}\pgf@circ@res@right
	\pgfsetlinewidth{2\pgflinewidth}
	\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@up}}
	\pgfpathcurveto
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/aaa}\pgf@circ@res@left}{\pgf@circ@res@up}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/bbb}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/ccc}\pgf@circ@res@up}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/bbb}\pgf@circ@res@left}{0pt}}
	\pgfpathcurveto
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/bbb}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/ccc}\pgf@circ@res@down}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/aaa}\pgf@circ@res@left}{\pgf@circ@res@down}}
		{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@down}}	

	\pgfpathcurveto
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/ddd}\pgf@circ@res@left}{\pgf@circ@res@down}}
		{\pgfpoint{\pgf@circ@res@other}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/ccc}\pgf@circ@res@down}}
		{\pgfpoint{\pgf@circ@res@other}{0pt}}
	\pgfpathcurveto
		{\pgfpoint{\pgf@circ@res@other}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/ccc}\pgf@circ@res@up}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/ddd}\pgf@circ@res@left}{\pgf@circ@res@up}}
		{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@up}}	
		
	\def\pgf@circ@temp{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/distance}\pgf@circ@res@right+}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@temp-\pgf@circ@res@other}{\pgf@circ@res@up}}
	
	\pgfpathcurveto
		{\pgfpoint{\pgf@circ@temp\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/aaa}\pgf@circ@res@left}{.95*\pgf@circ@res@up}}
		{\pgfpoint{\pgf@circ@temp\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/bbb}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/ccc}\pgf@circ@res@up}}
		{\pgfpoint{\pgf@circ@temp\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/bbb}\pgf@circ@res@left}{0pt}}
	\pgfpathcurveto
		{\pgfpoint{\pgf@circ@temp\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/bbb}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/ccc}\pgf@circ@res@down}}
		{\pgfpoint{\pgf@circ@temp\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/aaa}\pgf@circ@res@left}{.95*\pgf@circ@res@down}}
		{\pgfpoint{\pgf@circ@temp-\pgf@circ@res@other}{.95*\pgf@circ@res@down}}	
				
	\pgfusepath{draw}
}



\pgfcircdeclarelogicport{xnor}{

	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/input height}\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint
		{(\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/port width}-\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/input skip})*\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/input height}\pgf@circ@res@up}}
	
	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/input height}\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint
		{(\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/port width}-\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/input skip})*\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/input height}\pgf@circ@res@down}}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/port width}\pgf@circ@res@right}
		{0pt}}	
	
	\pgfusepath{draw}
	\pgf@circ@res@other=\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/port width}\pgf@circ@res@right
	\pgf@circ@res@step = \pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/circle width}\pgf@circ@res@right

	\pgfsetlinewidth{2\pgflinewidth}
	\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@up}}
	\pgfpathcurveto
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/aaa}\pgf@circ@res@left}{\pgf@circ@res@up}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/bbb}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/ccc}\pgf@circ@res@up}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/bbb}\pgf@circ@res@left}{0pt}}
	\pgfpathcurveto
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/bbb}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/ccc}\pgf@circ@res@down}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/aaa}\pgf@circ@res@left}{\pgf@circ@res@down}}
		{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@down}}	

	\pgfpathcurveto
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/ddd}\pgf@circ@res@left}{\pgf@circ@res@down}}
		{\pgfpoint{\pgf@circ@res@other-\pgf@circ@res@step}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/ccc}\pgf@circ@res@down}}
		{\pgfpoint{\pgf@circ@res@other-\pgf@circ@res@step}{0pt}}
	\pgfpathcurveto
		{\pgfpoint{\pgf@circ@res@other-\pgf@circ@res@step}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/ccc}\pgf@circ@res@up}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/ddd}\pgf@circ@res@left}{\pgf@circ@res@up}}
		{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@up}}	
		
	\def\pgf@circ@temp{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/distance}\pgf@circ@res@right+}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@temp-\pgf@circ@res@other}{\pgf@circ@res@up}}
	
	\pgfpathcurveto
		{\pgfpoint{\pgf@circ@temp\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/aaa}\pgf@circ@res@left}{.95*\pgf@circ@res@up}}
		{\pgfpoint{\pgf@circ@temp\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/bbb}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/ccc}\pgf@circ@res@up}}
		{\pgfpoint{\pgf@circ@temp\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/bbb}\pgf@circ@res@left}{0pt}}
	\pgfpathcurveto
		{\pgfpoint{\pgf@circ@temp\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/bbb}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/ccc}\pgf@circ@res@down}}
		{\pgfpoint{\pgf@circ@temp\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/aaa}\pgf@circ@res@left}{.95*\pgf@circ@res@down}}
		{\pgfpoint{\pgf@circ@temp-\pgf@circ@res@other}{.95*\pgf@circ@res@down}}	
		
		
	\pgfpathellipse
		{\pgfpoint{\pgf@circ@res@other-.5\pgf@circ@res@step}{0pt}}
		{\pgfpoint{.5\pgf@circ@res@step}{0pt}}
		{\pgfpoint{0pt}{.5\pgf@circ@res@step}}
				
	\pgfusepath{draw}
}


\pgfdeclareshape{american not port}
	{
	  \anchor{center}{\pgfpointorigin}
	  \savedanchor\northwest{%
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/bipoles/not port/height}\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/bipoles/not port/width}\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
	  }
	  \savedanchor\left{%
	  	\pgf@y=0pt
	  }
	  \anchor{in}{
		\northwest
		\pgf@y=0pt
	  }
	  \anchor{out}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	  }
	  \anchor{center}{
	  	\pgfpointorigin
	  }
	  \anchor{east}{
	  	\left
	  	\pgf@x=-.8\pgf@x  
	  }
	  \anchor{west}{
	  	\left
	  }
	  \anchor{south}{
		\northwest
		\pgf@x=0pt
		\pgf@y=-\pgf@y
	  }
	  \anchor{north}{
		\northwest
		\pgf@x=0pt
	  }
	  	  \anchor{south west}{
		\northwest
		\pgf@y=-\pgf@y
	  }
	  \anchor{north east}{
		\northwest
		\pgf@x=-\pgf@x
	  }
	  \anchor{north west}{
		\northwest
	  }
	  \anchor{south east}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@y=-\pgf@y
	  }	  
	  \backgroundpath{			
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			
			
			\northwest
			\pgf@circ@res@up = \pgf@y 
			\pgf@circ@res@down = -\pgf@y
			\pgf@circ@res@right = -\pgf@x
			\pgf@circ@res@left = \pgf@x
			
		\pgf@circ@res@other = \pgfkeysvalueof{/tikz/circuitikz/bipoles/not port/circle width}\pgf@circ@res@right
						
	\pgfscope
		\pgfsetlinewidth{2\pgflinewidth}
		\pgftransformxshift{.7\pgf@circ@res@left}
		\pgf@circ@res@step=\pgf@circ@res@right
		\advance\pgf@circ@res@step by -\pgf@circ@res@left
		\pgf@circ@res@step=.7\pgf@circ@res@step
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step-\pgf@circ@res@other}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@step-\pgf@circ@res@other}{0pt}}
		\pgfusepath{draw}
		\pgfpathellipse
			{\pgfpoint{\pgf@circ@res@step-.5\pgf@circ@res@other}{0pt}}
			{\pgfpoint{.5\pgf@circ@res@other}{0pt}}
			{\pgfpoint{0pt}{.5\pgf@circ@res@other}}
		\pgfusepath{draw}
	\endpgfscope
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{.7\pgf@circ@res@left}{0pt}}
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
		\pgfpathlineto{\pgfpoint{.7\pgf@circ@res@right}{0pt}}
	
		\pgfusepath{draw}
	  
	  }
	}

\pgfdeclareshape{invschmitt}
	{
	  \anchor{center}{\pgfpointorigin}
	  \savedanchor\northwest{%
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/bipoles/not port/height}\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/bipoles/not port/width}\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
	  }
	  \savedanchor\left{%
	  	\pgf@y=0pt
	  }
	  \anchor{in}{
		\northwest
		\pgf@y=0pt
	  }
	  \anchor{out}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	  }
	  \anchor{center}{
	  	\pgfpointorigin
	  }
	  \anchor{east}{
	  	\left
	  	\pgf@x=-.8\pgf@x  
	  }
	  \anchor{west}{
	  	\left
	  }
	  \anchor{south}{
		\northwest
		\pgf@x=0pt
		\pgf@y=-\pgf@y
	  }
	  \anchor{north}{
		\northwest
		\pgf@x=0pt
	  }
	  	  \anchor{south west}{
		\northwest
		\pgf@y=-\pgf@y
	  }
	  \anchor{north east}{
		\northwest
		\pgf@x=-\pgf@x
	  }
	  \anchor{north west}{
		\northwest
	  }
	  \anchor{south east}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@y=-\pgf@y
	  }	  
	  \backgroundpath{			
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			
			
			\northwest
			\pgf@circ@res@up = \pgf@y 
			\pgf@circ@res@down = -\pgf@y
			\pgf@circ@res@right = -\pgf@x
			\pgf@circ@res@left = \pgf@x
			
		\pgf@circ@res@other = \pgfkeysvalueof{/tikz/circuitikz/bipoles/not port/circle width}\pgf@circ@res@right
						
	\pgfscope
		\pgfsetlinewidth{2\pgflinewidth}
		\pgftransformxshift{.7\pgf@circ@res@left}
		\pgf@circ@res@step=\pgf@circ@res@right
		\advance\pgf@circ@res@step by -\pgf@circ@res@left
		\pgf@circ@res@step=.7\pgf@circ@res@step
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step-\pgf@circ@res@other}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathclose
		\pgfusepath{draw}
		\pgfpathellipse
			{\pgfpoint{\pgf@circ@res@step-.5\pgf@circ@res@other}{0pt}}
			{\pgfpoint{.5\pgf@circ@res@other}{0pt}}
			{\pgfpoint{0pt}{.5\pgf@circ@res@other}}
				\pgfsetfillcolor{white}
		\pgfusepath{draw,fill}
	\endpgfscope
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{.7\pgf@circ@res@left}{0pt}}
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
		\pgfpathlineto{\pgfpoint{.7\pgf@circ@res@right}{0pt}}
				\pgfusepath{draw}
		%draw inner shape
		
		\pgfsetlinewidth{2\pgflinewidth}
		
		\pgfpathmoveto{\pgfpoint{.6\pgf@circ@res@left}{.3\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{.4\pgf@circ@res@left}{.3\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{.4\pgf@circ@res@left}{.3\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{.05\pgf@circ@res@left}{.3\pgf@circ@res@up}}
		\pgfpathmoveto{\pgfpoint{.4\pgf@circ@res@left}{.3\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{.25\pgf@circ@res@left}{.3\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{.25\pgf@circ@res@left}{.3\pgf@circ@res@up}}
		\pgfusepath{draw}
	  
	  }
	}

\pgfdeclareshape{schmitt}
	{
	  \anchor{center}{\pgfpointorigin}
	  \savedanchor\northwest{%
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/bipoles/not port/height}\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/bipoles/not port/width}\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
	  }
	  \savedanchor\left{%
	  	\pgf@y=0pt
	  }
	  \anchor{in}{
		\northwest
		\pgf@y=0pt
	  }
	  \anchor{out}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	  }
	  \anchor{center}{
	  	\pgfpointorigin
	  }
	  \anchor{east}{
	  	\left
	  	\pgf@x=-.8\pgf@x  
	  }
	  \anchor{west}{
	  	\left
	  }
	  \anchor{south}{
		\northwest
		\pgf@x=0pt
		\pgf@y=-\pgf@y
	  }
	  \anchor{north}{
		\northwest
		\pgf@x=0pt
	  }
	  	  \anchor{south west}{
		\northwest
		\pgf@y=-\pgf@y
	  }
	  \anchor{north east}{
		\northwest
		\pgf@x=-\pgf@x
	  }
	  \anchor{north west}{
		\northwest
	  }
	  \anchor{south east}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@y=-\pgf@y
	  }	  
	  \backgroundpath{			
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			
			
			\northwest
			\pgf@circ@res@up = \pgf@y 
			\pgf@circ@res@down = -\pgf@y
			\pgf@circ@res@right = -\pgf@x
			\pgf@circ@res@left = \pgf@x
			
		\pgf@circ@res@other = \pgfkeysvalueof{/tikz/circuitikz/bipoles/not port/circle width}\pgf@circ@res@right
						
	\pgfscope
		\pgfsetlinewidth{2\pgflinewidth}
		\pgftransformxshift{.7\pgf@circ@res@left}
		\pgf@circ@res@step=\pgf@circ@res@right
		\advance\pgf@circ@res@step by -\pgf@circ@res@left
		\pgf@circ@res@step=.7\pgf@circ@res@step
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step-\pgf@circ@res@other}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathclose
		\pgfusepath{draw}
	\endpgfscope
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{.7\pgf@circ@res@left}{0pt}}
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
		\pgfpathlineto{\pgfpoint{.7\pgf@circ@res@right-\pgf@circ@res@other}{0pt}}
				\pgfusepath{draw}
		%draw inner shape
		
		\pgfsetlinewidth{2\pgflinewidth}
		
		\pgfpathmoveto{\pgfpoint{.6\pgf@circ@res@left}{.3\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{.4\pgf@circ@res@left}{.3\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{.4\pgf@circ@res@left}{.3\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{.05\pgf@circ@res@left}{.3\pgf@circ@res@up}}
		\pgfpathmoveto{\pgfpoint{.4\pgf@circ@res@left}{.3\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{.25\pgf@circ@res@left}{.3\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{.25\pgf@circ@res@left}{.3\pgf@circ@res@up}}
		\pgfusepath{draw}
	  
	  }
	}



%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%

% #1 - name
% #2 - text inside
% #3 - number of inputs
% #4 - is it a not

\long\def\pgfcircdeclareeurologicport#1#2#3#4{
	\pgfdeclareshape{european #1 port}
	{
	  \savedanchor\northwest{%
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/height}\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/width}\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
	  }
	  \savedanchor\left{%
	  	\pgf@y=0pt
	  }
	  \savedanchor\inOne{%
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/height}\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/input height}\pgf@y
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/width}\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
	  }	  
	  \anchor{in}{
		\inOne
	  }
	  \anchor{in 1}{
		\inOne
	  }
	  \anchor{in 2}{
		\inOne
		\pgf@y=-\pgf@y
	  }
	  \anchor{out}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	  }
  	  \anchor{center}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-.8\pgf@x  
	  }
	  \anchor{east}{
	  	\left
	  	\pgf@x=-.8\pgf@x  
	  }
	  \anchor{west}{
	  	\left
	  }
	  \anchor{south}{
		\northwest
		\pgf@x=0pt
		\pgf@y=-\pgf@y
	  }
	  \anchor{north}{
		\northwest
		\pgf@x=0pt
	  }
	  \anchor{south west}{
		\northwest
		\pgf@y=-\pgf@y
	  }
	  \anchor{north east}{
		\northwest
		\pgf@x=-\pgf@x
	  }
	  \anchor{north west}{
		\northwest
	  }
	  \anchor{south east}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@y=-\pgf@y
	  }	  
	  \backgroundpath{			
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			\northwest
			\pgf@circ@res@up = \pgf@y 
			\pgf@circ@res@down = -\pgf@y
			\pgf@circ@res@right = -\pgf@x
			\pgf@circ@res@left = \pgf@x
			\def\pgf@temp{1}
			\def\pgf@circ@temp{#3}
			\ifx\pgftemp\pgf@circ@temp % one input
				\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfpathlineto{
					\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/reserved}\pgf@circ@res@left}{0pt}}
			\else % two inputs
				\pgfpathmoveto{
					\pgfpoint{\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/input height}\pgf@circ@res@up}}
				\pgfpathlineto{
					\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/reserved}\pgf@circ@res@left}
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/input height}\pgf@circ@res@up}}
					%
				\pgfpathmoveto{
					\pgfpoint{\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/input height}\pgf@circ@res@down}}
				\pgfpathlineto{
					\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/reserved}\pgf@circ@res@left}
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/input height}\pgf@circ@res@down}}
			\fi%
			%
			%
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
			\pgfpathlineto{
				\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/reserved}\pgf@circ@res@right}{0pt}}
			%
			\edef\pgf@temp{not}
			\edef\pgf@circ@temp{#4}
			\ifx\pgf@temp\pgf@circ@temp % is a not
				\pgfpathmoveto{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/not width}\pgf@circ@res@right}{0pt}}
				\pgfpathlineto{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/reserved}\pgf@circ@res@right}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/not height}\pgf@circ@res@up}}
			\fi
			%
			\pgfusepath{draw}
			%
			\pgfpathmoveto{\pgfpointorigin}
			\pgftext{#2}
			%
			%
			%
			\pgfsetlinewidth{2\pgflinewidth}
			\pgfpathrectanglecorners
				{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/reserved}\pgf@circ@res@left}{\pgf@circ@res@up}}
				{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/reserved}\pgf@circ@res@right}{\pgf@circ@res@down}}
			\pgfusepath{draw}
%
%
	  }
	}
}



\pgfcircdeclareeurologicport{and}{$\&$}{2}{}
\pgfcircdeclareeurologicport{or}{$\ge 1$}{2}{}
\pgfcircdeclareeurologicport{xor}{$=1$}{2}{}
\pgfcircdeclareeurologicport{not}{$1$}{1}{not}
\pgfcircdeclareeurologicport{nand}{$\&$}{2}{not}
\pgfcircdeclareeurologicport{nor}{$\ge 1$}{2}{not}
\pgfcircdeclareeurologicport{xnor}{$=1$}{2}{not}

\long\def\pgfcircdeclaretransistor#1#2#3{
	\pgfdeclareshape{#1}
	{
	\anchor{center}{
		 \pgfpointorigin
	 }
	\savedanchor\northeast{% upper right
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/height}\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@x=0pt
	}
	\savedanchor\left{%center left
	  	\pgf@y=0pt
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/width}\pgf@circ@Rlen
	}
	\anchor{text}{
	 \northeast
	 \pgf@y=.7\pgf@y
	 \pgf@x= \pgf@circ@Rlen
	 \pgf@x=0.1\pgf@x
	}
	\anchor{pathstart}{ % south
		  	\northeast
			\pgf@y=-\pgf@y
	}
	\anchor{pathend}{
		  	\northeast
	}  
	\anchor{north}{
			\northeast
			\pgf@circ@res@step=\pgf@y
			\left
			\pgf@y=\pgf@circ@res@step
			\pgf@x=.5\pgf@x
		}  
	 \anchor{west}{
			\left
	 }
	 \anchor{east}{
		  	\northeast
			\pgf@y=0pt
	 }  
	\anchor{south}{
			\northeast
			\pgf@circ@res@step=\pgf@y
			\left
			\pgf@y=-\pgf@circ@res@step
			\pgf@x=.5\pgf@x
	}
	\anchor{south west}{
			\northeast
			\pgf@circ@res@step=\pgf@y
			\left
			\pgf@y=-\pgf@circ@res@step
	}
	\anchor{north east}{
		\northeast
	}
	\anchor{north west}{
			\northeast
			\pgf@circ@res@step=\pgf@y
			\left
			\pgf@y=\pgf@circ@res@step
	}
	\anchor{south east}{
		\northeast
		\pgf@y=-\pgf@y
	}
	\anchor{B}{
			 \northeast
	         \pgf@circ@res@step=\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/conn height}\pgf@y
	         \left
	         \pgf@y=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/curr direction}\pgf@circ@res@step
	}
	\anchor{base}{
			 \northeast
	         \pgf@circ@res@step=\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/conn height}\pgf@y
	         \left
	         \pgf@y=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/curr direction}\pgf@circ@res@step
	}
		\anchor{G}{
	         \northeast
	         \pgf@circ@res@step=\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/conn height}\pgf@y
	         \left
	         \pgf@y=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/curr direction}\pgf@circ@res@step
		}
		\anchor{gate}{
	         \northeast
	         \pgf@circ@res@step=\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/conn height}\pgf@y
	         \left
	         \pgf@y=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/curr direction}\pgf@circ@res@step
		}	
	 \anchor{nobase}{
	 		 	\left
	 		 	\pgf@x=\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@x
	 }
	 	\anchor{nogate}{
	 		\left
	 		\pgf@x=\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/gate width}\pgf@x
	 	}	
	 	\anchor{E}{
	 		\northeast
	 		\pgf@y=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/curr direction}\pgf@y
	 	}
	 	\anchor{emitter}{
	 		\northeast
	 		\pgf@y=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/curr direction}\pgf@y
	 	}
	 	\anchor{C}{
	 		\northeast
	 		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/curr direction}\pgf@y
	 	}
	 	\anchor{collector}{
	 		\northeast
	 		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/curr direction}\pgf@y
	 	}
	 	\anchor{S}{
	 		\northeast
	 		\pgf@y=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/curr direction}\pgf@y
	 	}
	 	\anchor{source}{
	 		\northeast
	 		\pgf@y=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/curr direction}\pgf@y
	 	}
	 	\anchor{D}{
	 		\northeast
	 		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/curr direction}\pgf@y
	 	}
	 	\anchor{drain}{
	 		\northeast
	 		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/curr direction}\pgf@y
	 	}	
	  #2
	  \backgroundpath{
	  	\pgftransformationadjustments		
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			%
			\ifnum \pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/curr direction} > 0
				\pgf@circuit@trans@ntypetrue
			\else
				\pgf@circuit@trans@ntypefalse
			\fi
			\northeast
			\pgf@circ@res@up = \pgf@y 
			\pgf@circ@res@down = -\pgf@y
			\pgf@circ@res@right = \pgf@x
			\left
			\pgf@circ@res@left = \pgf@x
			%
			#3
			% BODY DIODE
			\ifpgf@circuit@fet@bodydiode
			\drawbodydiode{#1}
			\fi
	  %
	  }
	}
}

\long\def\drawbodydiode#1{
        \pgfscope
	         \pgftransformshift{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/bodydiode distance}\pgf@circ@res@left}{\pgf@circ@res@up+\pgf@circ@res@down}}
	        \pgftransformrotate{90}
			\pgftransformscale{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/bodydiode scale}}
			\ifpgf@circuit@fulldiode
				\pgfnode{fulldiodeshape}{center}{}{pgf@bodydiode}{\pgfusepath{fill}}
			\else
				\pgfnode{emptydiodeshape}{center}{}{pgf@bodydiode}{\pgfusepath{fill}}
			\fi
		\endpgfscope
		%Draw upper connection to body diode
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}
						{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/bodydiode conn}\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/bodydiode distance}\pgf@circ@res@left}
						{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/bodydiode conn}\pgf@circ@res@up}}
			 	\pgfpathlineto{\pgfpointanchor{pgf@bodydiode}{east}}
		\pgfusepath{draw}
		\pgfscope
	        \pgftransformshift{\pgfpoint{\pgf@circ@res@right}
        	       {\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/bodydiode conn}\pgf@circ@res@up}}
   	       	\pgftransformscale{0.5}
        \pgfnode{circ}{center}{}{}{\pgfusepath{fill}}
      \endpgfscope{}
   		%Draw lower connection to body diode
	   \pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}
	        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/bodydiode conn}\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/bodydiode distance}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/bodydiode conn}\pgf@circ@res@down}}
			 	\pgfpathlineto{\pgfpointanchor{pgf@bodydiode}{west}}
		\pgfusepath{draw}
		\pgfscope
      \pgftransformshift{\pgfpoint{\pgf@circ@res@right}		        	       {\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/bodydiode conn}\pgf@circ@res@down}}
  	       		\pgftransformscale{0.5}
      \pgfnode{circ}{center}{}{}{\pgfusepath{fill}}
    \endpgfscope
}

\long\def\declarebpt#1{
	\pgfcircdeclaretransistor{#1}{}{
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up+\pgfverticaltransformationadjustment*.5*\pgflinewidth}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base height}\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint
			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@circ@res@left}
			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base height 2}\pgf@circ@res@up}}
		\pgfusepath{draw}
	
		\pgfscope
		\pgfpathmoveto{\pgfpoint
			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@circ@res@left}
			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base height}\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint
			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@circ@res@left}
			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base height}\pgf@circ@res@down}}
		\pgfsetlinewidth{2\pgflinewidth}
		\pgfusepath{draw}
		\endpgfscope
		
		\pgfpathmoveto{\pgfpoint
			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@circ@res@left}
			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base height 2}\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base height}\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down-\pgfverticaltransformationadjustment*.5*\pgflinewidth}}		
		\pgfusepath{draw}
		%draw arrow depending on type of transiytor
	 	\pgfscope
	 	\pgfslopedattimetrue
	 	\pgfallowupsidedownattimetrue
	 	\pgfresetnontranslationattimefalse
		\ifpgf@circuit@trans@ntype
		 	\pgftransformlineattime{.5}{%
		 		\pgfpoint%
		 			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@circ@res@left}%
		 			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base height 2}\pgf@circ@res@down}%
		 	}{%
		 		\pgfpoint{\pgf@circ@res@right}%
		 			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base height}\pgf@circ@res@down}%
		 	}
		\else
		 	\pgftransformlineattime{.5}{%
		 		\pgfpoint{\pgf@circ@res@right}%
		 				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base height}\pgf@circ@res@up}%
		 		}{%
		 		\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@circ@res@left}%
		 				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base height 2}\pgf@circ@res@up}%
		 		}
		\fi
		\pgfnode{currarrow}{center}{}{}{\pgfusepath{stroke}}
		\endpgfscope
	
		\ifpgf@circuit@bpt@drawphoto
					\pgfscope
					\pgfsetarrowsstart{latex'}
					\pgfpathmoveto{\pgfpointadd{\pgfpoint
										{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@circ@res@left}
										{\pgf@circ@res@up+\pgf@circ@res@down}}
										{\pgfpoint{0.05\pgf@circ@res@left}{0.1\pgf@circ@res@up}}}
					\pgfpathlineto{\pgfpointadd{\pgfpoint
										{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@circ@res@left}
										{\pgf@circ@res@up+\pgf@circ@res@down}}
										{\pgfpoint{0.5\pgf@circ@res@left}{0.3\pgf@circ@res@up}}}
					\pgfusepath{draw}
					\pgfpathmoveto{\pgfpointadd{\pgfpoint
										{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@circ@res@left}
										{\pgf@circ@res@up+\pgf@circ@res@down}}
										{\pgfpoint{0.05\pgf@circ@res@left}{-0.1\pgf@circ@res@up}}}
					\pgfpathlineto{\pgfpointadd{\pgfpoint
										{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@circ@res@left}
										{\pgf@circ@res@up+\pgf@circ@res@down}}
										{\pgfpoint{0.5\pgf@circ@res@left}{0.1\pgf@circ@res@up}}}
					\pgfusepath{draw}
					\endpgfscope
		\else
		\ifpgf@circuit@bpt@drawbase
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@circ@res@left}
				{\pgf@circ@res@up+\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@left-\pgfhorizontaltransformationadjustment*.5*\pgflinewidth}{\pgf@circ@res@up+\pgf@circ@res@down}}
			\pgfusepath{draw}
		\fi
		\fi
	}
}

\declarebpt{npn}
\declarebpt{pnp}

\long\def\declareigbt#1{
\pgfcircdeclaretransistor{#1}{}
{
	%draw upper connection
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up+\pgfverticaltransformationadjustment*.5*\pgflinewidth}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/gate height}\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/gate height 2}\pgf@circ@res@up}}
	\pgfusepath{draw}

	%draw thicker gate lines
	\pgfscope
	\pgfpathmoveto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/gate width}\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base height}\pgf@circ@res@up+\pgfverticaltransformationadjustment*.5\pgflinewidth}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/gate width}\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base height}\pgf@circ@res@down-\pgfverticaltransformationadjustment*.5\pgflinewidth}}
	\pgfpathmoveto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base height}\pgf@circ@res@up+\pgfverticaltransformationadjustment*.5\pgflinewidth}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base height}\pgf@circ@res@down-\pgfverticaltransformationadjustment*.5\pgflinewidth}}
	\pgfsetlinewidth{2\pgflinewidth}
	\pgfusepath{draw}
	\endpgfscope
	%draw lower connection		
	\pgfpathmoveto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/gate height 2}\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/gate height}\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down-\pgfverticaltransformationadjustment*.5*\pgflinewidth}}		
	\pgfusepath{draw}
	%draw arrow depending on type of transiytor
 	\pgfscope
 	\pgfslopedattimetrue
 	\pgfallowupsidedownattimetrue
 	\pgfresetnontranslationattimefalse
	\ifpgf@circuit@trans@ntype
	 	\pgftransformlineattime{.5}{%
	 		\pgfpoint%
	 			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@circ@res@left}%
	 			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/gate height 2}\pgf@circ@res@down}%
	 	}{%
	 		\pgfpoint{\pgf@circ@res@right}%
	 			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/gate height}\pgf@circ@res@down}%
	 	}
	\else
	 	\pgftransformlineattime{.5}{%
	 		\pgfpoint{\pgf@circ@res@right}%
	 				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/gate height}\pgf@circ@res@up}%
	 		}{%
	 		\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@circ@res@left}%
	 				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/gate height 2}\pgf@circ@res@up}%
	 		}
	\fi
	\pgfnode{currarrow}{center}{}{}{\pgfusepath{stroke}}
	\endpgfscope
	%draw gate
	\ifpgf@circuit@trans@ntype	
		\pgfpathmoveto{\pgfpoint
			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/gate width}\pgf@circ@res@left}
			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/conn height}\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@left-\pgfhorizontaltransformationadjustment*.5*\pgflinewidth}%
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/conn height}\pgf@circ@res@down}}				
	\else
		\pgfpathmoveto{\pgfpoint
			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/gate width}\pgf@circ@res@left}
			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/conn height}\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@left-\pgfhorizontaltransformationadjustment*.5*\pgflinewidth}%
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/conn height}\pgf@circ@res@up}}			
	\fi
	\pgfusepath{draw}
}
}

\declareigbt{pigbt}
\declareigbt{nigbt}
\declareigbt{Lnigbt}
\declareigbt{Lpigbt}


\pgfcircdeclaretransistor{nmos}{}{%
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up+\pgfverticaltransformationadjustment*.5*\pgflinewidth}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/gate height}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/base width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/gate height}\pgf@circ@res@up}}

			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/base width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/gate height}\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/gate height}\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down-\pgfverticaltransformationadjustment*.5*\pgflinewidth}}
			\pgfusepath{draw}
			
			\pgfscope
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/base width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/base height}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/base width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/base height}\pgf@circ@res@down}}
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/gate height}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/gate height}\pgf@circ@res@down}}
			\pgfsetlinewidth{2\pgflinewidth}
			\pgfusepath{draw}
			\endpgfscope
		\ifpgf@circuit@mos@arrows
			\pgfscope             
			\pgfslopedattimetrue 
			\pgfallowupsidedownattimetrue
			\pgfresetnontranslationattimefalse
			\pgftransformlineattime{.6}{%
				\pgfpoint%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/gate width}\pgf@circ@res@left}%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/gate height}\pgf@circ@res@down}%
			}{%
				\pgfpoint
					{\pgf@circ@res@right}%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/gate height}\pgf@circ@res@down}%
			}
			\pgfnode{currarrow}{center}{}{}{\pgfusepath{stroke}}
			\endpgfscope
		\fi

		\ifpgf@circuit@bpt@drawgate			
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/gate width}\pgf@circ@res@left}
				{\pgf@circ@res@up+\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@left-\pgfhorizontaltransformationadjustment*.5*\pgflinewidth}{\pgf@circ@res@up+\pgf@circ@res@down}}
			\pgfusepath{draw}
		\fi
}


\pgfcircdeclaretransistor{pmos}{}{%
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up+\pgfverticaltransformationadjustment*.5*\pgflinewidth}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/gate height}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/base width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/gate height}\pgf@circ@res@up}}
			\pgfusepath{draw}

		\ifpgf@circuit@mos@arrows
			\pgfscope             
			\pgfslopedattimetrue 
			\pgfallowupsidedownattimetrue
			\pgfresetnontranslationattimefalse
			\pgftransformlineattime{.4}{%
				\pgfpoint%
					{\pgf@circ@res@right}%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/gate height}\pgf@circ@res@up}%
			}{%
				\pgfpoint
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/gate width}\pgf@circ@res@left}%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/gate height}\pgf@circ@res@up}%
			}
			\pgfnode{currarrow}{center}{}{}{\pgfusepath{stroke}}
			\endpgfscope
		\fi

			\pgfscope
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/base width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/base height}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/base width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/base height}\pgf@circ@res@down}}
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/gate height}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/gate height}\pgf@circ@res@down}}
			\pgfsetlinewidth{2\pgflinewidth}
			\pgfusepath{draw}
			\endpgfscope
			
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/base width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/gate height}\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/gate height}\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down-\pgfverticaltransformationadjustment*.5*\pgflinewidth}}		


			\pgfusepath{draw}		
			\ifpgf@circuit@bpt@drawgate
				\pgfpathmoveto{\pgfpoint
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/gate width}\pgf@circ@res@left}
					{\pgf@circ@res@up+\pgf@circ@res@down}}
				\pgfpathlineto{\pgfpoint{\pgf@circ@res@left-\pgfhorizontaltransformationadjustment*.5*\pgflinewidth}{\pgf@circ@res@up+\pgf@circ@res@down}}
				\pgfusepath{draw}
			\fi
			\pgfpathcircle{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/gate width}\pgf@circ@res@left - \pgfkeysvalueof{/tikz/circuitikz/nodes width}*\pgf@circ@Rlen}
				{\pgf@circ@res@up+\pgf@circ@res@down}}{\pgfkeysvalueof{/tikz/circuitikz/nodes width}*\pgf@circ@Rlen}
			\ifpgf@circuit@pmos@emptycircle
				\pgfsetfillcolor{white}
			\fi
			\pgfusepath{draw,fill}		
}

\long\def\drawfetcore#1{
	\pgftransformationadjustments
		%top connection
      \pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up+\pgfverticaltransformationadjustment*.5*\pgflinewidth}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/gate height}\pgf@circ@res@up}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/gate height}\pgf@circ@res@up}}
		\pgfusepath{draw}
		\pgfscope
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base height}\pgf@circ@res@up}}
		\ifpgf@circuit@trans@depletiontype
		      \pgfpathlineto{\pgfpoint
		        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@circ@res@left}
		        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base height}\pgf@circ@res@down}}
		\else

      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base height}\pgf@circ@res@up*0.45}}
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base height}\pgf@circ@res@up*0.25}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base height}\pgf@circ@res@down*0.25}}
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nfet/base height}\pgf@circ@res@down*0.45}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base height}\pgf@circ@res@down}}
        \fi
      \pgfsetlinewidth{2\pgflinewidth}
		\pgfusepath{draw}
		\endpgfscope
		%Bulk connection line
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@circ@res@left}
        {\pgf@circ@res@up+\pgf@circ@res@down}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right+\pgfhorizontaltransformationadjustment*.5*\pgflinewidth}
        {\pgf@circ@res@up+\pgf@circ@res@down}}
      
      %bottom connection
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/gate height}\pgf@circ@res@down}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
       {\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/gate height}\pgf@circ@res@down}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down-\pgfverticaltransformationadjustment*.5*\pgflinewidth}}    
      \pgfusepath{draw}
     
     %draw thick gate line 
    \pgfscope
    \pgfpathmoveto{\pgfpoint
      {\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/gate width}\pgf@circ@res@left}
      {\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/gate height}\pgf@circ@res@up+\pgfverticaltransformationadjustment*.5*\pgflinewidth}}
    \pgfpathlineto{\pgfpoint
      {\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/gate width}\pgf@circ@res@left}
      {\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/gate height}\pgf@circ@res@down-\pgfverticaltransformationadjustment*.5*\pgflinewidth}}
    \pgfsetlinewidth{2\pgflinewidth}
    \pgfusepath{draw}
    \endpgfscope
    
      \pgfscope
          \pgfslopedattimetrue 
          \pgfallowupsidedownattimetrue
          \pgfresetnontranslationattimefalse
          
          \pgftransformlineattime{.6}{%
            \pgfpoint
              {\pgf@circ@res@right}%
              {\pgf@circ@res@up+\pgf@circ@res@down}%
          }{%
            \pgfpoint%
              {\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@circ@res@left}%
              {\pgf@circ@res@up+\pgf@circ@res@down}%
          }
          	  \ifpgf@circuit@trans@ntype
          	  \else
          	  \pgftransformrotate{180}
          	  \fi
          \pgfnode{currarrow}{center}{}{}{\pgfusepath{stroke}}
          \endpgfscope
      
      	% GATE CONNECTION
      	\ifpgf@circuit@bpt@drawgate
			\ifpgf@circuit@trans@ntype
		      	\pgfpathmoveto{\pgfpoint
		      		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/gate width}\pgf@circ@res@left}
		      		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/conn height}\pgf@circ@res@down}}
		      	\pgfpathlineto{\pgfpoint{\pgf@circ@res@left-\pgfhorizontaltransformationadjustment*.5*\pgflinewidth}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/conn height}\pgf@circ@res@down}}
	      	\else
		      	\pgfpathmoveto{\pgfpoint
		      		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/gate width}\pgf@circ@res@left}
		      		{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/conn height}\pgf@circ@res@down}}
		      	\pgfpathlineto{\pgfpoint{\pgf@circ@res@left-\pgfhorizontaltransformationadjustment*.5*\pgflinewidth}{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/conn height}\pgf@circ@res@down}}      	
	      	\fi
      	\pgfusepath{draw}
      	\fi

}

\long\def\pgfdeclaretransistorwrapperaddbulk#1#2#3
{\pgfcircdeclaretransistor{#1}{
	\anchor{bulk}{\left\pgf@x=0pt}
 	\anchor{B}{\left\pgf@x=0pt}%override Base anchor from npn&igbt
	 #2
	 }
	 {#3}
}


\pgfdeclaretransistorwrapperaddbulk{nfet}{}{%
	\pgf@circuit@trans@depletiontypefalse
	\drawfetcore{nfet}
}


\pgfdeclaretransistorwrapperaddbulk{pfet}{}{%
	\pgf@circuit@trans@depletiontypefalse
	\drawfetcore{pfet}
}

% N-CHANNEL IGFET ENHANCEMENT TYPE
\pgfdeclaretransistorwrapperaddbulk{nigfete}{}{%	
	\pgf@circuit@trans@depletiontypefalse
	\drawfetcore{nigfete}
	     
      % SOURCE CONNECTION
      \pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}    
      \pgfusepath{draw}
      
      % SOLDER DOT at source-bulk connection
      \ifpgf@circuit@fet@solderdot
      \pgfscope
        \pgftransformshift{\pgfpoint{\pgf@circ@res@right}{
          \pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/gate height}\pgf@circ@res@down}}
        \pgfnode{circ}{center}{}{}{}
      \endpgfscope{}
      \fi
}




% N-CHANNEL IGFET ENHANCEMENT TYPE with Bulk connector
\pgfdeclaretransistorwrapperaddbulk{nigfetebulk}{}{%
	\pgf@circuit@trans@depletiontypefalse
	\drawfetcore{nigfetebulk}
    % SOLDER DOT at source-bulk connection
      \ifpgf@circuit@fet@solderdot
      \pgfscope
        \pgftransformshift{\pgfpoint{\pgf@circ@res@right}{
          \pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfetebulk/gate height}\pgf@circ@res@down}}
        \pgfnode{circ}{center}{}{}{}
      \endpgfscope{}
      \fi
}



% N-CHANNEL IGFET DEPLETION TYPE
\pgfdeclaretransistorwrapperaddbulk{nigfetd}{}{%
	\pgf@circuit@trans@depletiontypetrue
	\drawfetcore{nigfetd}

      % SOURCE CONNECTION
      \pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}    
      \pgfusepath{draw}
             
      % SOLDER DOT at source-bulk connection
      \ifpgf@circuit@fet@solderdot
      \pgfscope
        \pgftransformshift{\pgfpoint{\pgf@circ@res@right}{
          \pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/gate height}\pgf@circ@res@down}}
        \pgfnode{circ}{center}{}{}{}
      \endpgfscope{}
      \fi
}

% P-CHANNEL IGFET ENHANCEMENT TYPE
\pgfdeclaretransistorwrapperaddbulk{pigfete}{}{%
	\pgf@circuit@trans@depletiontypefalse
	\drawfetcore{pigfete}
      \pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
    
      % SOURCE CONNECTION
      \pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}    
      \pgfusepath{draw}
      
      
      % SOLDER DOT at source-bulk connection
      \ifpgf@circuit@fet@solderdot
      \pgfscope
        \pgftransformshift{\pgfpoint{\pgf@circ@res@right}{
          \pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfete/gate height}\pgf@circ@res@up}}
        \pgfnode{circ}{center}{}{}{}
      \endpgfscope
      \fi
}

% P-CHANNEL IGFET ENHANCEMENT TYPE with bulk connector
\pgfdeclaretransistorwrapperaddbulk{pigfetebulk}{}{%
	\pgf@circuit@trans@depletiontypefalse
	\drawfetcore{pigfetebulk}
}


% P-CHANNEL IGFET DEPLETION TYPE
\pgfdeclaretransistorwrapperaddbulk{pigfetd}{}{%
	\pgf@circuit@trans@depletiontypetrue
	\drawfetcore{pigfetd}
  
      % SOURCE CONNECTION
      \pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}    
      \pgfusepath{draw}
      
            
      % SOLDER DOT at source-bulk connection
      \ifpgf@circuit@fet@solderdot
      \pgfscope
        \pgftransformshift{\pgfpoint{\pgf@circ@res@right}{
          \pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/gate height}\pgf@circ@res@up}}
        \pgfnode{circ}{center}{}{}{}
      \endpgfscope{}
      \fi
}

\pgfcircdeclaretransistor{njfet}{}{%
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up+\pgfverticaltransformationadjustment*.5*\pgflinewidth}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate height 2}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate height 2}\pgf@circ@res@up}}

			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate height 2}\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate height 2}\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down-\pgfverticaltransformationadjustment*.5*\pgflinewidth}}		
			\pgfusepath{draw}
			
			\pgfscope
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate height}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate height}\pgf@circ@res@down}}
			\pgfsetlinewidth{2\pgflinewidth}
			\pgfusepath{draw}
			\endpgfscope
			
			\pgfscope             
			\pgfslopedattimetrue 
			\pgfallowupsidedownattimetrue
			\pgfresetnontranslationattimefalse
			\pgftransformlineattime{.6}{%
				\pgfpoint{\pgf@circ@res@left}%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate height 2}\pgf@circ@res@down}%
			}{%
				\pgfpoint
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate width}\pgf@circ@res@left}%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate height 2}\pgf@circ@res@down}%
			}
			\pgfnode{currarrow}{center}{}{}{\pgfusepath{stroke}}
			\endpgfscope
	
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate height 2}\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@left-\pgfhorizontaltransformationadjustment*.5*\pgflinewidth}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate height 2}\pgf@circ@res@down}}
			\pgfusepath{draw}
}


\pgfcircdeclaretransistor{pjfet}{}{%
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up+\pgfverticaltransformationadjustment*.5*\pgflinewidth}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate height 2}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate height 2}\pgf@circ@res@up}}

			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate height 2}\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate height 2}\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down-\pgfverticaltransformationadjustment*.5*\pgflinewidth}}		
			\pgfusepath{draw}
			
			\pgfscope
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate height}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate height}\pgf@circ@res@down}}
			\pgfsetlinewidth{2\pgflinewidth}
			\pgfusepath{draw}
			\endpgfscope
			
			\pgfscope             
			\pgfslopedattimetrue 
			\pgfallowupsidedownattimetrue
			\pgfresetnontranslationattimefalse
			\pgftransformlineattime{.4}{%
				\pgfpoint%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate width}\pgf@circ@res@left}%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate height 2}\pgf@circ@res@up}%
			}{%
				\pgfpoint{\pgf@circ@res@left}%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate height 2}\pgf@circ@res@up}%
			}
			\pgfnode{currarrow}{center}{}{}{\pgfusepath{stroke}}
			\endpgfscope

					
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate height 2}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@left-\pgfhorizontaltransformationadjustment*.5*\pgflinewidth}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate height 2}\pgf@circ@res@up}}
			\pgfusepath{draw}
}


\pgfdeclaretransistorwrapperaddbulk{isfet}{}{%
      \pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up+\pgfverticaltransformationadjustment*.5*\pgflinewidth}}
      % DRAIN CONNECTION 
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/gate height}\pgf@circ@res@up}}
      % DRAIN
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/gate height}\pgf@circ@res@up}}
      \pgfusepath{draw}
      
      % GATE, DEPLETION TYPE
      \pgfscope %% added
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/base height}\pgf@circ@res@up}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/base height}\pgf@circ@res@down}}
      \pgfsetlinewidth{2\pgflinewidth} %% added
      \pgfusepath{draw} %% added
      \endpgfscope %% added
      
      % BULK
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/base width}\pgf@circ@res@left}
        {\pgf@circ@res@up+\pgf@circ@res@down}}
       \pgfpathlineto{\pgfpoint{\pgf@circ@res@right+.5\pgflinewidth}
         {\pgf@circ@res@up+\pgf@circ@res@down}}

      % SOURCE
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/gate height}\pgf@circ@res@down}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
         {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/gate height}\pgf@circ@res@down}}
      % SOURCE CONNECTION
      \pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down-\pgfverticaltransformationadjustment*.5*\pgflinewidth}}    
      \pgfusepath{draw}
      
      % GATE
      %\pgfscope
      %\pgfpathmoveto{\pgfpoint
       % {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/gate width}\pgf@circ@res@left}
       % {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/gate height}\pgf@circ@res@up}}
      %\pgfpathlineto{\pgfpoint
       % {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/gate width}\pgf@circ@res@left}
       % {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/gate height}\pgf@circ@res@down}}
      %\pgfsetlinewidth{2\pgflinewidth}
      %\pgfusepath{draw}
      %\endpgfscope
      
            
      % SOLDER DOT at source-bulk connection
      \ifpgf@circuit@fet@solderdot
	      \pgfscope
	        \pgftransformshift{\pgfpoint{\pgf@circ@res@right}{
	          \pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/gate height}\pgf@circ@res@down}}
	        \pgfnode{circ}{center}{}{}{}
	      \endpgfscope{}
      \fi
      % ARROW
      \pgfscope
      \pgfslopedattimetrue 
      \pgfallowupsidedownattimetrue
      \pgfresetnontranslationattimefalse
      \pgftransformlineattime{.6}{%
        \pgfpoint
          {\pgf@circ@res@right}%
          {\pgf@circ@res@up+\pgf@circ@res@down}%
      }{%
        \pgfpoint%
          {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/base width}\pgf@circ@res@left}%
          {\pgf@circ@res@up+\pgf@circ@res@down}%
      }
      \pgfnode{currarrow}{center}{}{}{\pgfusepath{stroke}}
      \endpgfscope
      \pgfusepath{draw}
      
      % Wavy lines
      	\pgfscope
			\pgfpathmoveto{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/waves x sep}\pgf@circ@res@up}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/waves y sep}\pgf@circ@res@up}}
			\pgfpathsine{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave width}\pgf@circ@res@up}{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave amp}\pgf@circ@res@up}}
			\pgfpathcosine{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave width}\pgf@circ@res@up}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave amp}\pgf@circ@res@up}}
			\pgfpathsine{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave width}\pgf@circ@res@up}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave amp}\pgf@circ@res@up}}
			\pgfpathcosine{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave width}\pgf@circ@res@up}{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave amp}\pgf@circ@res@up}}
			\pgfusepath{draw}

			\pgfpathmoveto{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/waves x sep}\pgf@circ@res@up}{0cm}}
			\pgfpathsine{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave width}\pgf@circ@res@up}{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave amp}\pgf@circ@res@up}}
			\pgfpathcosine{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave width}\pgf@circ@res@up}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave amp}\pgf@circ@res@up}}
			\pgfpathsine{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave width}\pgf@circ@res@up}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave amp}\pgf@circ@res@up}}
			\pgfpathcosine{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave width}\pgf@circ@res@up}{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave amp}\pgf@circ@res@up}}
			\pgfusepath{draw}

			\pgfpathmoveto{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/waves x sep}\pgf@circ@res@up}{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/waves y sep}\pgf@circ@res@up}}
			\pgfpathsine{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave width}\pgf@circ@res@up}{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave amp}\pgf@circ@res@up}}
			\pgfpathcosine{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave width}\pgf@circ@res@up}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave amp}\pgf@circ@res@up}}
			\pgfpathsine{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave width}\pgf@circ@res@up}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave amp}\pgf@circ@res@up}}
			\pgfpathcosine{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave width}\pgf@circ@res@up}{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave amp}\pgf@circ@res@up}}
			\pgfusepath{draw}
		\endpgfscope

}


%% Black thyristor

\pgfcircdeclarebipole{
	\anchor{gate}{
		\northeast
	}
	\anchor{anode}{
		\southwest
		\pgf@y=0cm
	}
	\anchor{G}{
		\northeast
	}
	\anchor{cathode}{
		\northeast
		\pgf@y=0cm
	}
}{\ctikzvalof{tripoles/thyristor/height 2}}{fullthyristor}{\ctikzvalof{tripoles/thyristor/height}}{\ctikzvalof{tripoles/thyristor/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

	\pgf@circ@res@other = \ctikzvalof{tripoles/thyristor/diode width left}\pgf@circ@res@left
	\pgf@circ@res@step = \ctikzvalof{tripoles/thyristor/diode width right}\pgf@circ@res@right

	\pgfscope
		\pgftransformxshift{\pgf@circ@res@other}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step-\pgf@circ@res@other}{0pt}}
				
		\pgfpathlineto{\pgfpoint{0pt}{-\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}} 
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@step-\pgf@circ@res@other}{0pt}}
		\pgfusepath{draw,fill}
		
		\pgfsetlinewidth{\pgfstartlinewidth}
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step-\pgf@circ@res@other}{0pt}}
		\pgfpathlineto{\pgfpoint{2*\pgf@circ@res@step-2*\pgf@circ@res@other}{\ctikzvalof{tripoles/thyristor/diode height}\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{2*\pgf@circ@res@step-2*\pgf@circ@res@other}{\pgf@circ@res@up}}
		\pgfusepath{draw}
	\endpgfscope
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{-\pgf@circ@res@down}}
	
	\pgfusepath{draw}
	
	\pgfsetlinewidth{\pgfstartlinewidth}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@other}{0pt}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{0pt}}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{0pt}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0pt}}
	
	\pgfusepath{draw}
	
}

%% Empty thyristor

\pgfcircdeclarebipole{
	\anchor{gate}{
		\northeast
	}
	\anchor{anode}{
		\southwest
		\pgf@y=0cm
	}
	\anchor{G}{
		\northeast
	}
	\anchor{cathode}{
		\northeast
		\pgf@y=0cm
	}
}{\ctikzvalof{tripoles/thyristor/height 2}}{emptythyristor}{\ctikzvalof{tripoles/thyristor/height}}{\ctikzvalof{tripoles/thyristor/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

	\pgf@circ@res@other = \ctikzvalof{tripoles/thyristor/diode width left}\pgf@circ@res@left
	\pgf@circ@res@step = \ctikzvalof{tripoles/thyristor/diode width right}\pgf@circ@res@right

	\pgfscope
		\pgftransformxshift{\pgf@circ@res@other}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step-\pgf@circ@res@other}{0pt}}
				
		\pgfpathlineto{\pgfpoint{0pt}{-\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}} 
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@step-\pgf@circ@res@other}{0pt}}
		\pgfusepath{draw}
		
		\pgfsetlinewidth{\pgfstartlinewidth}
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step-\pgf@circ@res@other}{0pt}}
		\pgfpathlineto{\pgfpoint{2*\pgf@circ@res@step-2*\pgf@circ@res@other}{\ctikzvalof{tripoles/thyristor/diode height}\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{2*\pgf@circ@res@step-2*\pgf@circ@res@other}{\pgf@circ@res@up}}
		\pgfusepath{draw}
	\endpgfscope
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{-\pgf@circ@res@down}}
	
	\pgfusepath{draw}
	
	\pgfsetlinewidth{\pgfstartlinewidth}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@other}{0pt}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{0pt}}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{0pt}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0pt}}
	
	\pgfusepath{draw}
	
}

%% Empty triac

\pgfcircdeclarebipole{
	\anchor{gate}{
		\northeast
	}
	\anchor{G}{
		\northeast
	}
	\anchor{anode}{
		\southwest
		\pgf@y=0cm
	}
	\anchor{cathode}{
		\northeast
		\pgf@y=0cm
	}
}{\ctikzvalof{tripoles/triac/height}}{emptytriac}{\ctikzvalof{tripoles/triac/height}}{\ctikzvalof{tripoles/triac/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

	\pgf@circ@res@other = \ctikzvalof{tripoles/triac/diode width left}\pgf@circ@res@left
	\pgf@circ@res@step = \ctikzvalof{tripoles/triac/diode width right}\pgf@circ@res@right

	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@other}{0pt}}
	\pgfpathlineto{\pgfpoint{0.95\pgf@circ@res@step}{0.707*(\pgf@circ@res@other-\pgf@circ@res@step)}} % sqrt(1/2)
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{1.414*(\pgf@circ@res@other-\pgf@circ@res@step)}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{-1.414*(\pgf@circ@res@other-\pgf@circ@res@step)}}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{0pt}}
	\pgfpathlineto{\pgfpoint{0.95\pgf@circ@res@other}{-0.707*(\pgf@circ@res@other-\pgf@circ@res@step)}} % sqrt(1/2)
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{-1.414*(\pgf@circ@res@other-\pgf@circ@res@step)}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{1.414*(\pgf@circ@res@other-\pgf@circ@res@step)}}
	
	\pgfusepath{draw}
	
	\pgfsetlinewidth{\pgfstartlinewidth}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{-0.707*(\pgf@circ@res@other-\pgf@circ@res@step)}} % sqrt(1/2)
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{-1.414*(\pgf@circ@res@other-\pgf@circ@res@step)}} % sqrt(1/2)
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}} % sqrt(1/2)
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@other}{0pt}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{0pt}}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{0pt}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0pt}}
	
	\pgfusepath{draw}
	
}

%% Empty triac

\pgfcircdeclarebipole{
	\anchor{gate}{
		\northeast
	}
	\anchor{G}{
		\northeast
	}
	\anchor{anode}{
		\southwest
		\pgf@y=0cm
	}
	\anchor{cathode}{
		\northeast
		\pgf@y=0cm
	}
}{\ctikzvalof{tripoles/triac/height}}{fulltriac}{\ctikzvalof{tripoles/triac/height}}{\ctikzvalof{tripoles/triac/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

	\pgf@circ@res@other = \ctikzvalof{tripoles/triac/diode width left}\pgf@circ@res@left
	\pgf@circ@res@step = \ctikzvalof{tripoles/triac/diode width right}\pgf@circ@res@right

	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@other}{0pt}}
	\pgfpathlineto{\pgfpoint{0.95\pgf@circ@res@step}{0.707*(\pgf@circ@res@other-\pgf@circ@res@step)}} % sqrt(1/2)
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{1.414*(\pgf@circ@res@other-\pgf@circ@res@step)}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{-1.414*(\pgf@circ@res@other-\pgf@circ@res@step)}}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{0pt}}
	\pgfpathlineto{\pgfpoint{0.95\pgf@circ@res@other}{-0.707*(\pgf@circ@res@other-\pgf@circ@res@step)}} % sqrt(1/2)
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{-1.414*(\pgf@circ@res@other-\pgf@circ@res@step)}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{1.414*(\pgf@circ@res@other-\pgf@circ@res@step)}}
	
	\pgfusepath{draw,fill}
	
	\pgfsetlinewidth{\pgfstartlinewidth}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{-0.707*(\pgf@circ@res@other-\pgf@circ@res@step)}} % sqrt(1/2)
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{-1.414*(\pgf@circ@res@other-\pgf@circ@res@step)}} % sqrt(1/2)
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}} % sqrt(1/2)
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@other}{0pt}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{0pt}}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{0pt}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0pt}}
	
	\pgfusepath{draw}
	
}







\pgfcircdeclarebipole{
	\anchor{out 1}{
		\northeast
		\pgf@y=0cm
	}
	\anchor{out 2}{
		\northeast
		\pgf@y=.8\pgf@y
	}
}{\ctikzvalof{tripoles/toggleswitch/height 2}}{toggleswitch}{\ctikzvalof{tripoles/toggleswitch/height}}{\ctikzvalof{tripoles/toggleswitch/width}}{

	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0pt}}
	\pgfpathlineto{\pgfpoint{.3\pgf@circ@res@left}{0pt}}
	\pgfusepath{draw}
	\pgfscope
	\pgfpathmoveto{\pgfpoint{.3\pgf@circ@res@left}{0pt}}
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathlineto{\pgfpoint{.7\pgf@circ@res@right}{.5\pgf@circ@res@up}}
	\pgfusepath{draw}
	\endpgfscope
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
	\pgfpathlineto{\pgfpoint{.5\pgf@circ@res@right}{0}}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{.8\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{.5\pgf@circ@res@right}{.8\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{.5\pgf@circ@res@right}{.15\pgf@circ@res@up}}
	\pgfusepath{draw}
	
	
	\pgfpathmoveto{\pgfpoint{.2\pgf@circ@res@left}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{.2\pgf@circ@res@right}{\pgf@circ@res@up}}
	\pgfusepath{draw}
	
	\pgfsetdash{{.08\pgf@circ@res@up}{.04\pgf@circ@res@up}{.7\pgf@circ@res@up}{.04\pgf@circ@res@up}{.8\pgf@circ@res@up}}{0cm}
	\pgfpathmoveto{\pgfpoint{0}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{0}{.8\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{.2\pgf@circ@res@left}{.6\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{0}{.4\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{0}{.2\pgf@circ@res@up}}
	\pgfusepath{draw}
	\pgfsetdash{}{0cm}
}










\pgfdeclareshape{op amp}
	{
	  \anchor{center}{\pgfpointorigin}
	  \savedanchor\northwest{%
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/height}\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/width}\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
	  }
	  \anchor{south}{
		\northwest
		\pgf@y=-\pgf@y
		\pgf@x=0pt
	  }
	  \anchor{north}{
		\northwest
		\pgf@x=0pt
	  }
	  \savedanchor\left{%
	  	\pgf@y=0pt
	  }
	  \anchor{leftedge}
	  {\left
		  \pgf@x = \pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}\pgf@x
	  }
	  \savedanchor\inOne{%
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/height}\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@y
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/width}\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
	  }	  
	  \anchor{-}{
		\inOne
	  }
	  \anchor{+}{
		\inOne
		\pgf@y=-\pgf@y
	  }
	  \savedanchor\up{%
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/height}\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/width}\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
			\pgf@circ@res@up = \pgf@y 
			\pgf@circ@res@right = -\pgf@x
			\pgf@circ@res@left = \pgf@x
	    \pgfpointlineattime{
			\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/up pos}}{
			\pgfpoint{
				\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}\pgf@circ@res@left}
				{\pgf@circ@res@up}}
			{\pgfpoint{.7\pgf@circ@res@right}{0pt}}
	  }
	  \anchor{up}{
		\up
	  }
	  \anchor{down}{
		\up
		\pgf@y=-\pgf@y
	  }
	  \anchor{out}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	  }
	  	\anchor{west}{
		  	\left
    	  }
		  \anchor{east}{
		  	\left
		  	\pgf@x=-\pgf@x
		  }  
	  
	  \backgroundpath{			
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			
			
			\northwest
			\pgf@circ@res@up = \pgf@y 
			\pgf@circ@res@down = -\pgf@y
			\pgf@circ@res@right = -\pgf@x
			\pgf@circ@res@left = \pgf@x
			
	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@up}}
	\pgftext[left, at=\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@up}]{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/font} $-$}
	

	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@down}}
	\pgftext[left, at=\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@down}]{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/font} $+$}
		
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
	\pgfpathlineto{\pgfpoint{.7\pgf@circ@res@right}{0pt}}
	\pgfsetrectcap
	\pgfusepath{draw}

						
	\pgfscope
		\pgfsetlinewidth{2\pgflinewidth}
		\pgftransformxshift{.7\pgf@circ@res@left}
		\pgf@circ@res@step=\pgf@circ@res@right
		\advance\pgf@circ@res@step by -\pgf@circ@res@left
		\pgf@circ@res@step=.7\pgf@circ@res@step
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathclose
		\pgfusepath{draw}
	\endpgfscope
		
		
	  
	  }
	}

%op amp shape as in european standard en 60617
\pgfdeclareshape{en amp}
{
	\anchor{center}{\pgfpointorigin}
	\savedanchor\northwest{%
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/en amp/height}\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/en amp/width}\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
	}
	\anchor{south}{
		\northwest
		\pgf@y=-\pgf@y
		\pgf@x=0pt
	}
	\anchor{north}{
		\northwest
		\pgf@x=0pt
	}
	\savedanchor\left{%
	  	\pgf@y=0pt
	}
	\anchor{leftedge}
	{
		\left
	 	\pgf@x = \pgfkeysvalueof{/tikz/circuitikz/tripoles/en amp/port width}\pgf@x
	}
	\savedanchor\inOne{%
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/en amp/height}\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/en amp/input height}\pgf@y
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/en amp/width}\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
	}	  
	\anchor{-}{
		\inOne
	}
	\anchor{+}{
		\inOne
		\pgf@y=-\pgf@y
	}
	\anchor{up}{
		\northwest
		\pgf@x=0pt
	}
	\anchor{down}{
		\northwest
		\pgf@x=0pt
		\pgf@y=-\pgf@y
	}
	\anchor{out}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	}
	\anchor{west}{
		\left
	}
	\anchor{east}{
	  	\left
		\pgf@x=-\pgf@x
	}
	\backgroundpath{			
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			\northwest
			\pgf@circ@res@up = \pgf@y 
			\pgf@circ@res@down = -\pgf@y
			\pgf@circ@res@right = -\pgf@x
			\pgf@circ@res@left = \pgf@x
			
	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/en amp/input height}\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/en amp/port width}\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/en amp/input height}\pgf@circ@res@up}}
	\pgftext[left, at=\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/en amp/port width}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/en amp/input height}\pgf@circ@res@up}]{\pgfkeysvalueof{/tikz/circuitikz/tripoles/en amp/font} $-$}
	
	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/en amp/input height}\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/en amp/port width}\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/en amp/input height}\pgf@circ@res@down}}
	\pgftext[left, at=\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/en amp/port width}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/en amp/input height}\pgf@circ@res@down}]{\pgfkeysvalueof{/tikz/circuitikz/tripoles/en amp/font} $+$}
		
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
	\pgfpathlineto{\pgfpoint{.7\pgf@circ@res@right}{0pt}}
	\pgfsetrectcap
	\pgfusepath{draw}
				
	\pgfscope
		\pgfsetlinewidth{2\pgflinewidth}
		\pgfpathmoveto{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nand port/port width}\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nand port/port width}\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nand port/port width}\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nand port/port width}\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfpathclose
		\pgfusepath{draw}
	\endpgfscope

	\pgftext[base,y=-3ex,at=\pgfpoint{.3\pgf@circ@res@left}{\pgf@circ@res@up}]{\pgfkeysvalueof{/tikz/circuitikz/tripoles/en amp/font2} $\triangleright$}
	\pgftext[base,y=-3ex,at=\pgfpoint{.3\pgf@circ@res@right}{\pgf@circ@res@up}]{\pgfkeysvalueof{/tikz/circuitikz/tripoles/en amp/font2} $\infty$}
	  }
}

%%Transkonduktanzverstärker
\pgfdeclareshape{gm amp}
	{
	  \anchor{center}{\pgfpointorigin}
	  \savedanchor\northwest{%
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/gm amp/height}\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/gm amp/width}\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
	  }
	  \anchor{south}{
		\northwest
		\pgf@y=-\pgf@y
	  }
	  \anchor{north}{
		\northwest
	  }
	  \savedanchor\left{%
	  	\pgf@y=0pt
	  }
	  \anchor{leftedge}
	  {\left
  	  	\pgf@x = \pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}\pgf@x
	  }
	  \savedanchor\inOne{%
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/gm amp/height}\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/gm amp/input height}\pgf@y
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/gm amp/width}\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
	  }	  
	  \anchor{-}{
		\inOne
	  }
	  \anchor{+}{
		\inOne
		\pgf@y=-\pgf@y
	  }
	  \savedanchor\up{%
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/gm amp/height}\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/gm amp/width}\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
			\pgf@circ@res@up = \pgf@y 
			\pgf@circ@res@right = -\pgf@x
			\pgf@circ@res@left = \pgf@x
	    \pgfpointlineattime{
			\pgfkeysvalueof{/tikz/circuitikz/tripoles/gm amp/up pos}}{
			\pgfpoint{
				\pgfkeysvalueof{/tikz/circuitikz/tripoles/gm amp/port width}\pgf@circ@res@left}
				{\pgf@circ@res@up}}
			{\pgfpoint{.7\pgf@circ@res@right}{0pt}}
	  }
	  \anchor{up}{
		\up
	  }
	  \anchor{down}{
		\up
		\pgf@y=-\pgf@y
	  }
	  \anchor{out}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	  }
	  	\anchor{west}{
		  	\left
    	  }
		  \anchor{east}{
		  	\left
		  	\pgf@x=-\pgf@x
		  }  
	  
	  \backgroundpath{			
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
						
			\northwest
			\pgf@circ@res@up = \pgf@y 
			\pgf@circ@res@down = -\pgf@y
			\pgf@circ@res@right = -\pgf@x
			\pgf@circ@res@left = \pgf@x
			
	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/gm amp/input height}\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/gm amp/port width}\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/gm amp/input height}\pgf@circ@res@up}}
	\pgftext[left, at=\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/gm amp/port width}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/gm amp/input height}\pgf@circ@res@up}]{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/font} $-$}
	

	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/gm amp/input height}\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/gm amp/port width}\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/gm amp/input height}\pgf@circ@res@down}}
	\pgftext[left, at=\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/gm amp/port width}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/gm amp/input height}\pgf@circ@res@down}]{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/font} $+$}
		
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
	\pgfpathlineto{\pgfpoint{.3\pgf@circ@res@right}{0pt}} %
		\pgfsetrectcap
	\pgfusepath{draw}

	\pgfscope
		\pgfsetlinewidth{2\pgflinewidth}
		\pgftransformxshift{.7\pgf@circ@res@left}
		\pgf@circ@res@step=\pgf@circ@res@right
		\advance\pgf@circ@res@step by -\pgf@circ@res@left
		\pgf@circ@res@step=.7\pgf@circ@res@step
		%Umrandung:
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0}} %geändert startpunkt neu am ausgangsstrich
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{.5\pgf@circ@res@up}}%vom Ausgang nach oben
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}} %neu ecke links oben nach rechts oben
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}} %bei deneigängen runter 
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{.5\pgf@circ@res@down}}%ecke links unten nach rechts unten
		\pgfpathclose
		\pgfusepath{draw}
	\endpgfscope
  
	  }
	}	



%% Potentiometer
\pgfcircdeclarebipole{
	\anchor{wiper}{
		\northeast
		\pgfpoint{0pt}{\pgf@y}
	}
	\anchor{W}{
		\northeast
		\pgfpoint{0pt}{\pgf@y}
	}	
}{\ctikzvalof{bipoles/potentiometer/height 2}}{potentiometer}{\ctikzvalof{bipoles/potentiometer/height}}{\ctikzvalof{bipoles/potentiometer/width}}{
\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
\pgftransformationadjustments
\pgfmathsetlength{\pgf@circ@res@step}{\ctikzvalof{bipoles/resistor/width}\pgf@circ@Rlen+\pgfhorizontaltransformationadjustment*0.5*\pgflinewidth}
\divide \pgf@circ@res@step by 12

\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left-\pgfhorizontaltransformationadjustment*0.5*\pgflinewidth}{\pgf@circ@res@zero}}

\pgf@circ@res@other = \pgf@circ@res@left
\advance\pgf@circ@res@other by \pgf@circ@res@step 
\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{-\pgf@circ@res@down}}
\advance\pgf@circ@res@other by 2\pgf@circ@res@step 
\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@down}}
\advance\pgf@circ@res@other by 2\pgf@circ@res@step
\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{-\pgf@circ@res@down}}
\advance\pgf@circ@res@other by 2\pgf@circ@res@step
\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@down}}
\advance\pgf@circ@res@other by 2\pgf@circ@res@step
\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{-\pgf@circ@res@down}}
\advance\pgf@circ@res@other by 2\pgf@circ@res@step
\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@down}}
\advance\pgf@circ@res@other by \pgf@circ@res@step
\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@zero}}
\pgfsetbeveljoin
\pgfusepath{draw}

\pgfscope
	%\pgfsetlinewidth{\pgfstartlinewidth}
	\pgfsetarrowsend{latex'}
	\pgfpathmoveto{\pgfpoint{0pt}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{0pt}{-\pgf@circ@res@down}}
	\pgfusepath{draw}
\endpgfscope
}





%% Generic tunable 

\pgfcircdeclarebipole{
	\anchor{wiper}{
		\northeast
		\pgfpoint{0pt}{\pgf@y}
	}
}{\ctikzvalof{bipoles/generic potentiometer/height 2}}{genericpotentiometer}{\ctikzvalof{bipoles/generic potentiometer/height}}{\ctikzvalof{bipoles/generic potentiometer/width}}{

		\pgf@circ@res@step = \ctikzvalof{bipoles/resistor/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 14

		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{-\pgf@circ@res@down}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
					
		\pgfusepath{draw} 
		
		\pgfscope
		%\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfsetarrowsend{latex'}
		\pgfpathmoveto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{-\pgf@circ@res@down}}
		\pgfusepath{draw}
		\endpgfscope
}


\pgfdeclareshape{mixer}
{
	\savedanchor\northwest{
		\ifpgf@circuit@boxed
			\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/bipoles/twoport/width}\pgf@circ@Rlen
			\pgf@y=.5\pgf@y
			\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/bipoles/twoport/width}\pgf@circ@Rlen
			\pgf@x=.5\pgf@x
		\else	
			\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/mixer/width}\pgf@circ@Rlen
			\pgf@y=.5\pgf@y
			\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/mixer/width}\pgf@circ@Rlen
			\pgf@x=.5\pgf@x
		\fi
	}
	\anchor{center}{
		\pgfpointorigin
	}
	\anchor{left}{%
		\northwest
		\pgf@y=0pt
	}
	\anchor{1}{
		\northwest
		\pgf@y=0pt
	}
	\anchor{2}{
		\northwest
		\pgf@y=-\pgf@y
		\pgf@x=0pt
	}
	\anchor{3}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	}
	\anchor{4}{
		\northwest
		\pgf@y=\pgf@y
		\pgf@x=0pt
	}
	\anchor{in 1}{
		\northwest
		\pgf@y=0pt
	}
	\anchor{in1}{
		\northwest
		\pgf@y=0pt
	}
	\anchor{in}{
		\northwest
		\pgf@y=0pt
	}	  
	\anchor{in 2}{
		\northwest
		\pgf@y=-\pgf@y
		\pgf@x=0pt
	}
	\anchor{in2}{
		\northwest
		\pgf@y=-\pgf@y
		\pgf@x=0pt
	}
	\anchor{out}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	}
	\anchor{center}{
		\pgf@y=0pt
		\pgf@x=0pt
	}
	\anchor{east}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x  
	}
	\anchor{west}{
		\northwest
		\pgf@y=0pt
	}
	\anchor{south}{
		\northwest
		\pgf@x=0pt
		\pgf@y=-\pgf@y
	}
	\anchor{north}{
		\northwest
		\pgf@x=0pt
	}
	\anchor{south west}{
		\northwest
		\pgf@y=-\pgf@y
	}
	\anchor{north east}{
		\northwest
		\pgf@x=-\pgf@x
	}
	\anchor{north west}{
		\northwest
	}
	\anchor{south east}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@y=-\pgf@y
	}
	\backgroundpath{
		\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			
		\pgf@circ@res@step=\ctikzvalof{tripoles/mixer/width}\pgf@circ@Rlen
			
		\pgfscope
			\pgfstartlinewidth=\pgflinewidth
			
			% draw outer box
			\ifpgf@circuit@boxed
				\pgfnode{box}{center}{}{pgf@box}{\pgfusepath{draw}}
			\fi
			
			% draw outer circle
			\ifpgf@circuit@boxed
				\pgf@circ@res@step=.7\pgf@circ@res@step
				\pgfsetdash{}{0pt}	% draw solid circle if boxed
			\else
				\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
			\fi
			\pgfpathcircle{\pgfpoint{0}{0}} {0.5\pgf@circ@res@step}
			\pgfusepath{draw}
			
			% draw inner stuff
			\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
			\pgfsetlinewidth{\pgfstartlinewidth}
			\pgfpathmoveto{\pgfpointorigin}
			\pgfpathmoveto{\pgfpointpolar{135}{0.5\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpointpolar{-45}{0.5\pgf@circ@res@step}}
			\pgfpathmoveto{\pgfpointorigin}
			\pgfpathmoveto{\pgfpointpolar{45}{0.5\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpointpolar{-135}{0.5\pgf@circ@res@step}}
			\pgfusepath{draw}
			
		\endpgfscope
	}
}

\pgfdeclareshape{adder}
{
	\savedanchor\northwest{
		\ifpgf@circuit@boxed
			\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/bipoles/twoport/width}\pgf@circ@Rlen
			\pgf@y=.5\pgf@y
			\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/bipoles/twoport/width}\pgf@circ@Rlen
			\pgf@x=.5\pgf@x
		\else	
			\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/adder/width}\pgf@circ@Rlen
			\pgf@y=.5\pgf@y
			\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/adder/width}\pgf@circ@Rlen
			\pgf@x=.5\pgf@x
		\fi
	}
	\anchor{center}{
		\pgfpointorigin
	}
	\anchor{left}{%
		\northwest
		\pgf@y=0pt
	}
	\anchor{1}{
		\northwest
		\pgf@y=0pt
	}
	\anchor{2}{
		\northwest
		\pgf@y=-\pgf@y
		\pgf@x=0pt
	}
	\anchor{3}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	}
	\anchor{4}{
		\northwest
		\pgf@y=\pgf@y
		\pgf@x=0pt
	}
	\anchor{in 1}{
		\northwest
		\pgf@y=0pt
	}
	\anchor{in1}{
		\northwest
		\pgf@y=0pt
	}
	\anchor{in}{
		\northwest
		\pgf@y=0pt
	}	  
	\anchor{in 2}{
		\northwest
		\pgf@y=-\pgf@y
		\pgf@x=0pt
	}
	\anchor{in2}{
		\northwest
		\pgf@y=-\pgf@y
		\pgf@x=0pt
	}
	\anchor{out}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	}
	\anchor{center}{
		\pgf@y=0pt
		\pgf@x=0pt
	}
	\anchor{east}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x  
	}
	\anchor{west}{
		\northwest
		\pgf@y=0pt
	}
	\anchor{south}{
		\northwest
		\pgf@x=0pt
		\pgf@y=-\pgf@y
	}
	\anchor{north}{
		\northwest
		\pgf@x=0pt
	}
	\anchor{south west}{
		\northwest
		\pgf@y=-\pgf@y
	}
	\anchor{north east}{
		\northwest
		\pgf@x=-\pgf@x
	}
	\anchor{north west}{
		\northwest
	}
	\anchor{south east}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@y=-\pgf@y
	}
	\backgroundpath{
		\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			
		\pgf@circ@res@step=\ctikzvalof{tripoles/adder/width}\pgf@circ@Rlen
			
		\pgfscope
			\pgfstartlinewidth=\pgflinewidth
			
			% draw outer box
			\ifpgf@circuit@boxed
				\pgfnode{box}{center}{}{pgf@box}{\pgfusepath{draw}}
			\fi
			
			% draw outer circle
			\ifpgf@circuit@boxed
				\pgf@circ@res@step=.7\pgf@circ@res@step{}
				\pgfsetdash{}{0pt}	% draw solid circle if boxed
			\else
				\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
			\fi
			\pgfpathcircle{\pgfpoint{0}{0}} {0.5\pgf@circ@res@step}
			\pgfusepath{draw}
			
			% draw inner stuff
			\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
			\pgfsetlinewidth{\pgfstartlinewidth}
			
			\pgfpathmoveto{\pgfpointorigin}
			\pgfpathmoveto{\pgfpointpolar{0}{0.3\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpointpolar{180}{0.3\pgf@circ@res@step}}
			\pgfpathmoveto{\pgfpointorigin}
			\pgfpathmoveto{\pgfpointpolar{90}{0.3\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpointpolar{270}{0.3\pgf@circ@res@step}}
			\pgfsetlinewidth{2\pgflinewidth}
			\pgfusepath{draw}
			
		\endpgfscope				  
	}
}

\pgfdeclareshape{oscillator}
{
	\savedanchor\northwest{
		\ifpgf@circuit@boxed
			\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/bipoles/twoport/width}\pgf@circ@Rlen
			\pgf@y=.5\pgf@y
			\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/bipoles/twoport/width}\pgf@circ@Rlen
		\else	
			\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/oscillator/width}\pgf@circ@Rlen
			\pgf@y=.5\pgf@y
			\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/oscillator/width}\pgf@circ@Rlen
		\fi
	}
	\anchor{center}{
		\pgfpointorigin
	}
	\anchor{north}{
		\northwest
		\pgf@x=.5\pgf@x
	}
	\anchor{south}{
		\northwest
		\pgf@x=.5\pgf@x
		\pgf@y=-\pgf@y
	}
	\anchor{east}{
		\northwest
		\pgf@y=0pt
		\pgf@x=0pt
	}
	\anchor{west}{
		\northwest
		\pgf@y=0pt
	}
	\anchor{text}{
		\pgf@x=-2\pgf@x
		\advance \pgf@x by -.5\wd\pgfnodeparttextbox
		\advance \pgf@y by -1.5\ht\pgfnodeparttextbox
	}
	\backgroundpath{
		\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}
			
		\pgf@circ@res@step=\ctikzvalof{tripoles/oscillator/width}\pgf@circ@Rlen{}
			
		\pgfscope
			\pgfstartlinewidth=\pgflinewidth
			
			\pgftransformxshift{-0.5\pgf@circ@res@step} % The oscillator is shifted to the left, so a connection comes out of the anchor "east"
			
			% draw outer box
			\ifpgf@circuit@boxed{}
				\pgfnode{box}{center}{}{pgf@box}{\pgfusepath{draw}}
			\fi
			
			% draw outer circle
			\ifpgf@circuit@boxed
				\pgf@circ@res@step=.7\pgf@circ@res@step{}
				\pgfsetdash{}{0pt}	% draw solid circle if boxed
			\else
				\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
			\fi
			\pgfpathcircle{\pgfpoint{0}{0}} {0.5\pgf@circ@res@step}
			\pgfusepath{draw}
			
			% draw inner sine waves
			\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
			\pgfsetlinewidth{\pgfstartlinewidth}
			\pgfsetcornersarced{\pgfpointorigin}% do not use rounded corners!
			\pgfpathmoveto{\pgfpoint{-0.3\pgf@circ@res@step}{0\pgf@circ@res@step}}
			\pgfpathsine{\pgfpoint{.15\pgf@circ@res@step}{.15\pgf@circ@res@step}}
			\pgfpathcosine{\pgfpoint{.15\pgf@circ@res@step}{-.15\pgf@circ@res@step}}
			\pgfpathsine{\pgfpoint{.15\pgf@circ@res@step}{-.15\pgf@circ@res@step}}
			\pgfpathcosine{\pgfpoint{.15\pgf@circ@res@step}{.15\pgf@circ@res@step}}
		
			\pgfusepath{draw}
			
		\endpgfscope				  
	}
}

\pgfdeclareshape{circulator}
{
	\savedanchor\northwest{
		\ifpgf@circuit@boxed
			\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/bipoles/twoport/width}\pgf@circ@Rlen
			\pgf@y=.5\pgf@y
			\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/bipoles/twoport/width}\pgf@circ@Rlen
			\pgf@x=.5\pgf@x
		\else	
			\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/circulator/width}\pgf@circ@Rlen
			\pgf@y=.5\pgf@y
			\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/circulator/width}\pgf@circ@Rlen
			\pgf@x=.5\pgf@x
		\fi
	}
	\anchor{center}{
		\pgfpointorigin
	}
	\anchor{left}{%
		\northwest
	  	\pgf@y=0pt
	}
	\anchor{1}{
		\northwest
		\pgf@y=0pt
	}
	\anchor{2}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	}
	\anchor{3}{
		\northwest
		\pgf@y=-\pgf@y
		\pgf@x=0pt
	}
	\anchor{east}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x  
	}
	\anchor{west}{
		\northwest
		\pgf@y=0pt
	}
	\anchor{south}{
		\northwest
		\pgf@x=0pt
		\pgf@y=-\pgf@y
	}
	\anchor{north}{
		\northwest
		\pgf@x=0pt
	}
	\anchor{south west}{
		\northwest
		\pgf@y=-\pgf@y
	}
	\anchor{north east}{
		\northwest
		\pgf@x=-\pgf@x
	}
	\anchor{north west}{
		\northwest
	}
	\anchor{south east}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@y=-\pgf@y
	}
	\backgroundpath{
		\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			
		\pgf@circ@res@step=\ctikzvalof{tripoles/circulator/width}\pgf@circ@Rlen
			
		\pgfscope
			\pgfstartlinewidth=\pgflinewidth
			
			% draw outer box
			\ifpgf@circuit@boxed
				\pgfnode{box}{center}{}{pgf@box}{\pgfusepath{draw}}
			\fi
			
			% draw outer circle
			\ifpgf@circuit@boxed{}
				\pgf@circ@res@step=.7\pgf@circ@res@step{}
				\pgfsetdash{}{0pt}	% draw solid circle if boxed
			\else
				\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
			\fi
			\pgfpathcircle{\pgfpoint{0}{0}} {0.5\pgf@circ@res@step}
			\pgfusepath{draw}
			
			% inner arrow
			\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
			\pgfsetlinewidth{\pgfstartlinewidth}
			
			\pgfsetarrowsend{latex}
			\pgfpathmoveto{\pgfpoint{-0.25\pgf@circ@res@step}{0}}
			\pgfpatharc{180}{-90} {0.25\pgf@circ@res@step}
			\pgfpathlineto{\pgfpoint{-5pt}{-0.2\pgf@circ@res@step}}
			\pgfusepath{draw}
			
		\endpgfscope				  
	}
}


% Wilkinson divider
\pgfdeclareshape{wilkinson}{
		\anchor{center}{
			\northwest
			\pgf@x=0pt
			\pgf@y=0pt
		}
		\savedanchor\northwest{%
			\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/wilkinson/height}\pgf@circ@Rlen
			\pgf@y=.5\pgf@y
			\pgf@x= \pgf@circ@Rlen
			\pgf@x=.5\pgf@x
			\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/wilkinson/width}\pgf@x
			}
		\anchor{north}{
			\northwest
			\pgf@x=0pt
		}
		\anchor{south}{
			\northwest
			\pgf@x=0pt
			\pgf@y=-\pgf@y
		}
		\anchor{west}{
			\northwest
			\pgf@y=0pt
		}
		\anchor{east}{
			\northwest
			\pgf@y=0pt
			\pgf@x=-\pgf@x
		}
		\anchor{south west}{
			\northwest
			\pgf@y=-\pgf@y
		}
		\anchor{north east}{
			\northwest
			\pgf@x=-\pgf@x
		}
			\anchor{north west}{
			\northwest
		}
		\anchor{south east}{
			\northwest
			\pgf@x=-\pgf@x
			\pgf@y=-\pgf@y
		}
		\anchor{in}{
			\northwest
			\pgf@y=0pt
		}
		\anchor{out1}{
			\northwest
			\pgf@x=-\pgf@x
			\pgf@y=-0.5\pgf@y
		}
		\anchor{out2}{
			\northwest
			\pgf@x=-\pgf@x
			\pgf@y=0.5\pgf@y
		}
		\anchor{text}{
			\northwest
			\advance \pgf@y by 0.5\ht\pgfnodeparttextbox
			\pgf@x=-.5\wd\pgfnodeparttextbox
		}
		\backgroundpath{			
				\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			
				\northwest
				\pgf@circ@res@up = \pgf@y 
				\pgf@circ@res@down = -\pgf@y
				\pgf@circ@res@right = -\pgf@x
				\pgf@circ@res@left = \pgf@x
			
				\pgfstartlinewidth=\pgflinewidth

				% draw outer box
				\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
				\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
				\pgfusepath{draw}
				
				% draw inner stuff
				\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
				\pgfsetarrows{-} %never draw arrows
				\pgfsetlinewidth{\pgfstartlinewidth}
				\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfpathlineto{\pgfpoint{0.5\pgf@circ@res@left}{0pt}}
				\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0.5\pgf@circ@res@up}}
				\pgfpathlineto{\pgfpoint{0.5\pgf@circ@res@right}{0.5\pgf@circ@res@up}}
				\pgfpathlineto{\pgfpoint{0.5\pgf@circ@res@left}{0pt}}
				\pgfpathlineto{\pgfpoint{0.5\pgf@circ@res@right}{0.5\pgf@circ@res@down}}
				\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0.5\pgf@circ@res@down}}				
				
				\pgfusepath{draw}
				
				\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
				% draw inner resisitor - european or american style is recognised
				{
					\pgftransformshift{\pgfpoint{0.5\pgf@circ@res@right}{0pt}}
					\pgftransformrotate{90}
					
					% calculate size of resistor
					\ifpgf@circuit@europeanresistor
						\pgfmathparse{\pgf@circ@res@up / \pgf@circ@Rlen / \ctikzvalof{bipoles/generic/width} / 2}
						\pgftransformscale{\pgfmathresult}
						\pgfnode{genericshape}{center}{}{pgf@generic}{\pgfusepath{fill}}
					\else
						\pgfmathparse{\pgf@circ@res@up / \pgf@circ@Rlen / \ctikzvalof{bipoles/resistor/width} / 2}
						\pgftransformscale{\pgfmathresult}
						\pgfnode{resistorshape}{center}{}{pgf@resistor}{\pgfusepath{fill}}
					\fi
				}
				
				\pgfpathmoveto{\pgfpoint{0.5\pgf@circ@res@right}{0.5\pgf@circ@res@up}}
				\pgfpathlineto{\pgfpoint{0.5\pgf@circ@res@right}{0.25\pgf@circ@res@up}}
				
				\pgfpathmoveto{\pgfpoint{0.5\pgf@circ@res@right}{0.25\pgf@circ@res@down}}
				\pgfpathlineto{\pgfpoint{0.5\pgf@circ@res@right}{0.5\pgf@circ@res@down}}
				\pgfusepath{draw}

		}
}

% electromechanical device (motor/generator)
\pgfdeclareshape{elmech}
{
	\savedanchor\northwest{
			\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/elmech/height}\pgf@circ@Rlen
			\pgf@y=.5\pgf@y
			\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/elmech/width}\pgf@circ@Rlen
			\pgf@x=.5\pgf@x
	}
	\anchor{center}{
		\pgfpointorigin
	}
	  \anchor{text}{
		\pgfpointorigin
		\advance \pgf@x by -.5\wd\pgfnodeparttextbox
		\advance \pgf@y by -.5\ht\pgfnodeparttextbox
	}
	\anchor{left}{%
		\northwest
		\pgf@y=0pt
	}
	\anchor{right}{%
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	}
	\anchor{top}{
		\northwest
		\pgf@x=0pt
	}
	\anchor{pathstart}{
		\northwest
		\pgf@x=0pt
	}
	\anchor{pathend}{
		\northwest
		\pgf@x=0pt
		\pgf@y=-\pgf@y
	}
	\anchor{bottom}{
		\northwest
		\pgf@x=0pt
		\pgf@y=-\pgf@y
	}
	\anchor{center}{
		\pgf@y=0pt
		\pgf@x=0pt
	}
	\anchor{east}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	}
	\anchor{west}{
		\northwest
		\pgf@y=0pt
	}
	\anchor{south}{
		\northwest
		\pgf@x=0pt
		\pgf@y=-\pgf@y
	}
	\anchor{north}{
		\northwest
		\pgf@x=0pt
	}
		\backgroundpath{
		\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}
		\pgf@circ@res@step=\ctikzvalof{tripoles/elmech/width}\pgf@circ@Rlen
		\pgf@circ@res@up=\ctikzvalof{tripoles/elmech/height}\pgf@circ@Rlen
		\pgfscope
			\pgfstartlinewidth=\pgflinewidth
			% draw outer box
		%	\ifpgf@circuit@boxed
		%		\pgfnode{box}{center}{}{pgf@box}{\pgfusepath{draw}}
		%	\fi
			% draw outer circle
			%\ifpgf@circuit@boxed
			%	\pgf@circ@res@step=.7\pgf@circ@res@step
			%	\pgfsetdash{}{0pt}	% draw solid circle if boxed
			%\else
				\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
			%\fi
			\pgfpathrectangle{\pgfpoint{-.25\pgf@circ@res@step}{-.5\pgf@circ@res@up}}{\pgfpoint{.5\pgf@circ@res@step}{\pgf@circ@res@up}}
			\pgfsetfillcolor{black}
			\pgfusepath{draw,fill}
			\pgfpathcircle{\pgfpoint{0}{0}} {0.5\pgf@circ@res@step}
			\pgfsetfillcolor{white}
			\pgfusepath{draw,fill}
		\endpgfscope
	}
}

\pgfdeclareshape{magnetron}
{
	\savedanchor\northwest{
			\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/magnetron/width}\pgf@circ@Rlen
			\pgf@y=.5\pgf@y
			\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/magnetron/width}\pgf@circ@Rlen
			\pgf@x=.5\pgf@x
	}
	\anchor{center}{
		\pgfpointorigin
	}
	\anchor{anode}{
		\northwest
		\pgf@x=0pt
		\pgf@y=-\pgf@y
	}
	\anchor{cathode1}{
		\northwest
		\pgf@circ@res@step=\pgf@y
		\pgfmathparse{cos(105)}
		\pgf@x=\pgfmathresult\pgf@circ@res@step
		\pgfmathparse{sin(105)}
		\pgf@y=\pgfmathresult\pgf@circ@res@step
		%\pgfpointorigin
		%\pgfpathmoveto{\pgfpointpolar{105}{\pgf@circ@res@step}}%not working in a scaled tikzpicture
	}
	\anchor{cathode2}{
		\northwest
		\pgf@circ@res@step=\pgf@y
		\pgfmathparse{cos(75)}
		\pgf@x=\pgfmathresult\pgf@circ@res@step
		\pgfmathparse{sin(75)}
		\pgf@y=\pgfmathresult\pgf@circ@res@step
		%\pgfpointorigin
		%\pgfpathmoveto{\pgfpointpolar{75}{\pgf@circ@res@step}}%not working in a scaled tikzpicture
	}
	  \anchor{text}{
		\pgfpointorigin
		\advance \pgf@x by -.5\wd\pgfnodeparttextbox
		\advance \pgf@y by -.5\ht\pgfnodeparttextbox
	}
	\anchor{left}{%
		\northwest
		\pgf@y=0pt
	}
	\anchor{right}{%
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	}
	\anchor{top}{
		\northwest
		\pgf@x=0pt
	}
	\anchor{pathstart}{
		\northwest
		\pgf@x=0pt
	}
	\anchor{pathend}{
		\northwest
		\pgf@x=0pt
		\pgf@y=-\pgf@y
	}
	\anchor{bottom}{
		\northwest
		\pgf@x=0pt
		\pgf@y=-\pgf@y
	}
	\anchor{center}{
		\pgf@y=0pt
		\pgf@x=0pt
	}
	\anchor{east}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	}
	\anchor{west}{
		\northwest
		\pgf@y=0pt
	}
	\anchor{south}{
		\northwest
		\pgf@x=0pt
		\pgf@y=-\pgf@y
	}
	\anchor{north}{
		\northwest
		\pgf@x=0pt
	}
		\backgroundpath{
		\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}
		\pgf@circ@res@step=\ctikzvalof{tripoles/magnetron/width}\pgf@circ@Rlen
			\northwest
			\pgf@circ@res@up = \pgf@y 
			\pgf@circ@res@down = -\pgf@y
			\pgf@circ@res@right = -\pgf@x  
			\pgf@circ@res@left = \pgf@x
			\pgfmathsetlength{\pgf@circ@res@other}{sin(15)*\pgf@circ@res@up}

		\pgfscope
			\pgfstartlinewidth=\pgflinewidth
			% draw outer box
		%	\ifpgf@circuit@boxed
		%		\pgfnode{box}{center}{}{pgf@box}{\pgfusepath{draw}}
		%	\fi
			% draw outer circle
			%\ifpgf@circuit@boxed
			%	\pgf@circ@res@step=.7\pgf@circ@res@step
			%	\pgfsetdash{}{0pt}	% draw solid circle if boxed
			%\else
				\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
			%\fi
			%create outer circle
			\pgfpathcircle{\pgfpoint{0}{0}} {\pgf@circ@res@right}
			\pgfsetfillcolor{white}
			\pgfusepath{draw}
			%create chambers
			 \foreach \angle in {45,135,225,315}{
						\pgfpathmoveto{ \pgfpointpolar{\angle}{0.6\pgf@circ@res@right}}
						\pgfpathlineto{ \pgfpointpolar{\angle}{\pgf@circ@res@right}}
					}
			\pgfsetroundcap
			\pgfusepath{draw}
			\pgfscope
			%draw connection from outside
			%anode
				\pgfsetlinewidth{\pgfstartlinewidth}
				\pgfpathmoveto{\pgfpoint{0\pgf@circ@res@left}{\pgf@circ@res@down}}
				\pgfpathlineto{\pgfpoint{0\pgf@circ@res@right}{.5\pgf@circ@res@down}}
				%cathodes
				\pgfpathmoveto{\pgfpointpolar{105}{\pgf@circ@res@up}}
				\pgfpathlineto{\pgfpoint{-\pgf@circ@res@other}{.5\pgf@circ@res@up}}
				\pgfpathmoveto{\pgfpointpolar{75}{\pgf@circ@res@up}}
				\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{.5\pgf@circ@res@up}}
				\pgfsetbuttcap
				\pgfusepath{draw}
			\endpgfscope
			%create cathode
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@other}{.5\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{0}{.15\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{-\pgf@circ@res@other}{.5\pgf@circ@res@up}}
						\pgfusepath{draw}
			%create anode
			\pgfpathmoveto{\pgfpoint{0.3\pgf@circ@res@left}{.5\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{0.3\pgf@circ@res@right}{.5\pgf@circ@res@down}}
			
			\pgfsetbuttcap
			\pgfusepath{draw}
		\endpgfscope
	}
}

%%%---------- close: tex/pgfcirctripoles
%%%%%%%%%%% Springe nach tex/pgfcircquadpoles
%%%---------- open: tex/pgfcircquadpoles.tex
% Copyright 2007-2009 by Massimo Redaelli
%
% This file may be distributed and/or modified
%
% 1. under the LaTeX Project Public License and/or
% 2. under the GNU Public License.
%
% See the file doc/LICENSE for more details.

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%% Quadripoles

\long\def\pgfcircdeclarequadpole#1#2#3{
	\pgfdeclareshape{#1}
	{
	  \anchor{center}{
	  	\northwest
		\pgf@x=0pt
	  }
	  \savedanchor\northwest{%
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/#1/height}\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@x=.5\pgf@circ@Rlen
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/quadpoles/#1/width}\pgf@x
	  }
	  \anchor{A2}{
		\northwest
		\pgf@y=-\pgf@y
	  }
	  \anchor{B1}{
		\northwest
		\pgf@x=-\pgf@x
	  }
	  \anchor{A1}{
		\northwest
	  }
	  \anchor{B2}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@y=-\pgf@y
	  }
	  \anchor{north}{
	  	\northwest
		\pgf@x=0pt
	  }
	  \anchor{south}{
	  	\northwest
		\pgf@x=0pt
		\pgf@y=-\pgf@y
	  }
	  \anchor{west}{
	  	\northwest
		\pgf@y=0pt
	  }
	  \anchor{east}{
	  	\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	  }
	  \anchor{south west}{
		\northwest
		\pgf@y=-\pgf@y
	  }
	  \anchor{north east}{
		\northwest
		\pgf@x=-\pgf@x
	  }
	  \anchor{north west}{
		\northwest
	  }
	  \anchor{south east}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@y=-\pgf@y
	  }	  
	  \anchor{base}{
	  	\northwest
		\pgf@x=0pt	  	
	  }
	  #3
	  \backgroundpath{			
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			
			\northwest
			\pgf@circ@res@up = \pgf@y 
			\pgf@circ@res@down = -\pgf@y
			\pgf@circ@res@right = -\pgf@x
			\pgf@circ@res@left = \pgf@x
			
			#2
	  
	  }
	}
}



\def\pgf@circ@drawtransformerbasicanchor{
	\pgfkeysvalueof{/tikz/circuitikz/quadpoles/trans/height}
	 \anchor{AA2}{
		\northwest
		\pgf@x=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/transformer/width1}\pgf@x
		\pgf@x=.7\pgf@x
		\pgf@y=-\pgf@y
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/transformer/height1}\pgf@y
	  }
	  \anchor{BB1}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@x=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/transformer/width1}\pgf@x
		\pgf@x=.7\pgf@x
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/transformer/height1}\pgf@y
	  }
	  \anchor{AA1}{
		\northwest
		\pgf@x=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/transformer/width1}\pgf@x
		\pgf@x=.7\pgf@x
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/transformer/height1}\pgf@y
	  }
	  \anchor{BB2}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@x=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/transformer/width1}\pgf@x
		\pgf@x=.7\pgf@x
		\pgf@y=-\pgf@y
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/transformer/height1}\pgf@y
	  }
}

\def\pgf@circ@drawtransformerbasicbody{
	\def\stretto{.4}
	\pgfscope             
			\pgfslopedattimetrue 
			\pgfallowupsidedownattimetrue
			\pgftransformlineattime{.5}{%
				\pgfpoint%
					{\stretto\pgf@circ@res@left}%
					{\pgf@circ@res@up}%
			}{%
				\pgfpoint
					{\stretto\pgf@circ@res@left}%
					{\pgf@circ@res@down}%
			}
			
			\edef\pgf@circ@temp{\ctikzvalof{inductor}}%
			\def\pgf@temp{european}%
			\ifx\pgf@temp\pgf@circ@temp%
				\pgfnode{fullgenericshape}{center}{}{pgf@inductor1}{\pgfusepath{stroke}}
			\else%
				\def\pgf@temp{cute}
				\ifx\pgf@temp\pgf@circ@temp%
					\pgfnode{cuteinductorshape}{center}{}{pgf@inductor1}{\pgfusepath{stroke}}
				\else%
					\pgfnode{americaninductorshape}{center}{}{pgf@inductor1}{\pgfusepath{stroke}}
				\fi%
			\fi%

			
	\endpgfscope
	\pgfscope             
			\pgfslopedattimetrue 
			\pgfallowupsidedownattimetrue
			\pgftransformlineattime{.5}{%
				\pgfpoint%
					{\stretto\pgf@circ@res@right}%
					{\pgf@circ@res@down}%
			}{%
				\pgfpoint
					{\stretto\pgf@circ@res@right}%
					{\pgf@circ@res@up}%
			}

			\edef\pgf@circ@temp{\ctikzvalof{inductor}}%
			\def\pgf@temp{european}%
			\ifx\pgf@temp\pgf@circ@temp%
				\pgfnode{fullgenericshape}{center}{}{pgf@inductor2}{\pgfusepath{stroke}}
			\else%
				\def\pgf@temp{cute} 
				\ifx\pgf@temp\pgf@circ@temp%
					\pgfnode{cuteinductorshape}{center}{}{pgf@inductor2}{\pgfusepath{stroke}}
				\else%
					\pgfnode{americaninductorshape}{center}{}{pgf@inductor2}{\pgfusepath{stroke}}
				\fi%
			\fi%
			
	\endpgfscope
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\stretto\pgf@circ@res@left}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpointanchor{pgf@inductor1}{b}}
	
	\pgfpathmoveto{\pgfpointanchor{pgf@inductor1}{a}}
	\pgfpathlineto{\pgfpoint{\stretto\pgf@circ@res@left}{\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@down}}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\stretto\pgf@circ@res@right}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpointanchor{pgf@inductor2}{a}}
	
	\pgfpathmoveto{\pgfpointanchor{pgf@inductor2}{b}}
	\pgfpathlineto{\pgfpoint{\stretto\pgf@circ@res@right}{\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
	
	\pgfusepath{draw}
	
}


	
	% contrib Kristofer M. Monisit
	
	\pgfdeclareshape{fd op amp}
	{
	  \anchor{center}{\pgfpointorigin}
	  \savedanchor\northwest{%
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/height}\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/width}\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
	  }
	  \anchor{south}{
		\northwest
		\pgf@y=-\pgf@y
	  }
	  \anchor{north}{
		\northwest
	  }
	  \savedanchor\left{%
	  	\pgf@y=0pt
	  }
	  \savedanchor\inOne{%
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/height}\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@y
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/width}\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
	  }
	  \anchor{-}{
		\inOne
	  }
	  \anchor{+}{
		\inOne
		\pgf@y=-\pgf@y
	  }
	  \savedanchor\up{%
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/height}\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/width}\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
			\pgf@circ@res@up = \pgf@y
			\pgf@circ@res@right = -\pgf@x
			\pgf@circ@res@left = \pgf@x
	    \pgfpointlineattime{
			\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/up pos}}{
			\pgfpoint{
				\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}\pgf@circ@res@left}
				{\pgf@circ@res@up}}
			{\pgfpoint{.7\pgf@circ@res@right}{0pt}}
	  }
	  \anchor{up}{
		\up
	  }
	  \anchor{down}{
		\up
		\pgf@y=-\pgf@y
	  }
	  \anchor{out +}{
		\northwest
		\pgf@y=.5\pgf@y
		\pgf@x=-.7\pgf@x
	  }
	  \anchor{out -}{
		\northwest
		\pgf@y=-.5\pgf@y
		\pgf@x=-.7\pgf@x
	  }
	  \anchor{west}{
	  	\left
      }
		\anchor{east}{
			\left
			\pgf@x=-\pgf@x
		}

	  \backgroundpath{
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}

      \northwest
      \pgf@circ@res@up = \pgf@y
      \pgf@circ@res@down = -\pgf@y
      \pgf@circ@res@right = -\pgf@x
      \pgf@circ@res@left = \pgf@x

      % Negative input terminal
      \pgfpathmoveto{\pgfpoint
        {\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@up}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@up}}
      \pgftext[left, at=\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@up}]{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/font} $-$}
  

      % Positive input terminal
      \pgfpathmoveto{\pgfpoint
        {\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@down}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@down}}
      \pgftext[left, at=\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@down}]{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/font} $+$}
  

      % Negative output terminal
      \pgfpathmoveto{\pgfpoint
        {0.7\pgf@circ@res@right}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@down}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@down}}
      \pgftext[left, at=\pgfpoint{0.3\pgf@circ@res@left}{.3\pgf@circ@res@down}]{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/font} $-$}
  

      % Positive output terminal
      \pgfpathmoveto{\pgfpoint
        {0.7\pgf@circ@res@right}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@up}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@up}}
      \pgftext[left, at=\pgfpoint{0.3\pgf@circ@res@left}{.3\pgf@circ@res@up}]{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/font} $+$}
  
	  \pgfsetrectcap
      % Draw them all!
      \pgfusepath{draw}

      % Triangle
      \pgfscope
        \pgfsetlinewidth{2\pgflinewidth}
        \pgftransformxshift{.7\pgf@circ@res@left}
        \pgf@circ@res@step=\pgf@circ@res@right
        \advance\pgf@circ@res@step by -\pgf@circ@res@left
        \pgf@circ@res@step=.7\pgf@circ@res@step
        \pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{0pt}}
        \pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
        \pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
        \pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{0pt}}
        \pgfpathclose
        \pgfusepath{draw}
      \endpgfscope
	  }
	}




\pgfcircdeclarequadpole{transformer}{

	\pgf@circ@drawtransformerbasicbody

}{\pgf@circ@drawtransformerbasicanchor}

\pgfcircdeclarequadpole{transformer core}{

	\pgf@circ@drawtransformerbasicbody
	
	\pgfmoveto{\pgfpoint%
					{\ctikzvalof{quadpoles/transformer core/core width}\pgf@circ@res@right}%
					{\ctikzvalof{quadpoles/transformer core/core height}\pgf@circ@res@down}%
					}
	\pgflineto{
				\pgfpoint
					{\ctikzvalof{quadpoles/transformer core/core width}\pgf@circ@res@right}%
					{\ctikzvalof{quadpoles/transformer core/core height}\pgf@circ@res@up}%
					}

	\pgfmoveto{\pgfpoint%
					{\ctikzvalof{quadpoles/transformer core/core width}\pgf@circ@res@left}%
					{\ctikzvalof{quadpoles/transformer core/core height}\pgf@circ@res@down}%
					}
	\pgflineto{
				\pgfpoint
					{\ctikzvalof{quadpoles/transformer core/core width}\pgf@circ@res@left}%
					{\ctikzvalof{quadpoles/transformer core/core height}\pgf@circ@res@up}%
					}					
	
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgflinewidth}
	\pgfusepath{draw}
}{\pgf@circ@drawtransformerbasicanchor}


\pgfcircdeclarequadpole{gyrator}{

	\def\stretto{.4}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\stretto\pgf@circ@res@left}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\stretto\pgf@circ@res@left}{\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@down}}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\stretto\pgf@circ@res@right}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\stretto\pgf@circ@res@right}{\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
	
	\pgfusepath{draw}
	
	\pgfsetlinewidth{2\pgflinewidth}
	\pgfpathmoveto{\pgfpoint{\stretto\pgf@circ@res@left}{.7*\stretto\pgf@circ@res@down}}
	\pgfpatharc{90}{270}{.7*\stretto\pgf@circ@res@down}
	
	\pgfpathmoveto{\pgfpoint{\stretto\pgf@circ@res@right}{.7*\stretto\pgf@circ@res@up}}
	\pgfpatharc{-90}{90}{.7*\stretto\pgf@circ@res@down}
	\pgfusepath{draw}

}{}

%% four-port
% defines a general outer box for four-ports
% TikZ usage: 
%		\draw (0,0) node[coupler](coup){\SI{-3}{dB}}
%		(coup.port1) to[short,-o] ++(-1,0)
%

\long\def\pgfcircdeclarefourport#1#2{
	\pgfdeclareshape{#1}{
		\anchor{center}{
			\northwest
			\pgf@x=0pt
			\pgf@y=0pt
		}
		\savedanchor\northwest{%
			\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/#1/height}\pgf@circ@Rlen
			\pgf@y=.5\pgf@y
			\pgf@x=.5\pgf@circ@Rlen
			\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/quadpoles/#1/width}\pgf@x
			}
		\anchor{north}{
			\northwest
			\pgf@x=0pt
		}
		\anchor{south}{
			\northwest
			\pgf@x=0pt
			\pgf@y=-\pgf@y
		}
		\anchor{west}{
			\northwest
			\pgf@y=0pt
		}
		\anchor{east}{
			\northwest
			\pgf@y=0pt
			\pgf@x=-\pgf@x
		}
		\anchor{south west}{
			\northwest
			\pgf@y=-\pgf@y
		}
		\anchor{north east}{
			\northwest
			\pgf@x=-\pgf@x
		}
			\anchor{north west}{
			\northwest
		}
		\anchor{south east}{
			\northwest
			\pgf@x=-\pgf@x
			\pgf@y=-\pgf@y
		}
		\anchor{port1}{
			\northwest
			\pgf@y=-0.5\pgf@y
		}
		\anchor{port2}{
			\northwest
			\pgf@x=-\pgf@x
			\pgf@y=-0.5\pgf@y
		}
		\anchor{port3}{
			\northwest
			\pgf@x=-\pgf@x
			\pgf@y=0.5\pgf@y
		}
		\anchor{port4}{
			\northwest
			\pgf@y=0.5\pgf@y
		}
		\anchor{1}{
			\northwest
			\pgf@y=-0.5\pgf@y
		}
		\anchor{2}{
			\northwest
			\pgf@x=-\pgf@x
			\pgf@y=-0.5\pgf@y
		}
		\anchor{3}{
			\northwest
			\pgf@x=-\pgf@x
			\pgf@y=0.5\pgf@y
		}
		\anchor{4}{
			\northwest
			\pgf@y=0.5\pgf@y
		}
		
		\anchor{text}{
			\northwest
			\advance \pgf@y by 0.5\ht\pgfnodeparttextbox
			\pgf@x=-.5\wd\pgfnodeparttextbox
		}
		\backgroundpath{			
				\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			
				\northwest
				\pgf@circ@res@up = \pgf@y 
				\pgf@circ@res@down = -\pgf@y
				\pgf@circ@res@right = -\pgf@x
				\pgf@circ@res@left = \pgf@x
			
				\pgfstartlinewidth=\pgflinewidth

				% draw outer box
				\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
				\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
				\pgfusepath{draw}
				
				% draw inner stuff
				#2
				
				% draw inner text
				\pgftext[center,x=-0.15\pgf@circ@res@step,y=0]{\ctikzvalof{bipoles/twoport/text}}
		}
	}
}

% four-port
\pgfcircdeclarefourport{fourport}{}


% straight coupler
\pgfcircdeclarefourport{coupler}{
	\pgfsetlinewidth{\pgfstartlinewidth}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0.5\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0.5\pgf@circ@res@up}}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0.5\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0.5\pgf@circ@res@down}}
	\pgfusepath{draw}
	
	\pgfpathmoveto{\pgfpoint{0.7\pgf@circ@res@left}{0.4\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{0.7\pgf@circ@res@right}{0.4\pgf@circ@res@up}}
	\pgfsetarrows{latex-latex}
	\pgfusepath{draw}
	\pgfpathmoveto{\pgfpoint{0.7\pgf@circ@res@left}{0.4\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{0.7\pgf@circ@res@right}{0.4\pgf@circ@res@down}}
	\pgfsetarrows{latex-latex}
	\pgfusepath{draw}
}

% "bended" coupler
\pgfcircdeclarefourport{coupler2}{
	\pgfsetlinewidth{\pgfstartlinewidth}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0.5\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0.5\pgf@circ@res@up}}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0.5\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0.5\pgf@circ@res@down}}
	\pgfusepath{draw}
	
	\pgfpathmoveto{\pgfpoint{0.1\pgf@circ@res@left}{0pt}}
	\pgfpatharc{0}{90} {0.4\pgf@circ@res@up}
	\pgfsetarrowsend{latex}
	\pgfusepath{draw}
	\pgfpathmoveto{\pgfpoint{0.1\pgf@circ@res@left}{0pt}}
	\pgfpatharc{0}{-90} {0.4\pgf@circ@res@up}
	\pgfsetarrowsend{latex}
	\pgfusepath{draw}
	
	\pgfpathmoveto{\pgfpoint{0.1\pgf@circ@res@right}{0pt}}
	\pgfpatharc{180}{90} {0.4\pgf@circ@res@up}
	\pgfsetarrowsend{latex}
	\pgfusepath{draw}
	\pgfpathmoveto{\pgfpoint{0.1\pgf@circ@res@right}{0pt}}
	\pgfpatharc{-180}{-90} {0.4\pgf@circ@res@up}
	\pgfsetarrowsend{latex}
	\pgfusepath{draw}
	
	
}
%%%---------- close: tex/pgfcircquadpoles

%%%%%%%%%%% Springe nach tex/pgfcirclabel
%%%---------- open: tex/pgfcirclabel.tex
% Copyright 2007-2009 by Massimo Redaelli
%
% This file may be distributed and/or modified
%
% 1. under the LaTeX Project Public License and/or
% 2. under the GNU Public License.
%
% See the file doc/LICENSE for more details.

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%% Bipole label positioning

%% Options
\ctikzset{label/.style = { l=#1 } }
\ctikzset{l/.code = { 
	\pgfkeys{/tikz/circuitikz/bipole/label/name=#1}
	\ctikzsetvalof{bipole/label/unit}{}
	\ifpgf@circ@siunitx 
		\pgf@circ@handleSI{#1}
		\ifpgf@circ@siunitx@res 
			\edef\pgf@temp{\pgf@circ@handleSI@val}
			\pgfkeyslet{/tikz/circuitikz/bipole/label/name}{\pgf@temp}
			\edef\pgf@temp{\pgf@circ@handleSI@unit}
			\pgfkeyslet{/tikz/circuitikz/bipole/label/unit}{\pgf@temp}
		\else
		\fi
	\else
	\fi
}}

\ctikzset{label above/.code = { 
		l=#1, 
		\circuitikzbasekey/bipole/label/position=90 }
}

\ctikzset{l^/.style = { 
		l=#1,
		\circuitikzbasekey/bipole/label/position=90 } 
}

\ctikzset{label below/.code = { 
		l=#1,
		\circuitikzbasekey/bipole/label/position=-90 } 
}

\ctikzset{l_/.style = { 
		l=#1,
		\circuitikzbasekey/bipole/label/position=-90 } 
}

\ctikzset{annotation/.style = { a=#1 } }
\ctikzset{a/.code = {
		\pgfkeys{/tikz/circuitikz/bipole/annotation/name=#1}
		\ctikzsetvalof{bipole/annotation/unit}{}
		\ifpgf@circ@siunitx
		\pgf@circ@handleSI{#1}
		\ifpgf@circ@siunitx@res
		\edef\pgf@temp{\pgf@circ@handleSI@val}
		\pgfkeyslet{/tikz/circuitikz/bipole/annotation/name}{\pgf@temp}
		\edef\pgf@temp{\pgf@circ@handleSI@unit}
		\pgfkeyslet{/tikz/circuitikz/bipole/annotation/unit}{\pgf@temp}
		\else
		\fi
		\else
		\fi
	}}

\ctikzset{annotation above/.code = { 
	a=#1, 
	\circuitikzbasekey/bipole/annotation/position=90 }
}

\ctikzset{a^/.style = { 
	a=#1,
	\circuitikzbasekey/bipole/annotation/position=90 } 
}

\ctikzset{annotation below/.code = { 
	a=#1,
	\circuitikzbasekey/bipole/annotation/position=-90 } 
}
\ctikzset{a_/.style = { 
	a=#1,
	\circuitikzbasekey/bipole/annotation/position=-90 } 
}



\def\pgf@circ@drawlabels#1{
	\pgfextra{
		\pgfmathsubtract{\pgf@circ@direction}{90}
		\edef\pgf@circ@labanc{\expandafter\pgf@circ@stripdecimals\pgfmathresult\pgf@nil}
		
		\edef\pgf@circ@temp{\ctikzvalof{bipole/#1/position}} 
		\ifnum \pgf@circ@temp < 0
			\pgfmathadd{\pgf@circ@labanc}{180}
			\edef\pgf@circ@labanc{\expandafter\pgf@circ@stripdecimals\pgfmathresult\pgf@nil}
		\fi
		\ifpgf@circuit@bipole@inverted
			\pgfmathadd{\pgf@circ@temp}{180} %If shape is inverted, use opposite anchor
			\edef\pgf@circ@temp{\expandafter\pgf@circ@stripdecimals\pgfmathresult\pgf@nil}
		\fi
		
		\ifnum \ctikzvalof{mirror value} = -1
			\pgfmathadd{\pgf@circ@temp}{180} %If shape is mirrored, use opposite anchor
			\edef\pgf@circ@temp{\expandafter\pgf@circ@stripdecimals\pgfmathresult\pgf@nil}
		\fi
	}
		%Firstly, place a coodinate directly at the edge of the shape
		(\ctikzvalof{bipole/name}.\pgf@circ@temp) coordinate (labelcoor)
		%now decide, which labels should be drawn
		\pgfextra{
			\edef\pgf@temp{\ctikzvalof{label/align}}
			\def\pgf@circ@temp{straight}
		}
		\ifx\pgf@temp\pgf@circ@temp %straight
			\pgf@circ@drawreglabels{#1}
		\else
			\pgfextra{\def\pgf@circ@temp{rotate}}
			\ifx\pgf@temp\pgf@circ@temp %rotate
				\pgf@circ@drawrotlabels{#1}
			\else% smart
				\pgf@circ@drawsmartlabels{#1}
			\fi
		\fi
}


\def\pgf@circ@drawsmartlabels#1{
	\pgfextra{
		\pgfmathmod{\pgf@circ@direction}{90}
		\edef\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgfmathresult\pgf@nil}
	}
	\ifnum \pgfcircmathresult > 20	
		\ifnum \pgfcircmathresult < 70
			\pgf@circ@drawrotlabels{#1}
		\else
			\pgf@circ@drawreglabels{#1}
		\fi
	\else
		\pgf@circ@drawreglabels{#1}
	\fi
}


\def\pgf@circ@drawrotlabels#1{
	\pgfextra{
		\ifnum \ctikzvalof{bipole/#1/position}>0
		%we need some more space for placement below, due to mid-anchor
			\def\pgf@circ@labposdistance{1.5ex}
			\else
			\def\pgf@circ@labposdistance{2ex}
		\fi
		%Calculate rotation of the label from direction and strip decimals
		\edef\pgfcirclabrot{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		% rotate the label at second or third quadrant:
		\ifnum \pgfcirclabrot > 90 \ifnum \pgfcirclabrot < 270
			\pgfmathsubtract{\pgf@circ@direction}{180}
			\edef\pgfcirclabrot{\expandafter\pgf@circ@stripdecimals\pgfmathresult\pgf@nil}
			%invert the space relationships due to rotatet strings
			\ifnum \ctikzvalof{bipole/#1/position}>0
				\def\pgf@circ@labposdistance{2ex}
			\else
				\def\pgf@circ@labposdistance{1.5ex}
			\fi
		\fi\fi
		\pgfmathparse{\ctikzvalof{bipole/#1/position}>0?\pgf@circ@direction+90:\pgf@circ@direction-90}
		\edef\pgf@circ@labposangle{\expandafter\pgf@circ@stripdecimals\pgfmathresult\pgf@nil}
	}				
	(labelcoor)++(\pgf@circ@labposangle:\pgf@circ@labposdistance) coordinate(labelcoor)
	node[anchor=mid,rotate=\pgfcirclabrot](\ctikzvalof{bipole/name}#1){\pgf@circ@finallabels{#1}}
}

\def\pgf@circ@drawreglabels#1{

	%Now calculate all shape positions
	%Use mid-anchor at x-axis and base-anchor at y-axis, respectively.
	%All points between will be addressed by angled-anchors:
	\pgfextra{
		\pgfmathadd{\pgf@circ@labanc}{90}
		\edef\pgf@circ@temp{\expandafter\pgf@circ@stripdecimals\pgfmathresult\pgf@nil}
		\pgfmathparse{mod(\pgf@circ@temp,180)>135?mod(\pgf@circ@temp,180)-180:mod(\pgf@circ@temp,180)}
		\edef\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgfmathresult\pgf@nil}
	}
	%Values between -5 and 5 are at pos /neg x-axis, values around 90 are at both y-axis
	\ifnum \pgfcircmathresult > 84 \ifnum \pgfcircmathresult< 96
		\pgfextra{\edef\pgf@circ@labpos{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}}
		\ifnum \pgf@circ@labpos > 180
			\ifnum \ctikzvalof{bipole/#1/position} > 0
				\pgfextra{\def\pgf@circ@labanc{mid west}}
			\else
				\pgfextra{\def\pgf@circ@labanc{mid east}}
			\fi
		\else
			\ifnum \ctikzvalof{bipole/#1/position} > 0
				\pgfextra{\def\pgf@circ@labanc{mid east}}
			\else
				\pgfextra{\def\pgf@circ@labanc{mid west}}
			\fi
		\fi
	\fi\fi
	\ifnum \pgfcircmathresult <6
		\ifnum \ctikzvalof{bipole/#1/position} < 0
			%we need some more space for placement below, due to mid-anchor
			(labelcoor)++(-\pgf@circ@labanc:2ex) coordinate(labelcoor)
		\else
			(labelcoor)++(-\pgf@circ@labanc:1.5ex) coordinate(labelcoor)
		\fi
		\pgfextra{\def\pgf@circ@labanc{mid}}
	\fi
	 (labelcoor) node[anchor=\pgf@circ@labanc](\ctikzvalof{bipole/name}#1){\pgf@circ@finallabels{#1}}
}

\def\pgf@circ@finallabels#1{%
	\edef\pgf@temp{}%
	\edef\pgf@circ@temp{\ctikzvalof{bipole/#1/unit}}%
	\ifx\pgf@temp\pgf@circ@temp%
	\ctikzvalof{bipole/#1/name}%
	\else%
	$\SI{\ctikzvalof{bipole/#1/name}}{\ctikzvalof{bipole/#1/unit}}$%
	\fi%
}

\ctikzset{text/.style = { t=#1 } }
\ctikzset{t/.code = { 
	\ctikzsetvalof{bipoles/twoport/text}{#1}
}}
%%%---------- close: tex/pgfcirclabel
%%%%%%%%%%% Springe nach tex/pgfcircvoltage
%%%---------- open: tex/pgfcircvoltage.tex
% Copyright 2007-2009 by Massimo Redaelli
%
% This file may be distributed and/or modified
%
% 1. under the LaTeX Project Public License and/or
% 2. under the GNU Public License.
%
% See the file doc/LICENSE for more details.

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%%  Voltage management


\ctikzset{v^>/.style = {
		v = #1,
		\circuitikzbasekey/bipole/voltage/direction = forward,
		\circuitikzbasekey/bipole/voltage/position = above
	}
}

\ctikzset{v^</.style = {
		v = #1,
		\circuitikzbasekey/bipole/voltage/direction = backward,
		\circuitikzbasekey/bipole/voltage/position = above
	}
}

\ctikzset{v_>/.style = {
		v = #1,
		\circuitikzbasekey/bipole/voltage/direction = forward,
		\circuitikzbasekey/bipole/voltage/position = below
	} 
}

\ctikzset{v_</.style = {
		v = #1,
		\circuitikzbasekey/bipole/voltage/direction = backward,
		\circuitikzbasekey/bipole/voltage/position = below
	}
}

\ctikzset{v_/.style = {v = #1, \circuitikzbasekey/bipole/voltage/position = below} }
\ctikzset{v^/.style = {v = #1, \circuitikzbasekey/bipole/voltage/position  = above} }
\ctikzset{v>/.style = {v = #1, \circuitikzbasekey/bipole/voltage/direction = forward} }
\ctikzset{v</.style = {v = #1, \circuitikzbasekey/bipole/voltage/direction = backward} }

% Default position varies whether the component is a voltage source
% or not
\ctikzset{v/.code = {
			\ifpgf@circuit@bipole@isvoltage
				\pgfkeys{\circuitikzbasekey/bipole/voltage/position=above,
					\circuitikzbasekey/bipole/voltage/direction=forward}
			\else
				\ifpgf@circ@oldvoltagedirection
				\pgfkeys{\circuitikzbasekey/bipole/voltage/position=below,
					\circuitikzbasekey/bipole/voltage/direction=backward}
				\else
				\pgfkeys{\circuitikzbasekey/bipole/voltage/position=below,
					\circuitikzbasekey/bipole/voltage/direction=forward}
				\fi
			\fi
			\ifpgf@circ@oldvoltagedirection\else
			\ifpgf@circuit@bipole@iscurrent
			\ifpgf@circuit@bipole@current@backward
					\pgfkeys{\circuitikzbasekey/bipole/voltage/position=below,
					\circuitikzbasekey/bipole/voltage/direction=forward}
			\else
					\pgfkeys{\circuitikzbasekey/bipole/voltage/position=below,
					\circuitikzbasekey/bipole/voltage/direction=backward}
			\fi\fi\fi
	\pgfkeys{/tikz/circuitikz/bipole/voltage/label/name=#1}
	\ctikzsetvalof{bipole/voltage/label/unit}{}
	\ifpgf@circ@siunitx 
		\pgf@circ@handleSI{#1}
		\ifpgf@circ@siunitx@res
			\edef\pgf@temp{\pgf@circ@handleSI@val}
			\pgfkeyslet{/tikz/circuitikz/bipole/voltage/label/name}{\pgf@temp}
			\edef\pgf@temp{\pgf@circ@handleSI@unit}
			\pgfkeyslet{/tikz/circuitikz/bipole/voltage/label/unit}{\pgf@temp}
		\else
		\fi
	\else
	\fi
	}
}




%% Output routine for generic bipoles

\def\pgf@circ@drawvoltagegeneric{
	\pgfextra{
			\edef\pgf@temp{/tikz/circuitikz/bipoles/\pgfkeysvalueof{/tikz/circuitikz/bipole/kind}/voltage/straight label distance}
			\pgfkeysifdefined{\pgf@temp}
				{ 
					\edef\partheight{\ctikzvalof{bipoles/\pgfkeysvalueof{/tikz/circuitikz/bipole/kind}/voltage/straight label distance}}
					\edef\tmpdistfromline{(\partheight\pgf@circ@Rlen)}
				}
				{
				\pgfkeysifdefined{/tikz/circuitikz/bipoles/voltage/straight label distance}
					{
						\edef\partheight{\ctikzvalof{bipoles/voltage/straight label distance}}
						\edef\tmpdistfromline{(\partheight\pgf@circ@Rlen)}
					}
					{%calculate default value from part height
						\edef\partheight{0.5*\ctikzvalof{bipoles/\pgfkeysvalueof{/tikz/circuitikz/bipole/kind}/height}}
						\edef\tmpdistfromline{(\partheight\pgf@circ@Rlen+0.2\pgf@circ@Rlen)}
					}
				}
		\ifnum \ctikzvalof{mirror value}=-1
			\ifpgf@circuit@bipole@inverted
				\ifpgf@circuit@bipole@voltage@straight
					\def\distfromline{\tmpdistfromline}
				\else
					\def\distfromline{\ctikzvalof{voltage/distance from line}\pgf@circ@Rlen}
				\fi
			\else
				\ifpgf@circuit@bipole@voltage@straight
					\def\distfromline{-\tmpdistfromline}
				\else
					\def\distfromline{-\ctikzvalof{voltage/distance from line}\pgf@circ@Rlen}
				\fi
			\fi
		\else
			\ifpgf@circuit@bipole@inverted
				\ifpgf@circuit@bipole@voltage@straight
					\def\distfromline{-\tmpdistfromline}
				\else
					\def\distfromline{-\ctikzvalof{voltage/distance from line}\pgf@circ@Rlen}
				\fi
			\else
				\ifpgf@circuit@bipole@voltage@straight
					\def\distfromline{\tmpdistfromline}
				\else
					\def\distfromline{\ctikzvalof{voltage/distance from line}\pgf@circ@Rlen}
				\fi
			\fi
		\fi
		\ifpgf@circuit@bipole@voltage@below
			\def\pgf@circ@voltage@angle{90}
		\else
			\def\pgf@circ@voltage@angle{-90}
		\fi
		\edef\pgf@temp{/tikz/circuitikz/bipoles/\pgfkeysvalueof{/tikz/circuitikz/bipole/kind}/voltage/distance from node}
		\pgfkeysifdefined{\pgf@temp}
			{ \edef\distacefromnode{\ctikzvalof{bipoles/\pgfkeysvalueof{/tikz/circuitikz/bipole/kind}/voltage/distance from node}} }
			{ \edef\distacefromnode{\ctikzvalof{voltage/distance from node}} }
		\edef\pgf@temp{/tikz/circuitikz/bipoles/\pgfkeysvalueof{/tikz/circuitikz/bipole/kind}/voltage/bump b}
		\pgfkeysifdefined{\pgf@temp}
			{ \edef\bumpb{\ctikzvalof{bipoles/\pgfkeysvalueof{/tikz/circuitikz/bipole/kind}/voltage/bump b}} }
			{ \edef\bumpb{\ctikzvalof{voltage/bump b}} }
	}
	% %\pgf@circ@Rlen/16 is equal to the length of the currarrow
	coordinate (pgfcirc@midtmp) at ($(\tikztostart) ! \pgf@circ@Rlen/16 ! (anchorstartnode)$) %absolute move, minimum space is length of arrowhead
	coordinate (pgfcirc@midtmp) at ($(pgfcirc@midtmp) ! \distacefromnode ! (anchorstartnode)$)

	coordinate (pgfcirc@Vfrom) at ($(pgfcirc@midtmp) ! -\distfromline ! \pgf@circ@voltage@angle:(anchorstartnode)$)
	coordinate (pgfcirc@midtmp) at ($(\tikztotarget) ! \pgf@circ@Rlen/16 ! (anchorendnode)$)%absolute move, minimum space is length of arrowhead
	coordinate (pgfcirc@midtmp) at ($(pgfcirc@midtmp) ! \distacefromnode ! (anchorendnode)$)

	coordinate (pgfcirc@Vto) at ($(pgfcirc@midtmp) ! \distfromline ! \pgf@circ@voltage@angle : (anchorendnode)$)

	\ifpgf@circuit@bipole@voltage@below
		coordinate (pgfcirc@Vcont1) at ($(\ctikzvalof{bipole/name}.center) ! \bumpb ! (\ctikzvalof{bipole/name}.-110)$)
		coordinate (pgfcirc@Vcont2) at ($(\ctikzvalof{bipole/name}.center) ! \bumpb ! (\ctikzvalof{bipole/name}.-70)$)
	\else
		coordinate (pgfcirc@Vcont1) at ($(\ctikzvalof{bipole/name}.center) ! \bumpb ! (\ctikzvalof{bipole/name}.110)$)
		coordinate (pgfcirc@Vcont2) at ($(\ctikzvalof{bipole/name}.center) ! \bumpb ! (\ctikzvalof{bipole/name}.70)$)
	\fi

	\ifpgf@circuit@europeanvoltage
		\ifpgf@circuit@bipole@voltage@straight
			\ifpgf@circuit@bipole@voltage@backward
				(pgfcirc@Vto) --(pgfcirc@Vfrom) node[currarrow, sloped,  allow upside down, pos=1,anchor=tip] {}
			\else
				(pgfcirc@Vfrom) --(pgfcirc@Vto) node[currarrow, sloped,  allow upside down, pos=1,anchor=tip] {}
			\fi
		\else
			\ifpgf@circuit@bipole@voltage@backward
				(pgfcirc@Vto) .. controls (pgfcirc@Vcont2)  and (pgfcirc@Vcont1) ..
					node[currarrow, sloped,  allow upside down, pos=1] {}
				(pgfcirc@Vfrom)
			\else
				(pgfcirc@Vfrom) .. controls (pgfcirc@Vcont1)  and (pgfcirc@Vcont2) ..
					node[currarrow, sloped,  allow upside down, pos=1] {}
				(pgfcirc@Vto)
			\fi
		\fi
	\else
		\ifpgf@circuit@bipole@voltage@backward
			\ifpgf@circ@oldvoltagedirection
				(pgfcirc@Vfrom) node[inner sep=0, anchor=\pgf@circ@bipole@voltage@label@anchor]{\scriptsize$+$}
				(pgfcirc@Vto) node[inner sep=0, anchor=\pgf@circ@bipole@voltage@label@anchor]{$-$}
			\else
				(pgfcirc@Vfrom) node[inner sep=0, anchor=\pgf@circ@bipole@voltage@label@anchor]{\scriptsize$-$}
				(pgfcirc@Vto) node[inner sep=0, anchor=\pgf@circ@bipole@voltage@label@anchor]{$+$}
			\fi
		\else
			\ifpgf@circ@oldvoltagedirection
				(pgfcirc@Vfrom) node[inner sep=0, anchor=\pgf@circ@bipole@voltage@label@anchor]{\scriptsize$-$}
				(pgfcirc@Vto) node[inner sep=0, anchor=\pgf@circ@bipole@voltage@label@anchor]{$+$}
			\else
				(pgfcirc@Vfrom) node[inner sep=0, anchor=\pgf@circ@bipole@voltage@label@anchor]{\scriptsize$+$}
				(pgfcirc@Vto) node[inner sep=0, anchor=\pgf@circ@bipole@voltage@label@anchor]{$-$}
			\fi
		\fi
	\fi
}

%% Output routine for voltage sources
\def\pgf@circ@drawvoltagegenerator{
	\ifpgf@circuit@bipole@voltage@below
		coordinate (pgfcirc@Vfrom) at ($(\ctikzvalof{bipole/name}.center) ! \ctikzvalof{voltage/bump a} ! (\ctikzvalof{bipole/name}.-120)$)
		coordinate (pgfcirc@Vto) at ($(\ctikzvalof{bipole/name}.center) ! \ctikzvalof{voltage/bump a} ! (\ctikzvalof{bipole/name}.-60)$)
	\else
		coordinate (pgfcirc@Vfrom) at ($ (\ctikzvalof{bipole/name}.center) ! \ctikzvalof{voltage/bump a} ! (\ctikzvalof{bipole/name}.120)$)
		coordinate (pgfcirc@Vto) at ($ (\ctikzvalof{bipole/name}.center) ! \ctikzvalof{voltage/bump a} ! (\ctikzvalof{bipole/name}.60)$)
	\fi
	\ifpgf@circuit@europeanvoltage
		\ifpgf@circuit@bipole@voltage@backward
			(pgfcirc@Vto)  -- node[currarrow, sloped,  allow upside down, pos=1] {} (pgfcirc@Vfrom)
		\else
			(pgfcirc@Vfrom)  -- node[currarrow, sloped,  allow upside down, pos=1] {} (pgfcirc@Vto)
		\fi
	\else% american voltage
		\ifpgf@circuit@bipole@voltageoutsideofsymbol
		% if it is a battery, must put + and -
			\ifpgf@circuit@bipole@voltage@backward
				(pgfcirc@Vfrom)  node {$-$}  (pgfcirc@Vto) node {$+$}
			\else
				(pgfcirc@Vfrom)  node {$+$}  (pgfcirc@Vto) node {$-$}
			\fi
		\fi
	\fi
}

%% Output routine
\def\pgf@circ@drawvoltage{% node name 
%\pgf@circ@direction
	\pgfextra{
		\edef\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum\pgfcircmathresult >4 \ifnum\pgfcircmathresult <86
			\ifpgf@circuit@bipole@voltage@below
				\def\pgf@circ@bipole@voltage@label@anchor{north west}
			\else \def\pgf@circ@bipole@voltage@label@anchor{south east}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >85 \ifnum\pgfcircmathresult <95
			\ifpgf@circuit@bipole@voltage@below
				\def\pgf@circ@bipole@voltage@label@anchor{west}
			\else \def\pgf@circ@bipole@voltage@label@anchor{east}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >94 \ifnum\pgfcircmathresult <176
			\ifpgf@circuit@bipole@voltage@below
				 \def\pgf@circ@bipole@voltage@label@anchor{south west}
			\else \def\pgf@circ@bipole@voltage@label@anchor{north east}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >175 \ifnum\pgfcircmathresult <185
			\ifpgf@circuit@bipole@voltage@below
				  \def\pgf@circ@bipole@voltage@label@anchor{south}
			\else\def\pgf@circ@bipole@voltage@label@anchor{north}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >184 \ifnum\pgfcircmathresult <266
			\ifpgf@circuit@bipole@voltage@below
				 \def\pgf@circ@bipole@voltage@label@anchor{south east}
			\else\def\pgf@circ@bipole@voltage@label@anchor{north west}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >265 \ifnum\pgfcircmathresult <275
			\ifpgf@circuit@bipole@voltage@below
				 \def\pgf@circ@bipole@voltage@label@anchor{east}
			\else \def\pgf@circ@bipole@voltage@label@anchor{west}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >274 \ifnum\pgfcircmathresult <356
			\ifpgf@circuit@bipole@voltage@below
				  \def\pgf@circ@bipole@voltage@label@anchor{north east}
			\else\def\pgf@circ@bipole@voltage@label@anchor{south west}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >-1 \ifnum\pgfcircmathresult <5
			\ifpgf@circuit@bipole@voltage@below
				 \def\pgf@circ@bipole@voltage@label@anchor{north}
			\else\def\pgf@circ@bipole@voltage@label@anchor{south}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >355 \ifnum\pgfcircmathresult <361
			\ifpgf@circuit@bipole@voltage@below
				  \def\pgf@circ@bipole@voltage@label@anchor{north}
			\else\def\pgf@circ@bipole@voltage@label@anchor{south}
			\fi
		\fi\fi

		\ifnum \ctikzvalof{mirror value}=-1
			\ifpgf@circuit@bipole@voltage@below
				\pgf@circuit@bipole@voltage@belowfalse
			\else
				\pgf@circuit@bipole@voltage@belowtrue
			\fi
		\fi

		\ifpgf@circuit@bipole@inverted
			\ifpgf@circuit@bipole@voltage@below
				\pgf@circuit@bipole@voltage@belowfalse
			\else
				\pgf@circuit@bipole@voltage@belowtrue
			\fi
		\fi

		\ifpgf@circuit@bipole@voltage@below
			\def\pgf@circ@bipole@voltage@label@where{-90}
		\else
			\def\pgf@circ@bipole@voltage@label@where{90}
		\fi


		\edef\pgf@temp{/tikz/circuitikz/bipoles/\pgfkeysvalueof{/tikz/circuitikz/bipole/kind}/voltage/european label distance}
		\pgfkeysifdefined{\pgf@temp}
			{ \edef\eudist{\ctikzvalof{bipoles/\pgfkeysvalueof{/tikz/circuitikz/bipole/kind}/voltage/european label distance}} }
			{ \edef\eudist{\ctikzvalof{voltage/european label distance}} }

	\pgfsetcornersarced{\pgfpointorigin}% do not use rounded corners!
	}%end pgfextra

		\ifpgf@circuit@bipole@isvoltage
			\pgf@circ@drawvoltagegenerator
		\else
			\pgf@circ@drawvoltagegeneric
		\fi

	%	(\ctikzvalof{bipole/name}.\pgf@circ@bipole@voltage@label@where) %Zeile sinnlos!?
		\ifpgf@circuit@bipole@voltage@straight
			coordinate (Vlab) at ($(pgfcirc@Vto)!0.5!(pgfcirc@Vfrom) $)
			node [anchor=\pgf@circ@bipole@voltage@label@anchor, inner sep=2pt]
					  at (Vlab) { \pgf@circ@finallabels{voltage/label} }
		\else
		coordinate (Vlab) at ($(\ctikzvalof{bipole/name}.center) !
			\ifpgf@circuit@europeanvoltage
				\eudist
			\else
				\ctikzvalof{voltage/american label distance}
			\fi !
			(\ctikzvalof{bipole/name}.\pgf@circ@bipole@voltage@label@where)$)
		node [anchor=\pgf@circ@bipole@voltage@label@anchor, inner sep=2pt] at (Vlab) { \pgf@circ@finallabels{voltage/label} }
		\fi
}%end drawvoltages
%%%---------- close: tex/pgfcircvoltage
%%%%%%%%%%% Springe nach tex/pgfcirccurrent
%%%---------- open: tex/pgfcirccurrent.tex
% Copyright 2007-2009 by Massimo Redaelli
%
% This file may be distributed and/or modified
%
% 1. under the LaTeX Project Public License and/or
% 2. under the GNU Public License.
%
% See the file doc/LICENSE for more details.

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%% Current handling

%% Options
\ctikzset{i^>/.style = {
		i = #1,
		\circuitikzbasekey/bipole/current/direction = forward,
		\circuitikzbasekey/bipole/current/x position = after,
		\circuitikzbasekey/bipole/current/y position = above
	}
}

\ctikzset{i_>/.style = {
		i = #1,
		\circuitikzbasekey/bipole/current/direction = forward,
		\circuitikzbasekey/bipole/current/x position = after,
		\circuitikzbasekey/bipole/current/y position = below
	}
}

\ctikzset{i>^/.style = {
		i = #1,
		\circuitikzbasekey/bipole/current/direction = forward,
		\circuitikzbasekey/bipole/current/x position = before,
		\circuitikzbasekey/bipole/current/y position = above
	}
}

\ctikzset{i>_/.style = {
		i = #1,
		\circuitikzbasekey/bipole/current/direction = forward,
		\circuitikzbasekey/bipole/current/x position = before,
		\circuitikzbasekey/bipole/current/y position = below
	}
}

\ctikzset{i^</.style = {
		i = #1,
		\circuitikzbasekey/bipole/current/direction = backward,
		\circuitikzbasekey/bipole/current/x position = after,
		\circuitikzbasekey/bipole/current/y position = above
	}
}

\ctikzset{i_</.style = {
		i = #1,
		\circuitikzbasekey/bipole/current/direction = backward,
		\circuitikzbasekey/bipole/current/x position = after,
		\circuitikzbasekey/bipole/current/y position = below
	}
}

\ctikzset{i<^/.style = {
		i = #1,
		\circuitikzbasekey/bipole/current/direction = backward,
		\circuitikzbasekey/bipole/current/x position = before,
		\circuitikzbasekey/bipole/current/y position = above
	}
}

\ctikzset{i<_/.style = {
		i = #1,
		\circuitikzbasekey/bipole/current/direction = backward,
		\circuitikzbasekey/bipole/current/x position = before,
		\circuitikzbasekey/bipole/current/y position = below
	}
}

\ctikzset{i/.code = {
	\pgfkeys{\circuitikzbasekey/bipole/current/direction = forward,
					\circuitikzbasekey/bipole/current/x position = after,
					\circuitikzbasekey/bipole/current/y position = above }
	\pgfkeys{/tikz/circuitikz/bipole/current/label/name=#1}
	\ctikzsetvalof{bipole/current/label/unit}{}
	\ifpgf@circ@siunitx 
		\pgf@circ@handleSI{#1}
		\ifpgf@circ@siunitx@res 
			\edef\pgf@temp{\pgf@circ@handleSI@val}
			\pgfkeyslet{/tikz/circuitikz/bipole/current/label/name}{\pgf@temp}
			\edef\pgf@temp{\pgf@circ@handleSI@unit}
			\pgfkeyslet{/tikz/circuitikz/bipole/current/label/unit}{\pgf@temp}
		\else
		\fi
	\else
	\fi
%reverse current direction for voltage sources
	\ifpgf@circ@oldvoltagedirection\else
		\ifpgf@circuit@bipole@isvoltage
		\ifpgf@circuit@bipole@voltage@backward
			\pgfkeys{\circuitikzbasekey/bipole/current/direction = forward,
					\circuitikzbasekey/bipole/current/x position = after,
					\circuitikzbasekey/bipole/current/y position = below }
		\else
			\pgfkeys{\circuitikzbasekey/bipole/current/direction = backward,
					\circuitikzbasekey/bipole/current/x position = before,
					\circuitikzbasekey/bipole/current/y position = above }
	\fi\fi\fi
}
}


\ifpgf@circ@oldvoltagedirection
	\ctikzset{i</.style = { i = #1, \circuitikzbasekey/bipole/current/direction = backward } }
\else
	\ctikzset{i</.style = { i = #1, \circuitikzbasekey/bipole/current/direction = backward, \circuitikzbasekey/bipole/current/x position = before } }
\fi
\ctikzset{i_/.style = { i = #1, \circuitikzbasekey/bipole/current/y position = below } }
\ctikzset{i>/.style = {i = #1, \circuitikzbasekey/bipole/current/direction = forward } }
\ctikzset{i^/.style = { i= #1, \circuitikzbasekey/bipole/current/y position = above } }

%% Output routine 
\def\pgf@circ@drawcurrent{
	\pgfextra{
		\edef\pgf@circ@ffffff{\pgf@circ@direction}
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@ffffff\pgf@nil}

		\ifnum\pgfcircmathresult >4 \ifnum\pgfcircmathresult <86
			\ifpgf@circuit@bipole@current@below
				\def\pgf@circ@dir{north west} \else \def\pgf@circ@dir{south east}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >85 \ifnum\pgfcircmathresult <95
			\ifpgf@circuit@bipole@current@below
				\def\pgf@circ@dir{west} \else \def\pgf@circ@dir{east} 
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >94 \ifnum\pgfcircmathresult <176
			\ifpgf@circuit@bipole@current@below
				 \def\pgf@circ@dir{south west}\else \def\pgf@circ@dir{north east}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >175 \ifnum\pgfcircmathresult <185
			\ifpgf@circuit@bipole@current@below
				  \def\pgf@circ@dir{south}\else\def\pgf@circ@dir{north}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >184 \ifnum\pgfcircmathresult <266
			\ifpgf@circuit@bipole@current@below
				 \def\pgf@circ@dir{south east}\else\def\pgf@circ@dir{north west}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >265 \ifnum\pgfcircmathresult <275
			\ifpgf@circuit@bipole@current@below
				 \def\pgf@circ@dir{east}\else \def\pgf@circ@dir{west}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >274 \ifnum\pgfcircmathresult <356
			\ifpgf@circuit@bipole@current@below
				  \def\pgf@circ@dir{north east}\else\def\pgf@circ@dir{south west}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult <5
			\ifpgf@circuit@bipole@current@below
				 \def\pgf@circ@dir{north}\else\def\pgf@circ@dir{south} 
			\fi
		\fi
		\ifnum\pgfcircmathresult >355
			\ifpgf@circuit@bipole@current@below
				 \def\pgf@circ@dir{north}\else\def\pgf@circ@dir{south} 
			\fi
		\fi
		
		\ifpgf@circuit@bipole@current@below
			\def\pgf@circ@bipole@current@label@where{-90}
		\else
			\def\pgf@circ@bipole@current@label@where{+90}
		\fi
	}
	
	\pgfextra{\def\pgf@temp{short}\edef\pgf@circ@temp{\ctikzvalof{bipole/kind}}}
		\ifx\pgf@circ@temp\pgf@temp%draw current at a short at middle of the line
				(\tikztostart)--(\tikztotarget)
		\else% normal bipole or source
			\ifpgf@circuit@bipole@current@before
				 (\tikztostart)--(anchorstartnode)
			\else
				(anchorendnode)--(\tikztotarget)
			\fi
		\fi
		\ifpgf@circuit@bipole@current@backward
			\pgfextra{
				\pgfmathsubtract{\pgf@circ@ffffff}{180}
				\edef\pgf@circ@ffffff{\expandafter\pgf@circ@stripdecimals\pgfmathresult\pgf@nil}
				}
		\fi
	coordinate[currarrow,pos=\ctikzvalof{current/distance},rotate=\pgf@circ@ffffff](Iarrow)
	(Iarrow.\pgf@circ@bipole@current@label@where) node[anchor=\pgf@circ@dir]{\pgf@circ@finallabels{current/label}}
}

%%%---------- close: tex/pgfcirccurrent
%%%%%%%%%%% Springe nach tex/pgfcircflow
%%%---------- open: tex/pgfcircflow.tex
% Copyright 2007-2009 by Massimo Redaelli
%
% This file may be distributed and/or modified
%
% 1. under the LaTeX Project Public License and/or
% 2. under the GNU Public License.
%
% See the file doc/LICENSE for more details.

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%% flow handling

%% Options
\ctikzset{f^>/.style = {
		f = #1,
		\circuitikzbasekey/bipole/flow/direction = forward,
		\circuitikzbasekey/bipole/flow/x position = after,
		\circuitikzbasekey/bipole/curflowrent/y position = above
	}
}

\ctikzset{f_>/.style = {
		f = #1,
		\circuitikzbasekey/bipole/flow/direction = forward,
		\circuitikzbasekey/bipole/flow/x position = after,
		\circuitikzbasekey/bipole/flow/y position = below
	}
}

\ctikzset{f>^/.style = {
		f = #1,
		\circuitikzbasekey/bipole/flow/direction = forward,
		\circuitikzbasekey/bipole/flow/x position = before,
		\circuitikzbasekey/bipole/flow/y position = above
	}
}

\ctikzset{f>_/.style = {
		f = #1,
		\circuitikzbasekey/bipole/flow/direction = forward,
		\circuitikzbasekey/bipole/flow/x position = before,
		\circuitikzbasekey/bipole/flow/y position = below
	}
}

\ctikzset{f^</.style = {
		f = #1,
		\circuitikzbasekey/bipole/flow/direction = backward,
		\circuitikzbasekey/bipole/flow/x position = after,
		\circuitikzbasekey/bipole/flow/y position = above
	}
}

\ctikzset{f_</.style = {
		f = #1,
		\circuitikzbasekey/bipole/flow/direction = backward,
		\circuitikzbasekey/bipole/flow/x position = after,
		\circuitikzbasekey/bipole/flow/y position = below
	}
}

\ctikzset{f<^/.style = {
		f = #1,
		\circuitikzbasekey/bipole/flow/direction = backward,
		\circuitikzbasekey/bipole/flow/x position = before,
		\circuitikzbasekey/bipole/flow/y position = above
	}
}

\ctikzset{f<_/.style = {
		f = #1,
		\circuitikzbasekey/bipole/flow/direction = backward,
		\circuitikzbasekey/bipole/flow/x position = before,
		\circuitikzbasekey/bipole/flow/y position = below
	}
}

\ctikzset{f</.style = { f = #1, \circuitikzbasekey/bipole/flow/direction = backward} }
\ctikzset{f_/.style = { f = #1, \circuitikzbasekey/bipole/flow/y position = below } }
\ctikzset{f>/.style = { f = #1, \circuitikzbasekey/bipole/flow/direction = forward } }
\ctikzset{f^/.style = { f = #1, \circuitikzbasekey/bipole/flow/y position = above } }

\ctikzset{f/.code = {
	\pgfkeys{\circuitikzbasekey/bipole/flow/direction = forward,
					\circuitikzbasekey/bipole/flow/x position = after,
					\circuitikzbasekey/bipole/flow/y position = above }
	\pgfkeys{/tikz/circuitikz/bipole/flow/label/name=#1}
	\ctikzsetvalof{bipole/flow/label/unit}{}
	\ifpgf@circ@siunitx 
		\pgf@circ@handleSI{#1}
		\ifpgf@circ@siunitx@res 
			\edef\pgf@temp{\pgf@circ@handleSI@val}
			\pgfkeyslet{/tikz/circuitikz/bipole/flow/label/name}{\pgf@temp}
			\edef\pgf@temp{\pgf@circ@handleSI@unit}
			\pgfkeyslet{/tikz/circuitikz/bipole/flow/label/unit}{\pgf@temp}
		\else
		\fi
	\else
	\fi
}
}

%% Output routine 
\def\pgf@circ@drawflow{
	\pgfextra{
		\edef\pgf@circ@ffffff{\pgf@circ@direction}
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@ffffff\pgf@nil}

		\ifnum\pgfcircmathresult >4 \ifnum\pgfcircmathresult <86
			\ifpgf@circuit@bipole@flow@below
				\def\pgf@circ@dir{north west} \else \def\pgf@circ@dir{south east}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >85 \ifnum\pgfcircmathresult <95
			\ifpgf@circuit@bipole@flow@below
				\def\pgf@circ@dir{west} \else \def\pgf@circ@dir{east} 
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >94 \ifnum\pgfcircmathresult <176
			\ifpgf@circuit@bipole@flow@below
				 \def\pgf@circ@dir{south west}\else \def\pgf@circ@dir{north east}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >175 \ifnum\pgfcircmathresult <185
			\ifpgf@circuit@bipole@flow@below
				  \def\pgf@circ@dir{south}\else\def\pgf@circ@dir{north}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >184 \ifnum\pgfcircmathresult <266
			\ifpgf@circuit@bipole@flow@below
				 \def\pgf@circ@dir{south east}\else\def\pgf@circ@dir{north west}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >265 \ifnum\pgfcircmathresult <275
			\ifpgf@circuit@bipole@flow@below
				 \def\pgf@circ@dir{east}\else \def\pgf@circ@dir{west}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >274 \ifnum\pgfcircmathresult <356
			\ifpgf@circuit@bipole@flow@below
				  \def\pgf@circ@dir{north east}\else\def\pgf@circ@dir{south west}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult <5
			\ifpgf@circuit@bipole@flow@below
				 \def\pgf@circ@dir{north}\else\def\pgf@circ@dir{south} 
			\fi
		\fi
		\ifnum\pgfcircmathresult >355
			\ifpgf@circuit@bipole@flow@below
				 \def\pgf@circ@dir{north}\else\def\pgf@circ@dir{south} 
			\fi
		\fi
		
		\ifpgf@circuit@bipole@flow@below
			\def\pgf@circ@bipole@flow@label@where{-90}
		\else
			\def\pgf@circ@bipole@flow@label@where{+90}
		\fi
	}
	
	\pgfextra{\def\pgf@temp{short}\edef\pgf@circ@temp{\ctikzvalof{bipole/kind}}}
		\ifx\pgf@circ@temp\pgf@temp%draw flow at a short at middle of the line
				(\tikztostart)--(\tikztotarget)
		\else% normal bipole or source
			\ifpgf@circuit@bipole@flow@before
				 (\tikztostart)--(anchorstartnode)
			\else
				(anchorendnode)--(\tikztotarget)
			\fi
		\fi
	\pgfextra{
		\ifpgf@circuit@bipole@flow@backward
			\ifpgf@circuit@bipole@flow@below
				\def\flow@offset{\ctikzvalof{flow/offset}\pgf@circ@Rlen}
			\else
				\def\flow@offset{-\ctikzvalof{flow/offset}\pgf@circ@Rlen}
			\fi
			\pgfmathsubtract{\pgf@circ@ffffff}{180}
			\edef\pgf@circ@ffffff{\expandafter\pgf@circ@stripdecimals\pgfmathresult\pgf@nil}	
		\else
			\ifpgf@circuit@bipole@flow@below
				\def\flow@offset{-\ctikzvalof{flow/offset}\pgf@circ@Rlen}
			\else
				\def\flow@offset{\ctikzvalof{flow/offset}\pgf@circ@Rlen}
			\fi
		\fi
	}
	coordinate[flowarrow,pos=\ctikzvalof{flow/distance},rotate=\pgf@circ@ffffff,yshift=\flow@offset](Farrowpos)
	(Farrowpos.\pgf@circ@bipole@flow@label@where) node[anchor=\pgf@circ@dir]{ \pgf@circ@finallabels{flow/label}}
}

%%%---------- close: tex/pgfcircflow

% defaults

\setupmodule
   [current=european,
    voltage=european,
    resistor=american,
    inductor=cute,
    logic=american,
    siunitx=true,
    arrowmos=false]

\processaction
   [\currentmoduleparameter{voltage}]
   [european=>\ctikzset{voltage=european},
    american=>\ctikzset{voltage=american}]

\processaction
   [\currentmoduleparameter{current}]
   [european=>\ctikzset{ current=european},
    american=>\ctikzset{ current=american}]

\processaction
   [\currentmoduleparameter{label}]
   [straight=>\ctikzset{label/align = straight},
    align=>\ctikzset{label/align = rotate},
    smart=>\ctikzset{label/align = smart}]

\processaction
   [\currentmoduleparameter{resistor}]
   [european=>\ctikzset{ resistor=european},
    american=>\ctikzset{ resistor=american}]

\processaction
   [\currentmoduleparameter{inductor}]
   [european=>\ctikzset{ inductor=european},
    american=>\ctikzset{ inductor=american},
    cute=>\ctikzset{ inductor=cute}]

\processaction
   [\currentmoduleparameter{diode}]
   [full=>\ctikzset{ diode=full},
    empty=>\ctikzset{ diode=empty}]

\processaction
   [\currentmoduleparameter{logic}]
   [european=>\ctikzset{ logic ports=european},
    american=>\ctikzset{ logic ports=american}]

\processaction
   [\currentmoduleparameter{siunitx}]
   [true=>\def\SI#1#2{#1\,#2}
    \def\ampere{\rm{A}}
    \def\volt{\rm{V}}
    \def\ohm{\Omega}
    \def\siemens{\rm{S}}
    \def\farad{\rm{F}}
    \def\henry{\rm{H}}
    \def\second{\rm{s}}
    \def\coulomb{\rm{C}}
    \def\siemens{\rm{S}}
    \def\radians{\rm{rad}}
    \def\milli{\rm{m}}
    \def\micro{\mu}
    \def\nano{\rm{n}}
    \def\pico{\rm{p}}
    \def\kilo{\rm{k}}
    \def\mega{\rm{M}}
    \def\giga{\rm{G}}
    \def\tera{\rm{T}},
    false=>]
%   \s!default=>\pgf@circ@siunitxtrue,

\processaction
   [\currentmoduleparameter{arrowmos}]
   [true=>\pgf@circuit@mos@arrowstrue,
    false=>\pgf@circuit@mos@arrowsfalse]
%   \s!default=>\pgf@circuit@mos@arrowstrue,


\ifpgf@circ@siunitx
 % nothing! siunitx and xstrings don't work in context
\fi


% Context specific

\ctikzset{tripoles/op amp/font/.initial=\switchtobodyfont[small]}

%%%%%%%%%%% Springe nach tex/pgfcircpath
%%%---------- open: tex/pgfcircpath.tex

\def\pgf@circ@direction{0.0}

% Names
\ctikzset{name/.style = { n=#1 } } %%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%@@@
\ctikzset{n/.code = { 
	\pgfkeys{/tikz/circuitikz/bipole/name=#1}
}}

% Reflect the node along
\ctikzset{mirrored/.is choice}
\ctikzset{mirror value/.initial=1}
\ctikzset{mirrored/true/.code = {\ctikzsetvalof{mirror value}{-1}} }
\ctikzset{mirrored/false/.code = {\ctikzsetvalof{mirror value}{1}} }
\ctikzset{mirror/.style = {/tikz/circuitikz/mirrored=true}}

% Invert node along path
\ctikzset{inverted/.is choice}
\ctikzset{invert value/.initial=1}
\ctikzset{inverted/true/.code = {\ctikzsetvalof{invert value}{-1}\pgf@circuit@bipole@invertedtrue}}
\ctikzset{inverted/false/.code = {\ctikzsetvalof{invert value}{1}\pgf@circuit@bipole@invertedfalse}}
\ctikzset{invert/.style = {/tikz/circuitikz/inverted=true}}
\newif\ifpgf@circuit@bipole@inverted
\ctikzset{bipole/inverted/.is if=pgf@circuit@bipole@inverted}


\newif\ifpgf@circuit@bipole@voltage@backward
\ctikzset{bipole/voltage/direction/.is choice}
\ctikzset{bipole/voltage/direction/forward/.code={\pgf@circuit@bipole@voltage@backwardfalse}}
\ctikzset{bipole/voltage/direction/backward/.code={\pgf@circuit@bipole@voltage@backwardtrue}}



% Initialize paths
\def\pgfcircresetpath{
	\ctikzset{bipole/name=, bipole/label/name=, bipole/label/position=90, ,bipole/annotation/name=, bipole/annotation/position=-90, 
		bipole/inverted=false, bipole/kind=,
	  	bipole/voltage/direction=backward, bipole/voltage/label/name=, bipole/voltage/position=below,
	  	bipole/nodes/left=none, bipole/nodes/right=none, bipole/is voltage=false,bipole/is voltageoutsideofsymbol=false,bipole/is strokedsymbol=false,
		bipole/is current=false, bipole/current/label/name=, bipole/current/x position=after,
		bipole/current/y position=above, bipole/current/direction=forward, 
		mirrored=false
   }
}

%% Helper function for path-function to ensure using anchors between nodes
\def\set@explicit@center@anchor#1{
	\pgfutil@ifundefined{pgf@sh@ns@#1}
	{
	%This coordinate is no node(but a relative position or a coordinate), no further handling needed
	}{
	\pgfutil@in@.{#1}
	\ifpgfutil@in@
	% Anchor is used, do nothing!
	\else%
		\let\tikz@moveto@waiting=\relax
		\pgfpathmoveto{\tikz@last@position}%force movement, because tikz@moveto@waiting
		\edef#1{#1.center}%ensure using center anchor
	\fi
	}
}


%% Generic bipole path
\def\pgf@circ@bipole@path#1#2{

\pgfextra{
		\set@explicit@center@anchor{\tikztostart}
		\set@explicit@center@anchor{\tikztotarget}
		\pgfsyssoftpath@getcurrentpath{\myp@th}%% save current path to extend after calculation of correct start/end coordinates
		\ctikzset{bipole/kind = #1}
		\edef\pgf@temp{\ctikzvalof{bipole/name}}
		\def\pgf@circ@temp{}
		\ifx\pgf@temp\pgf@circ@temp % if it has not a name
			\pgfmathrandominteger{\pgf@circ@rand}{1000}{9999}
			\ctikzset{bipole/name = #2\pgf@circ@rand} % create it
		\fi
	}
	
		(\tikztostart) coordinate (\ctikzvalof{bipole/name}start)%necessary to get correct coordinates in the case of relativ start/end or constructions like ((node1)-|(node2))
		(\tikztotarget) coordinate (\ctikzvalof{bipole/name}end)
		\pgfextra{
			\pgfmathanglebetweenpoints{\pgfpointanchor{\ctikzvalof{bipole/name}start}{center}}
							{\pgfpointanchor{\ctikzvalof{bipole/name}end}{center}}
			\edef\pgf@circ@direction{\pgfmathresult}%Calculate direction(angle) of path
			\pgfsyssoftpath@setcurrentpath{\myp@th}		
		}
	\pgfextra{\def\pgf@temp{open}\def\pgf@circ@temp{#1}}
	\ifx\pgf@temp\pgf@circ@temp  % if it is an open
	\else
		--($(\ctikzvalof{bipole/name}start) ! .5\pgflinewidth ! (\ctikzvalof{bipole/name}end)$) %ugly workaround to get correct linejoins(node breaks path?)
	\fi
		($(\tikztostart) ! .5 ! (\tikztotarget)$)%%positio of middle node 
		node[#1shape, rotate=\pgf@circ@direction, yscale=\ctikzvalof{mirror value}, xscale=\ctikzvalof{invert value}] 
			(\ctikzvalof{bipole/name}) {}
			\ifpgf@circuit@bipole@inverted
				\ifcsname pgf@anchor@#1shape@pathstart\endcsname%if special path-anchors are defined, use them!
					coordinate	(anchorstartnode) at (\ctikzvalof{bipole/name}.pathend)
					coordinate	(anchorendnode) at (\ctikzvalof{bipole/name}.pathstart)
				\else
					coordinate	(anchorstartnode) at (\ctikzvalof{bipole/name}.right)
					coordinate	(anchorendnode) at (\ctikzvalof{bipole/name}.left)
				\fi
			\else
				\ifcsname pgf@anchor@#1shape@pathstart\endcsname%if special path-anchors are defined, use them!
					coordinate	(anchorstartnode) at (\ctikzvalof{bipole/name}.pathstart)
					coordinate	(anchorendnode) at (\ctikzvalof{bipole/name}.pathend)
				\else
					coordinate	(anchorstartnode) at (\ctikzvalof{bipole/name}.left)
					coordinate	(anchorendnode) at (\ctikzvalof{bipole/name}.right)
				\fi
			\fi
	\pgfextra{\def\pgf@temp{open}\def\pgf@circ@temp{#1}}
	\ifx\pgf@temp\pgf@circ@temp  % if it is an open
	\else
		\ifpgf@circuit@bipole@strokedsymbol%draw line thrue symbol(e.g. diodes)
			\ifcsname pgf@anchor@#1shape@strokepathstart\endcsname%if special path-anchors are defined, use them!
				(\ctikzvalof{bipole/name}start.center) -- (\ctikzvalof{bipole/name}.strokepathstart)
				(\ctikzvalof{bipole/name}.strokepathend)  -- (\ctikzvalof{bipole/name}end.center)
			\else
				(\ctikzvalof{bipole/name}start.center) -- (\ctikzvalof{bipole/name}end.center)
			\fi
		\else		
			(\ctikzvalof{bipole/name}start.center) -- (anchorstartnode)
			(anchorendnode)  -- (\ctikzvalof{bipole/name}end.center)
		\fi
	\fi
	
	\drawpoles
	\pgf@circ@ifkeyempty{bipole/label/name}\else\pgf@circ@drawlabels{label}\fi
	\pgf@circ@ifkeyempty{bipole/annotation/name}\else\pgf@circ@drawlabels{annotation}\fi
	\pgf@circ@ifkeyempty{bipole/voltage/label/name}\else\pgf@circ@drawvoltage\fi
	\pgf@circ@ifkeyempty{bipole/current/label/name}\else\pgf@circ@drawcurrent\fi
	\pgf@circ@ifkeyempty{bipole/flow/label/name}\else\pgf@circ@drawflow\fi
	\pgfextra{\def\pgf@temp{open}\def\pgf@circ@temp{#1}}
	\ifx\pgf@temp\pgf@circ@temp  % if it is an open
		(\ctikzvalof{bipole/name}end)%Move to end of path
	\else
		($(\ctikzvalof{bipole/name}end) ! .5\pgflinewidth ! (\ctikzvalof{bipole/name}start)$) -- (\ctikzvalof{bipole/name}end)%ugly workaround to get correct linejoins(node breaks path?)
		%tikztostart and tikztotarget could not be used, because it would break if target coordinate is something like (node1-|node2)
		
	\fi
	% reset
	\pgfextra{
		\pgfcircresetpath
	}  
	\tikztonodes%draw pending nodes an path
}


%% Path definitions
\def\pgf@circ@resistor@path#1{\ifpgf@circuit@europeanresistor\pgf@circ@bipole@path{generic}{#1}\else\pgf@circ@bipole@path{resistor}{#1}\fi}
\def\pgf@circ@vresistor@path#1{\ifpgf@circuit@europeanresistor\pgf@circ@bipole@path{tgeneric}{#1}\else\pgf@circ@bipole@path{vresistor}{#1}\fi}
\def\pgf@circ@potentiometer@path#1{\ifpgf@circuit@europeanresistor\pgf@circ@bipole@path{genericpotentiometer}{#1}\else\pgf@circ@bipole@path{potentiometer}{#1}\fi}
\def\pgf@circ@thermistor@path#1{\pgf@circ@bipole@path{thermistor}{#1}}
\def\pgf@circ@thermistorptc@path#1{\pgf@circ@bipole@path{thermistorptc}{#1}}
\def\pgf@circ@thermistorntc@path#1{\pgf@circ@bipole@path{thermistorntc}{#1}}
\def\pgf@circ@varistor@path#1{\pgf@circ@bipole@path{varistor}{#1}}
\def\pgf@circ@capacitor@path#1{\pgf@circ@bipole@path{capacitor}{#1}}
\def\pgf@circ@ecapacitor@path#1{\pgf@circ@bipole@path{ecapacitor}{#1}}
\def\pgf@circ@polarcapacitor@path#1{\pgf@circ@bipole@path{polarcapacitor}{#1}}
\def\pgf@circ@vcapacitor@path#1{\pgf@circ@bipole@path{vcapacitor}{#1}}
\def\pgf@circ@piezoelectric@path#1{\pgf@circ@bipole@path{piezoelectric}{#1}}
\def\pgf@circ@battery@path#1{\pgf@circ@bipole@path{battery}{#1}}
\def\pgf@circ@batteryone@path#1{\pgf@circ@bipole@path{battery1}{#1}}
\def\pgf@circ@batterytwo@path#1{\pgf@circ@bipole@path{battery2}{#1}}
\def\pgf@circ@europeaninductor@path#1{\pgf@circ@bipole@path{fullgeneric}{#1}}
\def\pgf@circ@americaninductor@path#1{\pgf@circ@bipole@path{americaninductor}{#1}}
\def\pgf@circ@cuteinductor@path#1{\pgf@circ@bipole@path{cuteinductor}{#1}}
\def\pgf@circ@inductor@path#1{%
	\pgfextra{
		\edef\pgf@circ@temp{\ctikzvalof{inductor}}%
		\def\pgf@temp{european}%
	}
	\ifx\pgf@temp\pgf@circ@temp%
		\pgf@circ@europeaninductor@path{#1}%
	\else%
		\pgfextra{	\def\pgf@temp{cute} }%
		\ifx\pgf@temp\pgf@circ@temp%
			\pgf@circ@cuteinductor@path{#1}%
		\else%
			\pgf@circ@americaninductor@path{#1}%
		\fi%
	\fi%
}
\def\pgf@circ@vinductor@path#1{
	\pgfextra{
		\edef\pgf@circ@temp{\ctikzvalof{inductor}}%
		\def\pgf@temp{european}%
	}
	\ifx\pgf@temp\pgf@circ@temp%
		\pgf@circ@veuropeaninductor@path{#1}%
	\else%
		\pgfextra{	\def\pgf@temp{cute} }%
		\ifx\pgf@temp\pgf@circ@temp%
			\pgf@circ@vcuteinductor@path{#1}%
		\else%
			\pgf@circ@vamericaninductor@path{#1}%
		\fi%
	\fi%
}
\def\pgf@circ@veuropeaninductor@path#1{\pgf@circ@bipole@path{tfullgeneric}{#1}}
\def\pgf@circ@vamericaninductor@path#1{\pgf@circ@bipole@path{vamericaninductor}{#1}}
\def\pgf@circ@vcuteinductor@path#1{\pgf@circ@bipole@path{vcuteinductor}{#1}}
\def\pgf@circ@lamp@path#1{\pgf@circ@bipole@path{lamp}{#1}}
\def\pgf@circ@esource@path#1{\pgf@circ@bipole@path{esource}{#1}}
\def\pgf@circ@pvsource@path#1{\pgf@circ@bipole@path{pvsource}{#1}}
\def\pgf@circ@vsource@path#1{\pgf@circ@bipole@path{vsource}{#1}}
\def\pgf@circ@dcvsource@path#1{\pgf@circ@bipole@path{dcvsource}{#1}}
\def\pgf@circ@vsourceam@path#1{\pgf@circ@bipole@path{vsourceAM}{#1}}
\def\pgf@circ@vsourcesin@path#1{\pgf@circ@bipole@path{vsourcesin}{#1}}
\def\pgf@circ@isource@path#1{\pgf@circ@bipole@path{isource}{#1}}
\def\pgf@circ@oosource@path#1{\pgf@circ@bipole@path{oosource}{#1}}
\def\pgf@circ@dcisource@path#1{\pgf@circ@bipole@path{dcisource}{#1}}
\def\pgf@circ@isourcesin@path#1{\pgf@circ@bipole@path{isourcesin}{#1}}
\def\pgf@circ@vsourcesquare@path#1{\pgf@circ@bipole@path{vsourcesquare}{#1}}
\def\pgf@circ@vsourcetri@path#1{\pgf@circ@bipole@path{vsourcetri}{#1}}
\def\pgf@circ@isourceam@path#1{\pgf@circ@bipole@path{isourceAM}{#1}}
\def\pgf@circ@cvsource@path#1{\pgf@circ@bipole@path{cvsource}{#1}}
\def\pgf@circ@cvsourceam@path#1{\pgf@circ@bipole@path{cvsourceAM}{#1}}
\def\pgf@circ@cvsourcesin@path#1{\pgf@circ@bipole@path{cvsourcesin}{#1}}
\def\pgf@circ@cisource@path#1{\pgf@circ@bipole@path{cisource}{#1}}
\def\pgf@circ@cisourceam@path#1{\pgf@circ@bipole@path{cisourceAM}{#1}}
\def\pgf@circ@cisourcesin@path#1{\pgf@circ@bipole@path{cisourcesin}{#1}}
\def\pgf@circ@short@path#1{\pgf@circ@bipole@path{short}{#1}}
\def\pgf@circ@cspst@path#1{\pgf@circ@bipole@path{cspst}{#1}}
\def\pgf@circ@ospst@path#1{\pgf@circ@bipole@path{ospst}{#1}}
\def\pgf@circ@nos@path#1{\pgf@circ@bipole@path{nos}{#1}}
\def\pgf@circ@ncs@path#1{\pgf@circ@bipole@path{ncs}{#1}}
\def\pgf@circ@pushbutton@path#1{\pgf@circ@bipole@path{pushbutton}{#1}}
\def\pgf@circ@open@path#1{\pgf@circ@bipole@path{open}{#1}}
\def\pgf@circ@generic@path#1{\pgf@circ@bipole@path{generic}{#1}}
\def\pgf@circ@ageneric@path#1{\pgf@circ@bipole@path{ageneric}{#1}}
\def\pgf@circ@tgeneric@path#1{\pgf@circ@bipole@path{tgeneric}{#1}}
\def\pgf@circ@fullgeneric@path#1{\pgf@circ@bipole@path{fullgeneric}{#1}}
\def\pgf@circ@tfullgeneric@path#1{\pgf@circ@bipole@path{tfullgeneric}{#1}}
\def\pgf@circ@ammeter@path#1{\pgf@circ@bipole@path{ammeter}{#1}}
\def\pgf@circ@ohmmeter@path#1{\pgf@circ@bipole@path{ohmmeter}{#1}}
\def\pgf@circ@voltmeter@path#1{\pgf@circ@bipole@path{voltmeter}{#1}}
\def\pgf@circ@empty@path#1{}
\def\pgf@circ@photoresistor@path#1{\pgf@circ@bipole@path{photoresistor}{#1}}
\def\pgf@circ@emptythyristor@path#1{\pgf@circ@bipole@path{emptythyristor}{#1}}
\def\pgf@circ@fullthyristor@path#1{\pgf@circ@bipole@path{fullthyristor}{#1}}
\def\pgf@circ@toggleswitch@path#1{\pgf@circ@bipole@path{toggleswitch}{#1}}
\def\pgf@circ@memristor@path#1{\pgf@circ@bipole@path{memristor}{#1}}
\def\pgf@circ@emptytriac@path#1{\pgf@circ@bipole@path{emptytriac}{#1}}
\def\pgf@circ@fulltriac@path#1{\pgf@circ@bipole@path{fulltriac}{#1}}
\def\pgf@circ@tline@path#1{\pgf@circ@bipole@path{tline}{#1}}
\def\pgf@circ@squid@path#1{\pgf@circ@bipole@path{squid}{#1}}
\def\pgf@circ@barrier@path#1{\pgf@circ@bipole@path{barrier}{#1}}
\def\pgf@circ@thermocouple@path#1{\pgf@circ@bipole@path{thermocouple}{#1}}
\def\pgf@circ@fuse@path#1{\pgf@circ@bipole@path{fuse}{#1}}
\def\pgf@circ@afuse@path#1{\pgf@circ@bipole@path{afuse}{#1}}

\def\pgf@circ@gfsurgearrester@path#1{\ifpgf@circuit@europeangfsurgearrester\pgf@circ@europeangfsurgearrester@path{#1}\else\pgf@circ@americangfsurgearrester@path{#1}\fi}
\def\pgf@circ@europeangfsurgearrester@path#1{\pgf@circ@bipole@path{european gas filled surge arrester}{#1}}
\def\pgf@circ@americangfsurgearrester@path#1{\pgf@circ@bipole@path{american gas filled surge arrester}{#1}}

\def\pgf@circ@twoport@path#1{\pgf@circ@bipole@path{twoport}{#1}}
\def\pgf@circ@vco@path#1{\pgf@circ@bipole@path{vco}{#1}}
\def\pgf@circ@bandpass@path#1{\pgf@circ@bipole@path{bandpass}{#1}}
\def\pgf@circ@bandstop@path#1{\pgf@circ@bipole@path{bandstop}{#1}}
\def\pgf@circ@highpass@path#1{\pgf@circ@bipole@path{highpass}{#1}}
\def\pgf@circ@lowpass@path#1{\pgf@circ@bipole@path{lowpass}{#1}}
\def\pgf@circ@adc@path#1{\pgf@circ@bipole@path{adc}{#1}}
\def\pgf@circ@dac@path#1{\pgf@circ@bipole@path{dac}{#1}}
\def\pgf@circ@dsp@path#1{\pgf@circ@bipole@path{dsp}{#1}}
\def\pgf@circ@fft@path#1{\pgf@circ@bipole@path{fft}{#1}}
\def\pgf@circ@amp@path#1{\pgf@circ@bipole@path{amp}{#1}}
\def\pgf@circ@vamp@path#1{\pgf@circ@bipole@path{vamp}{#1}}
\def\pgf@circ@piattenuator@path#1{\pgf@circ@bipole@path{piattenuator}{#1}}
\def\pgf@circ@vpiattenuator@path#1{\pgf@circ@bipole@path{vpiattenuator}{#1}}
\def\pgf@circ@tattenuator@path#1{\pgf@circ@bipole@path{tattenuator}{#1}}
\def\pgf@circ@vtattenuator@path#1{\pgf@circ@bipole@path{vtattenuator}{#1}}
\def\pgf@circ@phaseshifter@path#1{\pgf@circ@bipole@path{phaseshifter}{#1}}
\def\pgf@circ@vphaseshifter@path#1{\pgf@circ@bipole@path{vphaseshifter}{#1}}
\def\pgf@circ@detector@path#1{\pgf@circ@bipole@path{detector}{#1}}

%%Mechanical
\def\pgf@circ@spring@path#1{\pgf@circ@bipole@path{spring}{#1}}
\def\pgf@circ@mass@path#1{\pgf@circ@bipole@path{mass}{#1}}
\def\pgf@circ@damper@path#1{\pgf@circ@bipole@path{damper}{#1}}




%% Styles

\def\comnpatname{\ifpgf@circuit@compat *\else\fi}
\def\compattikzset#1{\tikzset{\comnpatname#1}}

%\def\ctikzsetbipole#1#2{%
%	\tikzset{#1/.style= {to path=#2, \circuitikzbasekey, l=##1}}%
%}

\compattikzset{spring/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@spring@path, l=#1}}
\compattikzset{mass/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@mass@path, l=#1}}
\compattikzset{damper/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@damper@path, l=#1}}
\compattikzset{resistor/.style= {\circuitikzbasekey, /tikz/to path=\pgf@circ@resistor@path, l=#1}}
\compattikzset{american resistor/.style= {\circuitikzbasekey, /tikz/to path=\pgf@circ@bipole@path{resistor}{#1}, l=#1}}
\compattikzset{european resistor/.style= {\circuitikzbasekey, /tikz/to path=\pgf@circ@bipole@path{generic}{#1}, l=#1}}
\compattikzset{potentiometer/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@potentiometer@path, l=#1}}
\compattikzset{varistor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@varistor@path, l=#1}}
\compattikzset{photoresistor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@photoresistor@path, l=#1}}
\compattikzset{thermistor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@thermistor@path, l=#1}}
\compattikzset{thermistor ptc/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@thermistorptc@path, l=#1}}
\compattikzset{thermistor ntc/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@thermistorntc@path, l=#1}}
\compattikzset{american potentiometer/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@bipole@path{potentiometer}{#1}, l=#1}}
\compattikzset{european potentiometer/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@bipole@path{genericpotentiometer}{#1}, l=#1}}
\compattikzset{variable resistor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@vresistor@path, l=#1}}
\compattikzset{variable american resistor/.style= {\circuitikzbasekey, /tikz/to path=\pgf@circ@bipole@path{vresistor}{#1}, l=#1}}
\compattikzset{variable european resistor/.style= {\circuitikzbasekey, /tikz/to path=\pgf@circ@bipole@path{tgeneric}{#1}, l=#1}}
\compattikzset{capacitor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@capacitor@path, l=#1}}
\compattikzset{elko/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@ecapacitor@path, l=#1}}
\compattikzset{ecapacitor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@ecapacitor@path, l=#1}}
\compattikzset{polar capacitor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@polarcapacitor@path, l=#1}}
\compattikzset{variable capacitor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@vcapacitor@path, l=#1}}
\compattikzset{piezoelectric/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@piezoelectric@path, l=#1}}
\compattikzset{battery/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@battery@path, \circuitikzbasekey/bipole/is voltage=true,  \circuitikzbasekey/bipole/is voltageoutsideofsymbol=true, v=#1}}
\compattikzset{battery1/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@batteryone@path, \circuitikzbasekey/bipole/is voltage=true,  \circuitikzbasekey/bipole/is voltageoutsideofsymbol=true, v=#1}}
\compattikzset{battery2/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@batterytwo@path, \circuitikzbasekey/bipole/is voltage=true,  \circuitikzbasekey/bipole/is voltageoutsideofsymbol=true, v=#1}}
\compattikzset{inductor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@inductor@path, l=#1}}
\compattikzset{gf surge arrester/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@gfsurgearrester@path, l=#1}}
\compattikzset{american gas filled surge arrester/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@americangfsurgearrester@path, l=#1}}
\compattikzset{european gas filled surge arrester/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@europeangfsurgearrester@path, l=#1}}
\compattikzset{gas filled surge arrester/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@gfsurgearrester@path, l=#1}}
\compattikzset{american inductor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@americaninductor@path, l=#1}}
\compattikzset{cute inductor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@cuteinductor@path, l=#1}}
\compattikzset{european inductor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@europeaninductor@path, l=#1}}
\compattikzset{variable inductor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@vinductor@path, l=#1}}
\compattikzset{variable european inductor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@veuropeaninductor@path, l=#1}}
\compattikzset{variable american inductor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@vamericaninductor@path, l=#1}}
\compattikzset{variable cute inductor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@vcuteinductor@path, l=#1}}
\compattikzset{tline/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@tline@path, l=#1}}
\compattikzset{transmission line/.style = {tline = #1}}
\compattikzset{TL/.style = {tline = #1}}
\compattikzset{european voltage source/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@vsource@path, \circuitikzbasekey/bipole/is voltage=true, \circuitikzbasekey/bipole/is voltageoutsideofsymbol=true, v=#1}}
\compattikzset{american voltage source/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@vsourceam@path, \circuitikzbasekey/bipole/is voltage=true, v=#1}}
\compattikzset{european current source/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@isource@path, \circuitikzbasekey/bipole/is current=true, i=#1}}
\compattikzset{american current source/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@isourceam@path, \circuitikzbasekey/bipole/is current=true, i=#1}}
\compattikzset{european controlled voltage source/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@cvsource@path, \circuitikzbasekey/bipole/is voltage=true, \circuitikzbasekey/bipole/is voltageoutsideofsymbol=true, v=#1}}
\compattikzset{american controlled voltage source/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@cvsourceam@path, \circuitikzbasekey/bipole/is voltage=true, v=#1}}
\compattikzset{european controlled current source/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@cisource@path, \circuitikzbasekey/bipole/is current=true, i=#1}}
\compattikzset{american controlled current source/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@cisourceam@path, \circuitikzbasekey/bipole/is current=true, i=#1}}
\compattikzset{sinusoidal voltage source/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@vsourcesin@path, \circuitikzbasekey/bipole/is voltage=true, \circuitikzbasekey/bipole/is voltageoutsideofsymbol=true, v=#1 }}
\compattikzset{square voltage source/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@vsourcesquare@path, \circuitikzbasekey/bipole/is voltage=true, \circuitikzbasekey/bipole/is voltageoutsideofsymbol=true, v=#1 }}
\compattikzset{triangle voltage source/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@vsourcetri@path, \circuitikzbasekey/bipole/is voltage=true, \circuitikzbasekey/bipole/is voltageoutsideofsymbol=true, v=#1 }}
\compattikzset{sinusoidal current source/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@isourcesin@path, \circuitikzbasekey/bipole/is current=true, i=#1}}
\compattikzset{controlled sinusoidal voltage source/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@cvsourcesin@path, \circuitikzbasekey/bipole/is voltage=true, \circuitikzbasekey/bipole/is voltageoutsideofsymbol=true, v=#1}}
\compattikzset{controlled sinusoidal current source/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@cisourcesin@path, \circuitikzbasekey/bipole/is current=true, i=#1}}

\compattikzset{voltage source/.style = {\comnpatname \ifpgf@circuit@europeanvoltage european \else american \fi voltage source, \circuitikzbasekey/bipole/is voltage=true, v=#1}}
\compattikzset{current source/.style = {\comnpatname \ifpgf@circuit@europeancurrent european \else american \fi current source = #1, \circuitikzbasekey/bipole/is current=true}}
\compattikzset{controlled voltage source/.style = {\comnpatname \ifpgf@circuit@europeanvoltage european \else american \fi controlled voltage source, \circuitikzbasekey/bipole/is voltage=true, v=#1}}
\compattikzset{controlled current source/.style = {\comnpatname \ifpgf@circuit@europeancurrent european \else american \fi controlled current source = #1, \circuitikzbasekey/bipole/is current=true}}


\compattikzset{generic/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@generic@path, l=#1}}
\compattikzset{ageneric/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@ageneric@path, l=#1}}
\compattikzset{tgeneric/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@tgeneric@path, l=#1}}
\compattikzset{fullgeneric/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@fullgeneric@path, l=#1}}
\compattikzset{tfullgeneric/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@tfullgeneric@path, l=#1}}
\compattikzset{short/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@short@path}}
\compattikzset{open/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@open@path}}

\compattikzset{lamp/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@lamp@path}}

\compattikzset{squid/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@squid@path}}
\compattikzset{barrier/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@barrier@path}}
\compattikzset{thermocouple/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@thermocouple@path}}
\compattikzset{fuse/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@fuse@path}}
\compattikzset{asymmetric fuse/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@afuse@path}}

\compattikzset{twoport/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@twoport@path}}
\compattikzset{vco/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@vco@path}}
\compattikzset{bandpass/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@bandpass@path}}
\compattikzset{bandstop/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@bandstop@path}}
\compattikzset{highpass/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@highpass@path}}
\compattikzset{lowpass/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@lowpass@path}}
\compattikzset{adc/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@adc@path}}
\compattikzset{dac/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@dac@path}}
\compattikzset{dsp/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@dsp@path}}
\compattikzset{fft/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@fft@path}}
\compattikzset{amp/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@amp@path}}
\compattikzset{vamp/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@vamp@path}}
\compattikzset{piattenuator/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@piattenuator@path}}
\compattikzset{vpiattenuator/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@vpiattenuator@path}}
\compattikzset{tattenuator/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@tattenuator@path}}
\compattikzset{vtattenuator/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@vtattenuator@path}}
\compattikzset{phaseshifter/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@phaseshifter@path}}
\compattikzset{vphaseshifter/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@vphaseshifter@path}}
\compattikzset{detector/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@detector@path}}

% % % % % %
% % Beginn of Diodes
% % % % % %

\def\pgf@circ@fulldiode@path#1{\pgf@circ@bipole@path{fulldiode}{#1}}
\def\pgf@circ@fullzdiode@path#1{\pgf@circ@bipole@path{fullzdiode}{#1}}
\def\pgf@circ@fullzzdiode@path#1{\pgf@circ@bipole@path{fullzzdiode}{#1}}
\def\pgf@circ@fullsdiode@path#1{\pgf@circ@bipole@path{fullsdiode}{#1}}
\def\pgf@circ@fulltdiode@path#1{\pgf@circ@bipole@path{fulltdiode}{#1}}
\def\pgf@circ@fulllediode@path#1{\pgf@circ@bipole@path{fulllediode}{#1}}
\def\pgf@circ@fullpdiode@path#1{\pgf@circ@bipole@path{fullpdiode}{#1}}
\def\pgf@circ@fullvarcap@path#1{\pgf@circ@bipole@path{fullvarcap}{#1}}
\def\pgf@circ@emptydiode@path#1{\pgf@circ@bipole@path{emptydiode}{#1}}
\def\pgf@circ@emptyzdiode@path#1{\pgf@circ@bipole@path{emptyzdiode}{#1}}
\def\pgf@circ@emptyzzdiode@path#1{\pgf@circ@bipole@path{emptyzzdiode}{#1}}
\def\pgf@circ@emptysdiode@path#1{\pgf@circ@bipole@path{emptysdiode}{#1}}
\def\pgf@circ@emptytdiode@path#1{\pgf@circ@bipole@path{emptytdiode}{#1}}
\def\pgf@circ@emptylediode@path#1{\pgf@circ@bipole@path{emptylediode}{#1}}
\def\pgf@circ@emptypdiode@path#1{\pgf@circ@bipole@path{emptypdiode}{#1}}
\def\pgf@circ@emptyvarcap@path#1{\pgf@circ@bipole@path{emptyvarcap}{#1}}

\compattikzset{full diode/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@fulldiode@path}}
\compattikzset{full Schottky diode/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@fullsdiode@path}}
\compattikzset{full Zener diode/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@fullzdiode@path}}
\compattikzset{full ZZener diode/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@fullzzdiode@path}}
\compattikzset{full tunnel diode/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@fulltdiode@path}}
\compattikzset{full photodiode/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@fullpdiode@path}}
\compattikzset{full led/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@fulllediode@path}}
\compattikzset{full varcap/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@fullvarcap@path}}
\compattikzset{full thyristor/.style =  {\circuitikzbasekey, /tikz/to path=\pgf@circ@fullthyristor@path}}
\compattikzset{full triac/.style =  {\circuitikzbasekey, /tikz/to path=\pgf@circ@fulltriac@path}}

\compattikzset{empty diode/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@emptydiode@path}}
\compattikzset{empty Schottky diode/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@emptysdiode@path}}
\compattikzset{empty Zener diode/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@emptyzdiode@path}}
\compattikzset{empty ZZener diode/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@emptyzzdiode@path}}
\compattikzset{empty tunnel diode/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@emptytdiode@path}}
\compattikzset{empty photodiode/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@emptypdiode@path}}
\compattikzset{empty led/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@emptylediode@path}}
\compattikzset{empty varcap/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@emptyvarcap@path}}
\compattikzset{empty thyristor/.style =  {\circuitikzbasekey, /tikz/to path=\pgf@circ@emptythyristor@path}}
\compattikzset{empty triac/.style =  {\circuitikzbasekey, /tikz/to path=\pgf@circ@emptytriac@path}}

\compattikzset{stroke diode/.style = {\circuitikzbasekey,\circuitikzbasekey/bipole/is strokedsymbol=true, /tikz/to path=\pgf@circ@emptydiode@path}}
\compattikzset{stroke Schottky diode/.style = {\circuitikzbasekey,\circuitikzbasekey/bipole/is strokedsymbol=true, /tikz/to path=\pgf@circ@emptysdiode@path}}
\compattikzset{stroke Zener diode/.style = {\circuitikzbasekey,\circuitikzbasekey/bipole/is strokedsymbol=true, /tikz/to path=\pgf@circ@emptyzdiode@path}}
\compattikzset{stroke ZZener diode/.style = {\circuitikzbasekey,\circuitikzbasekey/bipole/is strokedsymbol=true, /tikz/to path=\pgf@circ@emptyzzdiode@path}}
\compattikzset{stroke tunnel diode/.style = {\circuitikzbasekey,\circuitikzbasekey/bipole/is strokedsymbol=true, /tikz/to path=\pgf@circ@emptytdiode@path}}
\compattikzset{stroke photodiode/.style = {\circuitikzbasekey,\circuitikzbasekey/bipole/is strokedsymbol=true, /tikz/to path=\pgf@circ@emptypdiode@path}}
\compattikzset{stroke led/.style = {\circuitikzbasekey,\circuitikzbasekey/bipole/is strokedsymbol=true, /tikz/to path=\pgf@circ@emptylediode@path}}
\compattikzset{stroke varcap/.style = {\circuitikzbasekey,\circuitikzbasekey/bipole/is strokedsymbol=true, /tikz/to path=\pgf@circ@emptyvarcap@path}}
\compattikzset{stroke thyristor/.style =  {\circuitikzbasekey,\circuitikzbasekey/bipole/is strokedsymbol=true, /tikz/to path=\pgf@circ@emptythyristor@path}}
%\compattikzset{stroke triac/.style =  {\circuitikzbasekey,\circuitikzbasekey/bipole/is strokedsymbol=true, /tikz/to path=\pgf@circ@emptytriac@path}}

\def\pgfcircdiodestylemacro{\ifpgf@circuit@strokediode stroke \else\ifpgf@circuit@fulldiode full \else empty \fi\fi}

\compattikzset{Schottky diode/.style = {\comnpatname \pgfcircdiodestylemacro Schottky diode}}
\compattikzset{Zener diode/.style = {\comnpatname \pgfcircdiodestylemacro Zener diode}}
\compattikzset{ZZener diode/.style = {\comnpatname \pgfcircdiodestylemacro ZZener diode}}
\compattikzset{tunnel diode/.style = {\comnpatname \pgfcircdiodestylemacro tunnel diode}}
\compattikzset{photodiode/.style = {\comnpatname \pgfcircdiodestylemacro photodiode}}
\compattikzset{led/.style = {\comnpatname \pgfcircdiodestylemacro led}}
\compattikzset{varcap/.style = {\comnpatname \pgfcircdiodestylemacro varcap}}
\compattikzset{diode/.style = {\comnpatname \pgfcircdiodestylemacro diode}}
\compattikzset{thyristor/.style =  {\comnpatname \pgfcircdiodestylemacro thyristor}}
\compattikzset{triac/.style =  {\comnpatname \ifpgf@circuit@fulldiode full \else empty \fi triac}}%no stroke triac!

%% Define Shortcuts
\compattikzset{Do/.style = {\comnpatname empty diode}}
\compattikzset{tDo/.style = {\comnpatname empty tunnel diode}}
\compattikzset{zDo/.style = {\comnpatname empty Zener diode}}
\compattikzset{zzDo/.style = {\comnpatname empty ZZener diode}}
\compattikzset{sDo/.style = {\comnpatname empty Schottky diode}}
\compattikzset{pDo/.style = {\comnpatname empty photodiode}}
\compattikzset{leDo/.style = {\comnpatname empty led}}
\compattikzset{VCo/.style = {\comnpatname empty varcap}}
\compattikzset{Tyo/.style = {\comnpatname empty thyristor}}
\compattikzset{Tro/.style = {\comnpatname empty triac}}

\compattikzset{D*/.style = {\comnpatname full diode}}
\compattikzset{tD*/.style = {\comnpatname full tunnel diode}}
\compattikzset{zD*/.style = {\comnpatname full Zener diode}}
\compattikzset{zzD*/.style = {\comnpatname full ZZener diode}}
\compattikzset{sD*/.style = {\comnpatname full Schottky diode}}
\compattikzset{pD*/.style = {\comnpatname full photodiode}}
\compattikzset{leD*/.style = {\comnpatname full led}}
\compattikzset{VC*/.style = {\comnpatname full varcap}}
\compattikzset{Ty*/.style = {\comnpatname full thyristor}}
\compattikzset{Tr*/.style = {\comnpatname full triac}}

\compattikzset{D/.style = {\comnpatname diode}}
\compattikzset{tD/.style = {\comnpatname tunnel diode}}
\compattikzset{zD/.style = {\comnpatname Zener diode}}
\compattikzset{zzD/.style = {\comnpatname ZZener diode}}
\compattikzset{sD/.style = {\comnpatname Schottky diode}}
\compattikzset{pD/.style = {\comnpatname photodiode}}
\compattikzset{leD/.style = {\comnpatname led}}
\compattikzset{VC/.style = {\comnpatname varcap}}
\compattikzset{Ty/.style = {\comnpatname thyristor}}
\compattikzset{Tr/.style = {\comnpatname triac}}

\compattikzset{D-/.style = {\comnpatname stroke diode}}
\compattikzset{tD-/.style = {\comnpatname stroke tunnel diode}}
\compattikzset{zD-/.style = {\comnpatname stroke Zener diode}}
\compattikzset{zzD-/.style = {\comnpatname stroke ZZener diode}}
\compattikzset{sD-/.style = {\comnpatname stroke Schottky diode}}
\compattikzset{pD-/.style = {\comnpatname stroke photodiode}}
\compattikzset{leD-/.style = {\comnpatname stroke led}}
\compattikzset{VC-/.style = {\comnpatname stroke varcap}}
\compattikzset{Ty-/.style = {\comnpatname stroke thyristor}}
\compattikzset{Tr-/.style = {\comnpatname empty triac}}%no stroke triac!

% % % % % %
% % End of Diodes
% % % % % %


\compattikzset{memristor/.style =  {\circuitikzbasekey, /tikz/to path=\pgf@circ@memristor@path}}
\compattikzset{closing switch/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@cspst@path, l=#1}}
\compattikzset{opening switch/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@ospst@path, l=#1}}
\compattikzset{ncs/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@ncs@path, l=#1}}
\compattikzset{nos/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@nos@path, l=#1}}
\compattikzset{normal closed switch/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@ncs@path, l=#1}}
\compattikzset{normal open switch/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@nos@path, l=#1}}
\compattikzset{switch/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@cspst@path, l=#1}}
\compattikzset{push button/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@pushbutton@path, l=#1}}
\compattikzset{toggle switch/.style =  {\circuitikzbasekey, /tikz/to path=\pgf@circ@toggleswitch@path}}

\compattikzset{ammeter/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@ammeter@path}}
\compattikzset{voltmeter/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@voltmeter@path}}
\compattikzset{ohmmeter/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@ohmmeter@path}}

% short forms
\compattikzset{esource/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@esource@path, \circuitikzbasekey/bipole/is voltage=true,\circuitikzbasekey/bipole/is voltageoutsideofsymbol=true,  v=#1}}
\compattikzset{pvsource/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@pvsource@path, \circuitikzbasekey/bipole/is voltage=true,\circuitikzbasekey/bipole/is voltageoutsideofsymbol=true,  v=#1}}
\compattikzset{dcvsource/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@dcvsource@path, \circuitikzbasekey/bipole/is voltage=true,\circuitikzbasekey/bipole/is voltageoutsideofsymbol=true, v=#1}}
\compattikzset{dcisource/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@dcisource@path, \circuitikzbasekey/bipole/is current=true, l=#1}}

\compattikzset{ioosource/.style = {\circuitikzbasekey, \circuitikzbasekey/bipole/is current=true,/tikz/to path=\pgf@circ@oosource@path, i=#1}}
\compattikzset{voosource/.style = {\circuitikzbasekey, \circuitikzbasekey/bipole/is voltage=true,/tikz/to path=\pgf@circ@oosource@path, v=#1}}

\compattikzset{vsource/.style = {\comnpatname voltage source = #1}}
\compattikzset{isource/.style = {\comnpatname current source = #1}}
\compattikzset{cisource/.style = {\comnpatname controlled current source = #1}}
\compattikzset{cvsource/.style = {\comnpatname controlled voltage source = #1}}
\compattikzset{vsourcesin/.style = {\comnpatname sinusoidal voltage source = #1}}
\compattikzset{vsourcesquare/.style = {\comnpatname square voltage source = #1}}
\compattikzset{vsourcetri/.style = {triangle voltage source = #1}}
\compattikzset{isourcesin/.style = {\comnpatname sinusoidal current source = #1}}
\compattikzset{cisourcesin/.style = {\comnpatname controlled sinusoidal current source = #1}}
\compattikzset{cvsourcesin/.style = {\comnpatname controlled sinusoidal  voltage source = #1}}

\compattikzset{controlled vsource/.style = {\comnpatname controlled voltage source = #1}}
\compattikzset{controlled isource/.style = {\comnpatname controlled current source = #1}}
\compattikzset{controlled vsourcesin/.style = {\comnpatname controlled sinusoidal  voltage source = #1}}
\compattikzset{controlled isourcesin/.style = {\comnpatname controlled sinusoidal current source = #1}}

\compattikzset{R/.style= {\comnpatname resistor = #1}}
%\ifpgf@circuit@compat\else\compattikzset{R/.style= {resistor = #1}}\fi
\compattikzset{vR/.style= {\comnpatname variable resistor = #1}}
\compattikzset{phR/.style= {\comnpatname photoresistor = #1}}
\compattikzset{thR/.style= {\comnpatname thermistor = #1}}
\compattikzset{thRp/.style= {\comnpatname thermistor ptc= #1}}
\compattikzset{thRn/.style= {\comnpatname thermistor ntc= #1}}
\compattikzset{pR/.style= {\comnpatname potentiometer = #1}}
\compattikzset{C/.style = {\comnpatname capacitor = #1}}
\compattikzset{eC/.style = {\comnpatname ecapacitor = #1}}
\compattikzset{pC/.style = {\comnpatname polar capacitor = #1}}
\compattikzset{vC/.style = {\comnpatname variable capacitor = #1}}
\compattikzset{PZ/.style = {\comnpatname piezoelectric = #1}}
\compattikzset{L/.style = {\comnpatname inductor = #1}}
\compattikzset{vL/.style = {\comnpatname variable inductor = #1}}
\compattikzset{V/.style = {\comnpatname voltage source = #1}}
\compattikzset{cV/.style = {\comnpatname controlled voltage source = #1}}
\compattikzset{sV/.style = {\comnpatname sinusoidal voltage source = #1}}
\compattikzset{sqV/.style = {\comnpatname square voltage source = #1}}
\compattikzset{tV/.style = {\comnpatname triangle voltage source = #1}}
\compattikzset{csV/.style = {\comnpatname controlled sinusoidal voltage source = #1}}
\def\pgf@temp#1{ 
	\compattikzset{V#1/.style = {\comnpatname voltage source, v#1=##1} } 
	\compattikzset{cV#1/.style = {\comnpatname controlled  voltage source, v#1=##1} } 
	\compattikzset{sV#1/.style = {\comnpatname sinusoidal  voltage source, v#1=##1} } 
	\compattikzset{csV#1/.style = {\comnpatname controlled sinusoidal voltage source, v#1=##1} } 
}
\pgf@temp{_>} \pgf@temp{_<} \pgf@temp{^>} \pgf@temp{^<} 
\pgf@temp{>} \pgf@temp{<} \pgf@temp{^} \pgf@temp{_}

%current sources
\compattikzset{I/.style = {\comnpatname current source = #1}}
\compattikzset{cI/.style = {\comnpatname controlled current source = #1}}
\compattikzset{sI/.style = {\comnpatname sinusoidal current source = #1}}
\compattikzset{csI/.style = {\comnpatname controlled sinusoidal current source = #1}}
\def\pgf@temp#1{ 
	\compattikzset{I#1/.style = {\comnpatname current source, i#1=##1} } 
	\compattikzset{cI#1/.style = {\comnpatname controlled current source, i#1=##1} } 
	\compattikzset{sI#1/.style = {\comnpatname sinusoidal current source, i#1=##1} } 
	\compattikzset{csI#1/.style = {\comnpatname controlled sinusoidal current source, i#1=##1} } 
}
\pgf@temp{_>} \pgf@temp{_<} \pgf@temp{^>} \pgf@temp{^<}
\pgf@temp{>_} \pgf@temp{<_} \pgf@temp{>^} \pgf@temp{<^}
\pgf@temp{>} \pgf@temp{<} \pgf@temp{^} \pgf@temp{_}



\compattikzset{Mr/.style = {\comnpatname memristor}}

\compattikzset{cspst/.style = {\comnpatname closing switch = #1}}
\compattikzset{ospst/.style = {\comnpatname opening switch = #1}}
\compattikzset{spst/.style = {\comnpatname switch = #1}}

\compattikzset{afuse/.style = {\comnpatname asymmetric fuse=#1}}

\compattikzset{vdd/.style = {\comnpatname vcc = #1}}
\compattikzset{vss/.style = {\comnpatname vee = #1}}

\def\inheritlogicport#1#2{
	\pgfdeclareshape{#2 port}{
		\inheritsavedanchors[from=#1 #2 port]
		\inheritbackgroundpath[from=#1 #2 port]
		\inheritanchor[from=#1 #2 port]{in}
		\inheritanchor[from=#1 #2 port]{in 1}
		\inheritanchor[from=#1 #2 port]{in 2}
		\inheritanchor[from=#1 #2 port]{out}
		\inheritanchor[from=#1 #2 port]{center}
		\inheritanchor[from=#1 #2 port]{left}
	}
}

\ifpgf@circuit@europeanlogicport
	\inheritlogicport{european}{and}
	\inheritlogicport{european}{or}
	\inheritlogicport{european}{xor}
	\inheritlogicport{european}{not}
	\inheritlogicport{european}{nand}
	\inheritlogicport{european}{nor}
	\inheritlogicport{european}{xnor}
\else
	\inheritlogicport{american}{and}
	\inheritlogicport{american}{or}
	\inheritlogicport{american}{xor}
	\inheritlogicport{american}{not}
	\inheritlogicport{american}{nand}
	\inheritlogicport{american}{nor}
	\inheritlogicport{american}{xnor}
\fi

% Transistor like bipoles

\def\pgf@circ@trans@path#1#2{
	\pgfextra{
		\edef\pgf@temp{\pgfkeysvalueof{/tikz/circuitikz/bipole/name}}
		\def\pgf@circ@temp{#2}
		\ifx\pgf@temp\pgf@circ@temp % if it has not a name
			\pgfmathrandominteger{\pgf@circ@rand}{1000}{9999}
			\ctikzset{bipole/name = trans\pgf@circ@rand} % create it
		\fi
	}
	\ifpgf@circuit@bipole@inverted
		(\tikztostart) node[coordinate] (\ctikzvalof{bipole/name}end) {}
		(\tikztotarget) node[coordinate] (\ctikzvalof{bipole/name}start) {} 	
	\else
		(\tikztostart) node[coordinate] (\ctikzvalof{bipole/name}start) {}
		(\tikztotarget) node[coordinate] (\ctikzvalof{bipole/name}end) {} 
	\fi
	\pgfextra{
		\pgfmathanglebetweenpoints{\pgfpointanchor{\ctikzvalof{bipole/name}start}{center}}
					   {\pgfpointanchor{\ctikzvalof{bipole/name}end}{center}}
		\pgfmathadd{\pgfmathresult}{-90}
		\edef\pgf@circ@direction{\pgfmathresult}
	}
	($(\tikztostart) ! .5 ! (\tikztotarget)$) 
		node[#1, /tikz/rotate=\pgf@circ@direction, xscale=\ctikzvalof{mirror value}]
			(\ctikzvalof{bipole/name}) {} node {\ctikzvalof{bipole/label/name}}
		\ifcsname pgf@anchor@#1@pathstart\endcsname%if special path-anchors are defined, use them!
			(\ctikzvalof{bipole/name}start.center) --(\ctikzvalof{bipole/name}.pathstart)
			(\ctikzvalof{bipole/name}.pathend)  -- (\ctikzvalof{bipole/name}end.center)
		\else
			(\ctikzvalof{bipole/name}start.center) --(\ctikzvalof{bipole/name}.left)
			(\ctikzvalof{bipole/name}.right)  -- (\ctikzvalof{bipole/name}end.center)
		\fi
	\pgfextra{
		\pgfcircresetpath
	}  
	(\tikztotarget) 	\tikztonodes  % e si continua
}


\def\pgf@circ@definetranspath#1{
	\compattikzset{T#1/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@trans@path{#1}{}, l=##1}}
}

\pgf@circ@definetranspath{elmech}
\pgf@circ@definetranspath{nmos}
\pgf@circ@definetranspath{pmos}
\pgf@circ@definetranspath{npn}
\pgf@circ@definetranspath{pnp}
\pgf@circ@definetranspath{nfet}
\pgf@circ@definetranspath{nigfete}
\pgf@circ@definetranspath{nigfetd}
\pgf@circ@definetranspath{nigfetebulk}
\pgf@circ@definetranspath{pfet}
\pgf@circ@definetranspath{pigfete}
\pgf@circ@definetranspath{pigfetd}
\pgf@circ@definetranspath{pigfetebulk}
\pgf@circ@definetranspath{njfet}
\pgf@circ@definetranspath{pjfet}
\pgf@circ@definetranspath{pigbt}
\pgf@circ@definetranspath{nigbt}
\pgf@circ@definetranspath{Lpigbt}
\pgf@circ@definetranspath{Lnigbt}
%%%---------- close: tex/pgfcircpath

\catcode`\@=\tikzatcode
\catcode`\|=\tikzbarcode
\catcode`\!=\tikzexclaimcode

% define the environment
\long\def\startcircuitikz#1\stopcircuitikz{\starttikzpicture#1\stoptikzpicture}

\protect

\stopmodule

\endinput
